;SIMES_Product Code##OTHER##;SIMES_Beam Angle##ANGLE##DEGREES;SIMES_Color Temperature##COLOR_TEMPERATURE##KELVIN;SIMES_Rated Wattage##ELECTRICAL_POWER##WATTS;SIMES_Rated Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;SIMES_Finishes##OTHER##;SIMES_Weigth##MASS##KILOGRAMS;SIMES_Warranty Period##OTHER##;SIMES_Supply Voltage Min##ELECTRICAL_POTENTIAL##VOLTS;SIMES_Supply Voltage Max##ELECTRICAL_POTENTIAL##VOLTS;SIMES_Supply Voltage##ELECTRICAL_POTENTIAL##VOLTS;SIMES_Source Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;SIMES_Remote Power Supply##OTHER##;SIMES_Protection Class##OTHER##;SIMES_Product Page URL##OTHER##;SIMES_Product Description##OTHER##;SIMES_Product Data Sheet URL##OTHER##;SIMES_Number of Poles##OTHER##;SIMES_Nominal Width##LENGTH##MILLIMETERS;SIMES_Nominal Length##LENGTH##MILLIMETERS;SIMES_Nominal Height##LENGTH##MILLIMETERS;SIMES_Mounting Type##OTHER##;SIMES_Model##OTHER##;SIMES_Material Description##OTHER##;SIMES_Manufacturer Comment##OTHER##;SIMES_Luminous Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;SIMES_Light Source Type##OTHER##;SIMES_Lamp Count##OTHER##;SIMES_Installation Note URL##OTHER##;SIMES_IP Rating##OTHER##;SIMES_IK Rating##OTHER##;SIMES_Frequency##OTHER##;SIMES_Energy Efficiency Class##OTHER##;SIMES_Dimmable##OTHER##;SIMES_Current##ELECTRICAL_CURRENT##AMPERES;SIMES_Control Gear##OTHER##;SIMES_Cable Length##OTHER##;SIMES_CRI##OTHER##;SIMES_Approval Mark##OTHER##;LightFixturePlacingType##OTHER##;LightFixtureMountingType##OTHER##;Light Source##OTHER##;HasProtectiveEarth##OTHER##;Ground Stake##OTHER##;Body##OTHER##;Photometric_Type##OTHER##
S.1900H.14_MINI OVER-ALL_12°_2700K_723lm_8.2W_Aluminium grey;S.1900H.14;12;2700;8.2;723;14 Aluminium Grey;1.2;3 years;0;0;0;741;need remote power supply type S.3423 230V/700mA 39W;III;https://www.simes.it/en/overview/153/over-all;Over-all is an up-light of easy and immediate application: a special nylon fixing plate isolating it from the ground, is directly fixed to the surface without any recessed in-ground device.;https://www.simes.it/en/search/?q=1900;1;200;200;29;Surface Up-light;Mini Over-all 12°;Aluminium body;n/a;76,11111111;LED;1;https://www.simes.it/download/montaggio/ISTROVERALL.pdf;IP65/IP67;IK 09;DC 0Hz;A+;yes;0.7;n/a;5.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Mini Over-all_Photometrics : S.1900H
S.1900H.24_MINI OVER-ALL_12°_2700K_723lm_8.2W_Anthracite grey;S.1900H.24;12;2700;8.2;723;24 Anthracite Grey;1.2;3 years;0;0;0;741;need remote power supply type S.3423 230V/700mA 39W;III;https://www.simes.it/en/overview/153/over-all;Over-all is an up-light of easy and immediate application: a special nylon fixing plate isolating it from the ground, is directly fixed to the surface without any recessed in-ground device.;https://www.simes.it/en/search/?q=1900;1;200;200;29;Surface Up-light;Mini Over-all 12°;Aluminium body;n/a;76,11111111;LED;1;https://www.simes.it/download/montaggio/ISTROVERALL.pdf;IP65/IP67;IK 09;DC 0Hz;A+;yes;0.7;n/a;5.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_24_Anthracyte grey;Simes_Mini Over-all_Photometrics : S.1900H
S.1900N.14_MINI OVER-ALL_12°_4000K_855lm_8.2W_Aluminium grey;S.1900N.14;12;4000;8.2;855;14 Aluminium Grey;1.2;3 years;0;0;0;842;need remote power supply type S.3423 230V/700mA 39W;III;https://www.simes.it/en/overview/153/over-all;Over-all is an up-light of easy and immediate application: a special nylon fixing plate isolating it from the ground, is directly fixed to the surface without any recessed in-ground device.;https://www.simes.it/en/search/?q=1900;1;200;200;29;Surface Up-light;Mini Over-all 12°;Aluminium body;n/a;90,11111111;LED;1;https://www.simes.it/download/montaggio/ISTROVERALL.pdf;IP65/IP67;IK 08;DC 0Hz;A+;yes;0.7;n/a;5.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Mini Over-all_Photometrics : S.1900N
S.1900N.24_MINI OVER-ALL_12°_4000K_855lm_8.2W_Anthracite grey;S.1900N.24;12;4000;8.2;855;24 Anthracite Grey;1.2;3 years;0;0;0;842;need remote power supply type S.3423 230V/700mA 39W;III;https://www.simes.it/en/overview/153/over-all;Over-all is an up-light of easy and immediate application: a special nylon fixing plate isolating it from the ground, is directly fixed to the surface without any recessed in-ground device.;https://www.simes.it/en/search/?q=1900;1;200;200;29;Surface Up-light;Mini Over-all 12°;Aluminium body;n/a;90,11111111;LED;1;https://www.simes.it/download/montaggio/ISTROVERALL.pdf;IP65/IP67;IK 08;DC 0Hz;A+;yes;0.7;n/a;5.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_24_Anthracyte grey;Simes_Mini Over-all_Photometrics : S.1900N
S.1900W.14_MINI OVER-ALL_12°_3000K_789lm_8.2W_Aluminium grey;S.1900W.14;12;3000;8.2;789;14 Aluminium Grey;1.2;3 years;0;0;0;780;need remote power supply type S.3423 230V/700mA 39W;III;https://www.simes.it/en/overview/153/over-all;Over-all is an up-light of easy and immediate application: a special nylon fixing plate isolating it from the ground, is directly fixed to the surface without any recessed in-ground device.;https://www.simes.it/en/search/?q=1900;1;200;200;29;Surface Up-light;Mini Over-all 12°;Aluminium body;n/a;76,11111111;LED;1;https://www.simes.it/download/montaggio/ISTROVERALL.pdf;IP65/IP67;IK 09;DC 0Hz;A+;yes;0.7;n/a;5.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Mini Over-all_Photometrics : S.1900W
S.1900W.24_MINI OVER-ALL_12°_3000K_789lm_8.2W_Anthracite grey;S.1900W.24;12;3000;8.2;789;24 Anthracite Grey;1.2;3 years;0;0;0;780;need remote power supply type S.3423 230V/700mA 39W;III;https://www.simes.it/en/overview/153/over-all;Over-all is an up-light of easy and immediate application: a special nylon fixing plate isolating it from the ground, is directly fixed to the surface without any recessed in-ground device.;https://www.simes.it/en/search/?q=1900;1;200;200;29;Surface Up-light;Mini Over-all 12°;Aluminium body;n/a;76,11111111;LED;1;https://www.simes.it/download/montaggio/ISTROVERALL.pdf;IP65/IP67;IK 09;DC 0Hz;A+;yes;0.7;n/a;5.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_24_Anthracyte grey;Simes_Mini Over-all_Photometrics : S.1900W
S.1901H.14_MINI OVER-ALL_33°_2700K_694lm_8.2W_Aluminium grey;S.1901H.14;33;2700;8.2;694;14 Aluminium Grey;1.2;3 years;0;0;0;741;need remote power supply type S.3423 230V/700mA 39W;III;https://www.simes.it/en/overview/153/over-all;Over-all is an up-light of easy and immediate application: a special nylon fixing plate isolating it from the ground, is directly fixed to the surface without any recessed in-ground device.;https://www.simes.it/en/search/?q=1901;1;200;200;29;Surface Up-light;Mini Over-all 33°;Aluminium body;n/a;75,11111111;LED;1;https://www.simes.it/download/montaggio/ISTROVERALL.pdf;IP65/IP67;IK 09;DC 0Hz;A+;yes;0.7;n/a;5.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Mini Over-all_Photometrics : S.1901H
S.1901H.24_MINI OVER-ALL_33°_2700K_694lm_8.2W_Anthracite grey;S.1901H.24;33;2700;8.2;694;24 Anthracite Grey;1.2;3 years;0;0;0;741;need remote power supply type S.3423 230V/700mA 39W;III;https://www.simes.it/en/overview/153/over-all;Over-all is an up-light of easy and immediate application: a special nylon fixing plate isolating it from the ground, is directly fixed to the surface without any recessed in-ground device.;https://www.simes.it/en/search/?q=1901;1;200;200;29;Surface Up-light;Mini Over-all 33°;Aluminium body;n/a;75,11111111;LED;1;https://www.simes.it/download/montaggio/ISTROVERALL.pdf;IP65/IP67;IK 09;DC 0Hz;A+;yes;0.7;n/a;5.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_24_Anthracyte grey;Simes_Mini Over-all_Photometrics : S.1901H
S.1901N.14_MINI OVER-ALL_33°_4000K_820lm_8.2W_Aluminium grey;S.1901N.14;33;4000;8.2;820;14 Aluminium Grey;1.2;3 years;0;0;0;842;need remote power supply type S.3423 230V/700mA 39W;III;https://www.simes.it/en/overview/153/over-all;Over-all is an up-light of easy and immediate application: a special nylon fixing plate isolating it from the ground, is directly fixed to the surface without any recessed in-ground device.;https://www.simes.it/en/search/?q=1901;1;200;200;29;Surface Up-light;Mini Over-all 33°;Aluminium body;n/a;85,66666667;LED;1;https://www.simes.it/download/montaggio/ISTROVERALL.pdf;IP65/IP67;IK 08;DC 0Hz;A+;yes;0.7;n/a;5.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Mini Over-all_Photometrics : S.1901N
S.1901N.24_MINI OVER-ALL_33°_4000K_820lm_8.2W_Anthracite grey;S.1901N.24;33;4000;8.2;820;24 Anthracite Grey;1.2;3 years;0;0;0;842;need remote power supply type S.3423 230V/700mA 39W;III;https://www.simes.it/en/overview/153/over-all;Over-all is an up-light of easy and immediate application: a special nylon fixing plate isolating it from the ground, is directly fixed to the surface without any recessed in-ground device.;https://www.simes.it/en/search/?q=1901;1;200;200;29;Surface Up-light;Mini Over-all 33°;Aluminium body;n/a;85,66666667;LED;1;https://www.simes.it/download/montaggio/ISTROVERALL.pdf;IP65/IP67;IK 08;DC 0Hz;A+;yes;0.7;n/a;5.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_24_Anthracyte grey;Simes_Mini Over-all_Photometrics : S.1901N
S.1901W.14_MINI OVER-ALL_33°_3000K_757lm_8.2W_Aluminium grey;S.1901W.14;33;3000;8.2;757;14 Aluminium Grey;1.2;3 years;0;0;0;780;need remote power supply type S.3423 230V/700mA 39W;III;https://www.simes.it/en/overview/153/over-all;Over-all is an up-light of easy and immediate application: a special nylon fixing plate isolating it from the ground, is directly fixed to the surface without any recessed in-ground device.;https://www.simes.it/en/search/?q=1901;1;200;200;29;Surface Up-light;Mini Over-all 33°;Aluminium body;n/a;75,11111111;LED;1;https://www.simes.it/download/montaggio/ISTROVERALL.pdf;IP65/IP67;IK 09;DC 0Hz;A+;yes;0.7;n/a;5.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Mini Over-all_Photometrics : S.1901W
S.1901W.24_MINI OVER-ALL_33°_3000K_757lm_8.2W_Anthracite grey;S.1901W.24;33;3000;8.2;757;24 Anthracite Grey;1.2;3 years;0;0;0;780;need remote power supply type S.3423 230V/700mA 39W;III;https://www.simes.it/en/overview/153/over-all;Over-all is an up-light of easy and immediate application: a special nylon fixing plate isolating it from the ground, is directly fixed to the surface without any recessed in-ground device.;https://www.simes.it/en/search/?q=1901;1;200;200;29;Surface Up-light;Mini Over-all 33°;Aluminium body;n/a;75,11111111;LED;1;https://www.simes.it/download/montaggio/ISTROVERALL.pdf;IP65/IP67;IK 09;DC 0Hz;A+;yes;0.7;n/a;5.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_24_Anthracyte grey;Simes_Mini Over-all_Photometrics : S.1901W
S.1905H.14_MINI OVER-ALL_ASY_2700K_658lm_8.2W_Aluminium grey;S.1905H.14;0;2700;8.2;658;14 Aluminium Grey;1.2;3 years;0;0;0;741;need remote power supply type S.3423 230V/700mA 39W;III;https://www.simes.it/en/overview/153/over-all;Over-all is an up-light of easy and immediate application: a special nylon fixing plate isolating it from the ground, is directly fixed to the surface without any recessed in-ground device.;https://www.simes.it/en/search/?q=1905;1;200;200;29;Surface Up-light;Mini Over-all ASY;Aluminium body;n/a;72,55555556;LED;1;https://www.simes.it/download/montaggio/ISTROVERALL.pdf;IP65/IP67;IK 09;DC 0Hz;A+;yes;0.7;n/a;5.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Mini Over-all_Photometrics : S.1905H
S.1905H.24_MINI OVER-ALL_ASY_2700K_658lm_8.2W_Anthracite grey;S.1905H.24;0;2700;8.2;658;24 Anthracite Grey;1.2;3 years;0;0;0;741;need remote power supply type S.3423 230V/700mA 39W;III;https://www.simes.it/en/overview/153/over-all;Over-all is an up-light of easy and immediate application: a special nylon fixing plate isolating it from the ground, is directly fixed to the surface without any recessed in-ground device.;https://www.simes.it/en/search/?q=1905;1;200;200;29;Surface Up-light;Mini Over-all ASY;Aluminium body;n/a;72,55555556;LED;1;https://www.simes.it/download/montaggio/ISTROVERALL.pdf;IP65/IP67;IK 09;DC 0Hz;A+;yes;0.7;n/a;5.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_24_Anthracyte grey;Simes_Mini Over-all_Photometrics : S.1905H
S.1905N.14_MINI OVER-ALL_ASY_4000K_778lm_8.2W_Aluminium grey;S.1905N.14;0;4000;8.2;778;14 Aluminium Grey;1.2;3 years;0;0;0;842;need remote power supply type S.3423 230V/700mA 39W;III;https://www.simes.it/en/overview/153/over-all;Over-all is an up-light of easy and immediate application: a special nylon fixing plate isolating it from the ground, is directly fixed to the surface without any recessed in-ground device.;https://www.simes.it/en/search/?q=1905;1;200;200;29;Surface Up-light;Mini Over-all ASY;Aluminium body;n/a;82,66666667;LED;1;https://www.simes.it/download/montaggio/ISTROVERALL.pdf;IP65/IP67;IK 08;DC 0Hz;A+;yes;0.7;n/a;5.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Mini Over-all_Photometrics : S.1905N
S.1905N.24_MINI OVER-ALL_ASY_4000K_778lm_8.2W_Anthracite grey;S.1905N.24;0;4000;8.2;778;24 Anthracite Grey;1.2;3 years;0;0;0;842;need remote power supply type S.3423 230V/700mA 39W;III;https://www.simes.it/en/overview/153/over-all;Over-all is an up-light of easy and immediate application: a special nylon fixing plate isolating it from the ground, is directly fixed to the surface without any recessed in-ground device.;https://www.simes.it/en/search/?q=1905;1;200;200;29;Surface Up-light;Mini Over-all ASY;Aluminium body;n/a;82,66666667;LED;1;https://www.simes.it/download/montaggio/ISTROVERALL.pdf;IP65/IP67;IK 08;DC 0Hz;A+;yes;0.7;n/a;5.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_24_Anthracyte grey;Simes_Mini Over-all_Photometrics : S.1905N
S.1905W.14_MINI OVER-ALL_ASY_3000K_718lm_8.2W_Aluminium grey;S.1905W.14;0;3000;8.2;718;14 Aluminium Grey;1.2;3 years;0;0;0;780;need remote power supply type S.3423 230V/700mA 39W;III;https://www.simes.it/en/overview/153/over-all;Over-all is an up-light of easy and immediate application: a special nylon fixing plate isolating it from the ground, is directly fixed to the surface without any recessed in-ground device.;https://www.simes.it/en/search/?q=1905;1;200;200;29;Surface Up-light;Mini Over-all ASY;Aluminium body;n/a;72,55555556;LED;1;https://www.simes.it/download/montaggio/ISTROVERALL.pdf;IP65/IP67;IK 09;DC 0Hz;A+;yes;0.7;n/a;5.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Mini Over-all_Photometrics : S.1905W
S.1905W.24_MINI OVER-ALL_ASY_3000K_718lm_8.2W_Anthracite grey;S.1905W.24;0;3000;8.2;718;24 Anthracite Grey;1.2;3 years;0;0;0;780;need remote power supply type S.3423 230V/700mA 39W;III;https://www.simes.it/en/overview/153/over-all;Over-all is an up-light of easy and immediate application: a special nylon fixing plate isolating it from the ground, is directly fixed to the surface without any recessed in-ground device.;https://www.simes.it/en/search/?q=1905;1;200;200;29;Surface Up-light;Mini Over-all ASY;Aluminium body;n/a;72,55555556;LED;1;https://www.simes.it/download/montaggio/ISTROVERALL.pdf;IP65/IP67;IK 09;DC 0Hz;A+;yes;0.7;n/a;5.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_24_Anthracyte grey;Simes_Mini Over-all_Photometrics : S.1905W
