;SIMES_Product Code##OTHER##;SIMES_Beam Angle##ANGLE##DEGREES;SIMES_Color Temperature##COLOR_TEMPERATURE##KELVIN;SIMES_Rated Wattage##ELECTRICAL_POWER##WATTS;SIMES_Rated Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;SIMES_Finishes##OTHER##;SIMES_Weigth##MASS##KILOGRAMS;SIMES_Warranty Period##OTHER##;SIMES_Supply Voltage Min##ELECTRICAL_POTENTIAL##VOLTS;SIMES_Supply Voltage Max##ELECTRICAL_POTENTIAL##VOLTS;SIMES_Supply Voltage##ELECTRICAL_POTENTIAL##VOLTS;SIMES_Source Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;SIMES_Remote Power Supply##OTHER##;SIMES_Protection Class##OTHER##;SIMES_Product Page URL##OTHER##;SIMES_Product Description##OTHER##;SIMES_Product Data Sheet URL##OTHER##;SIMES_Number of Poles##OTHER##;SIMES_Nominal Width##LENGTH##MILLIMETERS;SIMES_Nominal Length##LENGTH##MILLIMETERS;SIMES_Nominal Height##LENGTH##MILLIMETERS;SIMES_Mounting Type##OTHER##;SIMES_Model##OTHER##;SIMES_Material Description##OTHER##;SIMES_Manufacturer Comment##OTHER##;SIMES_Luminous Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;SIMES_Light Source Type##OTHER##;SIMES_Lamp Count##OTHER##;SIMES_Installation Note URL##OTHER##;SIMES_IP Rating##OTHER##;SIMES_IK Rating##OTHER##;SIMES_Frequency##OTHER##;SIMES_Energy Efficiency Class##OTHER##;SIMES_Dimmable##OTHER##;SIMES_Current##ELECTRICAL_CURRENT##AMPERES;SIMES_Control Gear##OTHER##;SIMES_Cable Length##OTHER##;SIMES_CRI##OTHER##;SIMES_Approval Mark##OTHER##;LightFixturePlacingType##OTHER##;LightFixtureMountingType##OTHER##;Light Source##OTHER##;HasProtectiveEarth##OTHER##;Ground Stake##OTHER##;Body##OTHER##;Photometric_Type##OTHER##
S.7245H.01_COOL BOLLARD_H290_2700K_1237lm_12.1W_White;S.7245H.01;0;2700;12.1;1237;01 White;3.73;3 years;220;240;230;1831;n/a;I;https://www.simes.it/en/overview/95/cool-bollard;COOL is a simple void volume diffusing light in two directions from a very thin LED circuit right below its protective glass.;https://www.simes.it/en/search/?q=7245;1;43;290;290;Ground mounted;COOL H290 GROUND MOUNTED;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRCOOLPAL.pdf;IP54;IK 06;AC 50-60Hz / DC;A+;PHASE-CUT DIM;0;Electronic ballast;0.4m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_01_White;Simes_Cool_Photometrics : S.7270H
S.7245H.09_COOL BOLLARD_H290_2700K_1237lm_12.1W_Black;S.7245H.09;0;2700;12.1;1237;09 Black;3.73;3 years;220;240;230;1831;n/a;I;https://www.simes.it/en/overview/95/cool-bollard;COOL is a simple void volume diffusing light in two directions from a very thin LED circuit right below its protective glass.;https://www.simes.it/en/search/?q=7245;1;43;290;290;Ground mounted;COOL H290 GROUND MOUNTED;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRCOOLPAL.pdf;IP54;IK 06;AC 50-60Hz / DC;A+;PHASE-CUT DIM;0;Electronic ballast;0.4m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_09_Black;Simes_Cool_Photometrics : S.7270H
S.7245H.14_COOL BOLLARD_H290_2700K_1237lm_12.1W_Aluminium grey;S.7245H.14;0;2700;12.1;1237;14 Aluminium Grey;3.73;3 years;220;240;230;1831;n/a;I;https://www.simes.it/en/overview/95/cool-bollard;COOL is a simple void volume diffusing light in two directions from a very thin LED circuit right below its protective glass.;https://www.simes.it/en/search/?q=7245;1;43;290;290;Ground mounted;COOL H290 GROUND MOUNTED;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRCOOLPAL.pdf;IP54;IK 06;AC 50-60Hz / DC;A+;PHASE-CUT DIM;0;Electronic ballast;0.4m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Cool_Photometrics : S.7270H
S.7245N.01_COOL BOLLARD_H290_4000K_1454lm_12.1W_White;S.7245N.01;0;4000;12.1;1454;01 White;3.73;3 years;220;240;230;1928;n/a;I;https://www.simes.it/en/overview/95/cool-bollard;COOL is a simple void volume diffusing light in two directions from a very thin LED circuit right below its protective glass.;https://www.simes.it/en/search/?q=7245;1;43;290;290;Ground mounted;COOL H290 GROUND MOUNTED;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRCOOLPAL.pdf;IP54;IK 06;AC 50-60Hz / DC;A+;PHASE-CUT DIM;0;Electronic ballast;0.4m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_01_White;Simes_Cool_Photometrics : S.7270N
S.7245N.09_COOL BOLLARD_H290_4000K_1454lm_12.1W_Black;S.7245N.09;0;4000;12.1;1454;09 Black;3.73;3 years;220;240;230;1928;n/a;I;https://www.simes.it/en/overview/95/cool-bollard;COOL is a simple void volume diffusing light in two directions from a very thin LED circuit right below its protective glass.;https://www.simes.it/en/search/?q=7245;1;43;290;290;Ground mounted;COOL H290 GROUND MOUNTED;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRCOOLPAL.pdf;IP54;IK 06;AC 50-60Hz / DC;A+;PHASE-CUT DIM;0;Electronic ballast;0.4m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_09_Black;Simes_Cool_Photometrics : S.7270N
S.7245N.14_COOL BOLLARD_H290_4000K_1454lm_12.1W_Aluminium grey;S.7245N.14;0;4000;12.1;1454;14 Aluminium Grey;3.73;3 years;220;240;230;1928;n/a;I;https://www.simes.it/en/overview/95/cool-bollard;COOL is a simple void volume diffusing light in two directions from a very thin LED circuit right below its protective glass.;https://www.simes.it/en/search/?q=7245;1;43;290;290;Ground mounted;COOL H290 GROUND MOUNTED;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRCOOLPAL.pdf;IP54;IK 06;AC 50-60Hz / DC;A+;PHASE-CUT DIM;0;Electronic ballast;0.4m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Cool_Photometrics : S.7270N
S.7245W.01_COOL BOLLARD_H290_3000K_1273lm_12.1W_White;S.7245W.01;0;3000;12.1;1273;01 White;3.73;3 years;220;240;230;1885;n/a;I;https://www.simes.it/en/overview/95/cool-bollard;COOL is a simple void volume diffusing light in two directions from a very thin LED circuit right below its protective glass.;https://www.simes.it/en/search/?q=7245;1;43;290;290;Ground mounted;COOL H290 GROUND MOUNTED;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRCOOLPAL.pdf;IP54;IK 06;AC 50-60Hz / DC;A+;PHASE-CUT DIM;0;Electronic ballast;0.4m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_01_White;Simes_Cool_Photometrics : S.7270W
S.7245W.09_COOL BOLLARD_H290_3000K_1273lm_12.1W_Black;S.7245W.09;0;3000;12.1;1273;09 Black;3.73;3 years;220;240;230;1885;n/a;I;https://www.simes.it/en/overview/95/cool-bollard;COOL is a simple void volume diffusing light in two directions from a very thin LED circuit right below its protective glass.;https://www.simes.it/en/search/?q=7245;1;43;290;290;Ground mounted;COOL H290 GROUND MOUNTED;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRCOOLPAL.pdf;IP54;IK 06;AC 50-60Hz / DC;A+;PHASE-CUT DIM;0;Electronic ballast;0.4m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_09_Black;Simes_Cool_Photometrics : S.7270W
S.7245W.14_COOL BOLLARD_H290_3000K_1273lm_12.1W_Aluminium grey;S.7245W.14;0;3000;12.1;1273;14 Aluminium Grey;3.73;3 years;220;240;230;1885;n/a;I;https://www.simes.it/en/overview/95/cool-bollard;COOL is a simple void volume diffusing light in two directions from a very thin LED circuit right below its protective glass.;https://www.simes.it/en/search/?q=7245;1;43;290;290;Ground mounted;COOL H290 GROUND MOUNTED;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRCOOLPAL.pdf;IP54;IK 06;AC 50-60Hz / DC;A+;PHASE-CUT DIM;0;Electronic ballast;0.4m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Cool_Photometrics : S.7270W
S.7246H.01_COOL BOLLARD_H580_2700K_1237lm_12.1W_White;S.7246H.01;0;2700;12.1;1237;01 White;6.02;3 years;220;240;230;1831;n/a;I;https://www.simes.it/en/overview/95/cool-bollard;COOL is a simple void volume diffusing light in two directions from a very thin LED circuit right below its protective glass.;https://www.simes.it/en/search/?q=7246;1;43;290;580;Ground mounted;COOL H580 GROUND MOUNTED;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRCOOLPAL.pdf;IP54;IK 06;AC 50-60Hz / DC;A+;PHASE-CUT DIM;0;Electronic ballast;0.4m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_01_White;Simes_Cool_Photometrics : S.7270H
S.7246H.09_COOL BOLLARD_H580_2700K_1237lm_12.1W_Black;S.7246H.09;0;2700;12.1;1237;09 Black;6.02;3 years;220;240;230;1831;n/a;I;https://www.simes.it/en/overview/95/cool-bollard;COOL is a simple void volume diffusing light in two directions from a very thin LED circuit right below its protective glass.;https://www.simes.it/en/search/?q=7246;1;43;290;580;Ground mounted;COOL H580 GROUND MOUNTED;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRCOOLPAL.pdf;IP54;IK 06;AC 50-60Hz / DC;A+;PHASE-CUT DIM;0;Electronic ballast;0.4m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_09_Black;Simes_Cool_Photometrics : S.7270H
S.7246H.14_COOL BOLLARD_H580_2700K_1237lm_12.1W_Aluminium grey;S.7246H.14;0;2700;12.1;1237;14 Aluminium Grey;6.02;3 years;220;240;230;1831;n/a;I;https://www.simes.it/en/overview/95/cool-bollard;COOL is a simple void volume diffusing light in two directions from a very thin LED circuit right below its protective glass.;https://www.simes.it/en/search/?q=7246;1;43;290;580;Ground mounted;COOL H580 GROUND MOUNTED;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRCOOLPAL.pdf;IP54;IK 06;AC 50-60Hz / DC;A+;PHASE-CUT DIM;0;Electronic ballast;0.4m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Cool_Photometrics : S.7270H
S.7246N.01_COOL BOLLARD_H580_4000K_1454lm_12.1W_White;S.7246N.01;0;4000;12.1;1454;01 White;6.02;3 years;220;240;230;1928;n/a;I;https://www.simes.it/en/overview/95/cool-bollard;COOL is a simple void volume diffusing light in two directions from a very thin LED circuit right below its protective glass.;https://www.simes.it/en/search/?q=7246;1;43;290;580;Ground mounted;COOL H580 GROUND MOUNTED;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRCOOLPAL.pdf;IP54;IK 06;AC 50-60Hz / DC;A+;PHASE-CUT DIM;0;Electronic ballast;0.4m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_01_White;Simes_Cool_Photometrics : S.7270N
S.7246N.09_COOL BOLLARD_H580_4000K_1454lm_12.1W_Black;S.7246N.09;0;4000;12.1;1454;09 Black;6.02;3 years;220;240;230;1928;n/a;I;https://www.simes.it/en/overview/95/cool-bollard;COOL is a simple void volume diffusing light in two directions from a very thin LED circuit right below its protective glass.;https://www.simes.it/en/search/?q=7246;1;43;290;580;Ground mounted;COOL H580 GROUND MOUNTED;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRCOOLPAL.pdf;IP54;IK 06;AC 50-60Hz / DC;A+;PHASE-CUT DIM;0;Electronic ballast;0.4m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_09_Black;Simes_Cool_Photometrics : S.7270N
S.7246N.14_COOL BOLLARD_H580_4000K_1454lm_12.1W_Aluminium grey;S.7246N.14;0;4000;12.1;1454;14 Aluminium Grey;6.02;3 years;220;240;230;1928;n/a;I;https://www.simes.it/en/overview/95/cool-bollard;COOL is a simple void volume diffusing light in two directions from a very thin LED circuit right below its protective glass.;https://www.simes.it/en/search/?q=7246;1;43;290;580;Ground mounted;COOL H580 GROUND MOUNTED;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRCOOLPAL.pdf;IP54;IK 06;AC 50-60Hz / DC;A+;PHASE-CUT DIM;0;Electronic ballast;0.4m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Cool_Photometrics : S.7270N
S.7246W.01_COOL BOLLARD_H580_3000K_1273lm_12.1W_White;S.7246W.01;0;3000;12.1;1273;01 White;6.02;3 years;220;240;230;1885;n/a;I;https://www.simes.it/en/overview/95/cool-bollard;COOL is a simple void volume diffusing light in two directions from a very thin LED circuit right below its protective glass.;https://www.simes.it/en/search/?q=7246;1;43;290;580;Ground mounted;COOL H580 GROUND MOUNTED;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRCOOLPAL.pdf;IP54;IK 06;AC 50-60Hz / DC;A+;PHASE-CUT DIM;0;Electronic ballast;0.4m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_01_White;Simes_Cool_Photometrics : S.7270W
S.7246W.09_COOL BOLLARD_H580_3000K_1273lm_12.1W_Black;S.7246W.09;0;3000;12.1;1273;09 Black;6.02;3 years;220;240;230;1885;n/a;I;https://www.simes.it/en/overview/95/cool-bollard;COOL is a simple void volume diffusing light in two directions from a very thin LED circuit right below its protective glass.;https://www.simes.it/en/search/?q=7246;1;43;290;580;Ground mounted;COOL H580 GROUND MOUNTED;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRCOOLPAL.pdf;IP54;IK 06;AC 50-60Hz / DC;A+;PHASE-CUT DIM;0;Electronic ballast;0.4m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_09_Black;Simes_Cool_Photometrics : S.7270W
S.7246W.14_COOL BOLLARD_H580_3000K_1273lm_12.1W_Aluminium grey;S.7246W.14;0;3000;12.1;1273;14 Aluminium Grey;6.02;3 years;220;240;230;1885;n/a;I;https://www.simes.it/en/overview/95/cool-bollard;COOL is a simple void volume diffusing light in two directions from a very thin LED circuit right below its protective glass.;https://www.simes.it/en/search/?q=7246;1;43;290;580;Ground mounted;COOL H580 GROUND MOUNTED;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRCOOLPAL.pdf;IP54;IK 06;AC 50-60Hz / DC;A+;PHASE-CUT DIM;0;Electronic ballast;0.4m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Cool_Photometrics : S.7270W
