;SIMES_Product Code##OTHER##;SIMES_Beam Angle##ANGLE##DEGREES;SIMES_Color Temperature##COLOR_TEMPERATURE##KELVIN;SIMES_Rated Wattage##ELECTRICAL_POWER##WATTS;SIMES_Rated Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;SIMES_Finishes##OTHER##;SIMES_Weigth##MASS##KILOGRAMS;SIMES_Warranty Period##OTHER##;SIMES_Supply Voltage Min##ELECTRICAL_POTENTIAL##VOLTS;SIMES_Supply Voltage Max##ELECTRICAL_POTENTIAL##VOLTS;SIMES_Supply Voltage##ELECTRICAL_POTENTIAL##VOLTS;SIMES_Source Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;SIMES_Remote Power Supply##OTHER##;SIMES_Protection Class##OTHER##;SIMES_Product Page URL##OTHER##;SIMES_Product Description##OTHER##;SIMES_Product Data Sheet URL##OTHER##;SIMES_Number of Poles##OTHER##;SIMES_Nominal Width##LENGTH##MILLIMETERS;SIMES_Nominal Length##LENGTH##MILLIMETERS;SIMES_Nominal Height##LENGTH##MILLIMETERS;SIMES_Mounting Type##OTHER##;SIMES_Model##OTHER##;SIMES_Material Description##OTHER##;SIMES_Manufacturer Comment##OTHER##;SIMES_Luminous Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;SIMES_Light Source Type##OTHER##;SIMES_Lamp Count##OTHER##;SIMES_Installation Note URL##OTHER##;SIMES_IP Rating##OTHER##;SIMES_IK Rating##OTHER##;SIMES_Frequency##OTHER##;SIMES_Energy Efficiency Class##OTHER##;SIMES_Dimmable##OTHER##;SIMES_Current##ELECTRICAL_CURRENT##AMPERES;SIMES_Control Gear##OTHER##;SIMES_Cable Length##OTHER##;SIMES_CRI##OTHER##;SIMES_Approval Mark##OTHER##;LightFixturePlacingType##OTHER##;LightFixtureMountingType##OTHER##;Light Source##OTHER##;HasProtectiveEarth##OTHER##;Ground Stake##OTHER##;Body##OTHER##;Photometric_Type##OTHER##
S.4655H.01_STEP_2700K_15lm_2.9W_White;S.4655H.01;0;2700;2.9;15;01 White;0.5;3 years;220;240;230;163;n/a;I;https://www.simes.it/en/overview/58/step-bollard;Sharp and minimal design combined with a perfect light beam. STEP, equipped with LED source, creates a marked blade of light on the wall.;https://www.simes.it/en/search/?q=4655;1;85;54;208;Wall recessed;STEP WALL RECESSED;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRSTEP2.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;0.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_01_White;Simes_Step_Photometrics : S.4655H
S.4655H.14_STEP_2700K_15lm_2.9W_Aluminium grey;S.4655H.14;0;2700;2.9;15;14 Aluminium Grey;0.5;3 years;220;240;230;163;n/a;I;https://www.simes.it/en/overview/58/step-bollard;Sharp and minimal design combined with a perfect light beam. STEP, equipped with LED source, creates a marked blade of light on the wall.;https://www.simes.it/en/search/?q=4655;1;85;54;208;Wall recessed;STEP WALL RECESSED;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRSTEP2.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;0.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Step_Photometrics : S.4655H
S.4655N.01_STEP_4000K_17lm_2.9W_White;S.4655N.01;0;4000;2.9;17;01 White;0.5;3 years;220;240;230;186;n/a;I;https://www.simes.it/en/overview/58/step-bollard;Sharp and minimal design combined with a perfect light beam. STEP, equipped with LED source, creates a marked blade of light on the wall.;https://www.simes.it/en/search/?q=4655;1;85;54;208;Wall recessed;STEP WALL RECESSED;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRSTEP2.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;0.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_01_White;Simes_Step_Photometrics : S.4655N
S.4655N.14_STEP_4000K_17lm_2.9W_Aluminium grey;S.4655N.14;0;4000;2.9;17;14 Aluminium Grey;0.5;3 years;220;240;230;186;n/a;I;https://www.simes.it/en/overview/58/step-bollard;Sharp and minimal design combined with a perfect light beam. STEP, equipped with LED source, creates a marked blade of light on the wall.;https://www.simes.it/en/search/?q=4655;1;85;54;208;Wall recessed;STEP WALL RECESSED;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRSTEP2.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;0.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Step_Photometrics : S.4655N
S.4655W.01_STEP_3000K_16lm_2.9W_White;S.4655W.01;0;3000;2.9;16;01 White;0.5;3 years;220;240;230;172;n/a;I;https://www.simes.it/en/overview/58/step-bollard;Sharp and minimal design combined with a perfect light beam. STEP, equipped with LED source, creates a marked blade of light on the wall.;https://www.simes.it/en/search/?q=4655;1;85;54;208;Wall recessed;STEP WALL RECESSED;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRSTEP2.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;0.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_01_White;Simes_Step_Photometrics : S.4655W
S.4655W.14_STEP_3000K_16lm_2.9W_Aluminium grey;S.4655W.14;0;3000;2.9;16;14 Aluminium Grey;0.5;3 years;220;240;230;172;n/a;I;https://www.simes.it/en/overview/58/step-bollard;Sharp and minimal design combined with a perfect light beam. STEP, equipped with LED source, creates a marked blade of light on the wall.;https://www.simes.it/en/search/?q=4655;1;85;54;208;Wall recessed;STEP WALL RECESSED;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRSTEP2.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;0.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Step_Photometrics : S.4655W
