;SIMES_Product Code##OTHER##;SIMES_Beam Angle##ANGLE##DEGREES;SIMES_Color Temperature##COLOR_TEMPERATURE##KELVIN;SIMES_Rated Wattage##ELECTRICAL_POWER##WATTS;SIMES_Rated Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;SIMES_Finishes##OTHER##;SIMES_Weigth##MASS##KILOGRAMS;SIMES_Warranty Period##OTHER##;SIMES_Supply Voltage Min##ELECTRICAL_POTENTIAL##VOLTS;SIMES_Supply Voltage Max##ELECTRICAL_POTENTIAL##VOLTS;SIMES_Supply Voltage##ELECTRICAL_POTENTIAL##VOLTS;SIMES_Source Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;SIMES_Remote Power Supply##OTHER##;SIMES_Protection Class##OTHER##;SIMES_Product Page URL##OTHER##;SIMES_Product Description##OTHER##;SIMES_Product Data Sheet URL##OTHER##;SIMES_Number of Poles##OTHER##;SIMES_Nominal Width##LENGTH##MILLIMETERS;SIMES_Nominal Length##LENGTH##MILLIMETERS;SIMES_Nominal Height##LENGTH##MILLIMETERS;SIMES_Mounting Type##OTHER##;SIMES_Model##OTHER##;SIMES_Material Description##OTHER##;SIMES_Manufacturer Comment##OTHER##;SIMES_Luminous Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;SIMES_Light Source Type##OTHER##;SIMES_Lamp Count##OTHER##;SIMES_Installation Note URL##OTHER##;SIMES_IP Rating##OTHER##;SIMES_IK Rating##OTHER##;SIMES_Frequency##OTHER##;SIMES_Energy Efficiency Class##OTHER##;SIMES_Dimmable##OTHER##;SIMES_Current##ELECTRICAL_CURRENT##AMPERES;SIMES_Control Gear##OTHER##;SIMES_Cable Length##OTHER##;SIMES_CRI##OTHER##;SIMES_Approval Mark##OTHER##;LightFixturePlacingType##OTHER##;LightFixtureMountingType##OTHER##;Light Source##OTHER##;HasProtectiveEarth##OTHER##;Ground Stake##OTHER##;Body##OTHER##;Photometric_Type##OTHER##
S.6400H.01_APPEAL_2700K_455lm_15W_White;S.6400H.01;0;2700;15;455;01 White;1;3 years;220;240;230;997;n/a;II;https://www.simes.it/en/overview/101/appeal;This is APPEAL, a bi-emission luminaire for external uses which creates indirect light all-around or an asymmetrical distribution.;https://www.simes.it/en/search/?q=6400;1;30;310;65;Wall mounted;APPEAL;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRAPPEAL2.pdf;IP54;IK 08;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;2.0m;CRI80;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_01_White;Simes_Appeal_Photometrics : S.6400H
S.6400H.14_APPEAL_2700K_455lm_15W_Aluminium grey;S.6400H.14;0;2700;15;455;14 Aluminium Grey;1;3 years;220;240;230;997;n/a;II;https://www.simes.it/en/overview/101/appeal;This is APPEAL, a bi-emission luminaire for external uses which creates indirect light all-around or an asymmetrical distribution.;https://www.simes.it/en/search/?q=6400;1;30;310;65;Wall mounted;APPEAL;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRAPPEAL2.pdf;IP54;IK 08;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;2.0m;CRI80;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Appeal_Photometrics : S.6400H
S.6400N.01_APPEAL_4000K_515lm_15W_White;S.6400N.01;0;4000;15;515;01 White;1;3 years;220;240;230;1130;n/a;II;https://www.simes.it/en/overview/101/appeal;This is APPEAL, a bi-emission luminaire for external uses which creates indirect light all-around or an asymmetrical distribution.;https://www.simes.it/en/search/?q=6400;1;30;310;65;Wall mounted;APPEAL;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRAPPEAL2.pdf;IP54;IK 08;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;2.0m;CRI80;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_01_White;Simes_Appeal_Photometrics : S.6400N
S.6400N.14_APPEAL_4000K_515lm_15W_Aluminium grey;S.6400N.14;0;4000;15;515;14 Aluminium Grey;1;3 years;220;240;230;1130;n/a;II;https://www.simes.it/en/overview/101/appeal;This is APPEAL, a bi-emission luminaire for external uses which creates indirect light all-around or an asymmetrical distribution.;https://www.simes.it/en/search/?q=6400;1;30;310;65;Wall mounted;APPEAL;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRAPPEAL2.pdf;IP54;IK 08;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;2.0m;CRI80;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Appeal_Photometrics : S.6400N
S.6400W.01_APPEAL_3000K_479lm_15W_White;S.6400W.01;0;3000;15;479;01 White;1;3 years;220;240;230;1050;n/a;II;https://www.simes.it/en/overview/101/appeal;This is APPEAL, a bi-emission luminaire for external uses which creates indirect light all-around or an asymmetrical distribution.;https://www.simes.it/en/search/?q=6400;1;30;310;65;Wall mounted;APPEAL;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRAPPEAL2.pdf;IP54;IK 08;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;2.0m;CRI80;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_01_White;Simes_Appeal_Photometrics : S.6400W
S.6400W.14_APPEAL_3000K_479lm_15W_Aluminium grey;S.6400W.14;0;3000;15;479;14 Aluminium Grey;1;3 years;220;240;230;1050;n/a;II;https://www.simes.it/en/overview/101/appeal;This is APPEAL, a bi-emission luminaire for external uses which creates indirect light all-around or an asymmetrical distribution.;https://www.simes.it/en/search/?q=6400;1;30;310;65;Wall mounted;APPEAL;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRAPPEAL2.pdf;IP54;IK 08;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;2.0m;CRI80;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Appeal_Photometrics : S.6400W
