;SIMES_Product Code##OTHER##;SIMES_Beam Angle##ANGLE##DEGREES;SIMES_Color Temperature##COLOR_TEMPERATURE##KELVIN;SIMES_Rated Wattage##ELECTRICAL_POWER##WATTS;SIMES_Rated Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;SIMES_Finishes##OTHER##;SIMES_Weigth##MASS##KILOGRAMS;SIMES_Warranty Period##OTHER##;SIMES_Supply Voltage Min##ELECTRICAL_POTENTIAL##VOLTS;SIMES_Supply Voltage Max##ELECTRICAL_POTENTIAL##VOLTS;SIMES_Supply Voltage##ELECTRICAL_POTENTIAL##VOLTS;SIMES_Source Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;SIMES_Remote Power Supply##OTHER##;SIMES_Protection Class##OTHER##;SIMES_Product Page URL##OTHER##;SIMES_Product Description##OTHER##;SIMES_Product Data Sheet URL##OTHER##;SIMES_Number of Poles##OTHER##;SIMES_Nominal Width##LENGTH##MILLIMETERS;SIMES_Nominal Length##LENGTH##MILLIMETERS;SIMES_Nominal Height##LENGTH##MILLIMETERS;SIMES_Mounting Type##OTHER##;SIMES_Model##OTHER##;SIMES_Material Description##OTHER##;SIMES_Manufacturer Comment##OTHER##;SIMES_Luminous Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;SIMES_Light Source Type##OTHER##;SIMES_Lamp Count##OTHER##;SIMES_Installation Note URL##OTHER##;SIMES_IP Rating##OTHER##;SIMES_IK Rating##OTHER##;SIMES_Frequency##OTHER##;SIMES_Energy Efficiency Class##OTHER##;SIMES_Dimmable##OTHER##;SIMES_Current##ELECTRICAL_CURRENT##AMPERES;SIMES_Control Gear##OTHER##;SIMES_Cable Length##OTHER##;SIMES_CRI##OTHER##;SIMES_Approval Mark##OTHER##;LightFixturePlacingType##OTHER##;LightFixtureMountingType##OTHER##;Light Source##OTHER##;HasProtectiveEarth##OTHER##;Ground Stake##OTHER##;Body##OTHER##;Photometric_Type##OTHER##
S.6080H.09_BLINKER_2700K_538lm_23W_Black;S.6080H.09;0;2700;23;538;09 Black;2.4;3 years;220;240;230;2298;n/a;I;https://www.simes.it/en/overview/18/blinker;With a clear personality, BLINKER is an elegant wall recess fitting, ideal for discrete illumination of walkways, passages and stairs.;https://www.simes.it/en/search/?q=6080;1;120;180;287;Wall recessed;BLINKER WALL RECESSED;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRBLINKER2.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;DALI 2 / PUSH;0;Electronic ballast;0.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_09_Black;Simes_Blinker_Photometrics : S.6080H
S.6080H.14_BLINKER_2700K_538lm_23W_Aluminium grey;S.6080H.14;0;2700;23;538;14 Aluminium Grey;2.4;3 years;220;240;230;2298;n/a;I;https://www.simes.it/en/overview/18/blinker;With a clear personality, BLINKER is an elegant wall recess fitting, ideal for discrete illumination of walkways, passages and stairs.;https://www.simes.it/en/search/?q=6080;1;120;180;287;Wall recessed;BLINKER WALL RECESSED;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRBLINKER2.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;DALI 2 / PUSH;0;Electronic ballast;0.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Blinker_Photometrics : S.6080H
S.6080N.09_BLINKER_4000K_597lm_23W_Black;S.6080N.09;0;4000;23;597;09 Black;2.4;3 years;220;240;230;2490;n/a;I;https://www.simes.it/en/overview/18/blinker;With a clear personality, BLINKER is an elegant wall recess fitting, ideal for discrete illumination of walkways, passages and stairs.;https://www.simes.it/en/search/?q=6080;1;120;180;287;Wall recessed;BLINKER WALL RECESSED;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRBLINKER2.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;DALI 2 / PUSH;0;Electronic ballast;0.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_09_Black;Simes_Blinker_Photometrics : S.6080N
S.6080N.14_BLINKER_4000K_597lm_23W_Aluminium grey;S.6080N.14;0;4000;23;597;14 Aluminium Grey;2.4;3 years;220;240;230;2490;n/a;I;https://www.simes.it/en/overview/18/blinker;With a clear personality, BLINKER is an elegant wall recess fitting, ideal for discrete illumination of walkways, passages and stairs.;https://www.simes.it/en/search/?q=6080;1;120;180;287;Wall recessed;BLINKER WALL RECESSED;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRBLINKER2.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;DALI 2 / PUSH;0;Electronic ballast;0.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Blinker_Photometrics : S.6080N
S.6080W.09_BLINKER_3000K_567lm_23W_Black;S.6080W.09;0;3000;23;567;09 Black;2.4;3 years;220;240;230;2419;n/a;I;https://www.simes.it/en/overview/18/blinker;With a clear personality, BLINKER is an elegant wall recess fitting, ideal for discrete illumination of walkways, passages and stairs.;https://www.simes.it/en/search/?q=6080;1;120;180;287;Wall recessed;BLINKER WALL RECESSED;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRBLINKER2.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;DALI 2 / PUSH;0;Electronic ballast;0.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_09_Black;Simes_Blinker_Photometrics : S.6080W
S.6080W.14_BLINKER_3000K_567lm_23W_Aluminium grey;S.6080W.14;0;3000;23;567;14 Aluminium Grey;2.4;3 years;220;240;230;2419;n/a;I;https://www.simes.it/en/overview/18/blinker;With a clear personality, BLINKER is an elegant wall recess fitting, ideal for discrete illumination of walkways, passages and stairs.;https://www.simes.it/en/search/?q=6080;1;120;180;287;Wall recessed;BLINKER WALL RECESSED;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRBLINKER2.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;DALI 2 / PUSH;0;Electronic ballast;0.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Blinker_Photometrics : S.6080W
