;SIMES_Product Code##OTHER##;SIMES_Beam Angle##ANGLE##DEGREES;SIMES_Color Temperature##COLOR_TEMPERATURE##KELVIN;SIMES_Rated Wattage##ELECTRICAL_POWER##WATTS;SIMES_Rated Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;SIMES_Finishes##OTHER##;SIMES_Weigth##MASS##KILOGRAMS;SIMES_Warranty Period##OTHER##;SIMES_Supply Voltage Min##ELECTRICAL_POTENTIAL##VOLTS;SIMES_Supply Voltage Max##ELECTRICAL_POTENTIAL##VOLTS;SIMES_Supply Voltage##ELECTRICAL_POTENTIAL##VOLTS;SIMES_Source Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;SIMES_Remote Power Supply##OTHER##;SIMES_Protection Class##OTHER##;SIMES_Product Page URL##OTHER##;SIMES_Product Description##OTHER##;SIMES_Product Data Sheet URL##OTHER##;SIMES_Number of Poles##OTHER##;SIMES_Nominal Width##LENGTH##MILLIMETERS;SIMES_Nominal Length##LENGTH##MILLIMETERS;SIMES_Nominal Height##LENGTH##MILLIMETERS;SIMES_Mounting Type##OTHER##;SIMES_Model##OTHER##;SIMES_Material Description##OTHER##;SIMES_Manufacturer Comment##OTHER##;SIMES_Luminous Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;SIMES_Light Source Type##OTHER##;SIMES_Lamp Count##OTHER##;SIMES_Installation Note URL##OTHER##;SIMES_IP Rating##OTHER##;SIMES_IK Rating##OTHER##;SIMES_Frequency##OTHER##;SIMES_Energy Efficiency Class##OTHER##;SIMES_Dimmable##OTHER##;SIMES_Current##ELECTRICAL_CURRENT##AMPERES;SIMES_Control Gear##OTHER##;SIMES_Cable Length##OTHER##;SIMES_CRI##OTHER##;SIMES_Approval Mark##OTHER##;LightFixturePlacingType##OTHER##;LightFixtureMountingType##OTHER##;Light Source##OTHER##;HasProtectiveEarth##OTHER##;Ground Stake##OTHER##;Body##OTHER##;Photometric_Type##OTHER##;SIMES_AltezzaTraf##LENGTH##MILLIMETERS
S.7206H.01_MINILOOK_2700K_584lm_8.7W_H220_White;S.7206H.01;0;2700;8.7;584;01 White;1.5;3 years;220;240;230;1282;n/a;II;https://www.simes.it/en/overview/93/look-bollard;LOOK has an elegant rectangular body, minimal and compact, mounted on wall or on its bollard. The light is directed on one side through a glass window.;https://www.simes.it/en/search/?q=7206;1;66;220;220;Ground;MINILOOK BOLLARD H220;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRLOOKPAL2.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;0.4m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_01_White;Simes_Minilook_Bollard_Photometrics : S.7206H;187
S.7206H.14_MINILOOK_2700K_584lm_8.7W_H220_Aluminium grey;S.7206H.14;0;2700;8.7;584;14 Aluminium Grey;1.5;3 years;220;240;230;1282;n/a;II;https://www.simes.it/en/overview/93/look-bollard;LOOK has an elegant rectangular body, minimal and compact, mounted on wall or on its bollard. The light is directed on one side through a glass window.;https://www.simes.it/en/search/?q=7206;1;66;220;220;Ground;MINILOOK BOLLARD H220;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRLOOKPAL2.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;0.4m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Minilook_Bollard_Photometrics : S.7206H;187
S.7206H.20_MINILOOK_2700K_584lm_8.7W_H220_Burnished bronze;S.7206H.20;0;2700;8.7;584;20 Burnished bronze;1.5;3 years;220;240;230;1282;n/a;II;https://www.simes.it/en/overview/93/look-bollard;LOOK has an elegant rectangular body, minimal and compact, mounted on wall or on its bollard. The light is directed on one side through a glass window.;https://www.simes.it/en/search/?q=7206;1;66;220;220;Ground;MINILOOK BOLLARD H220;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRLOOKPAL2.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;0.4m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_20_Burnished bronze;Simes_Minilook_Bollard_Photometrics : S.7206H;187
S.7206H.24_MINILOOK_2700K_584lm_8.7W_H220_Anthracite grey;S.7206H.24;0;2700;8.7;584;24 Anthracite Grey;1.5;3 years;220;240;230;1282;n/a;II;https://www.simes.it/en/overview/93/look-bollard;LOOK has an elegant rectangular body, minimal and compact, mounted on wall or on its bollard. The light is directed on one side through a glass window.;https://www.simes.it/en/search/?q=7206;1;66;220;220;Ground;MINILOOK BOLLARD H220;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRLOOKPAL2.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;0.4m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_24_Anthracyte grey;Simes_Minilook_Bollard_Photometrics : S.7206H;187
S.7206W.01_MINILOOK_3000K_601lm_8.7W_H220_White;S.7206W.01;0;3000;8.7;601;01 White;1.5;3 years;220;240;230;1319;n/a;II;https://www.simes.it/en/overview/93/look-bollard;LOOK has an elegant rectangular body, minimal and compact, mounted on wall or on its bollard. The light is directed on one side through a glass window.;https://www.simes.it/en/search/?q=7206;1;66;220;220;Ground;MINILOOK BOLLARD H220;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRLOOKPAL2.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;0.4m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_01_White;Simes_Minilook_Bollard_Photometrics : S.7206W;187
S.7206W.14_MINILOOK_3000K_601lm_8.7W_H220_Aluminium grey;S.7206W.14;0;3000;8.7;601;14 Aluminium Grey;1.5;3 years;220;240;230;1319;n/a;II;https://www.simes.it/en/overview/93/look-bollard;LOOK has an elegant rectangular body, minimal and compact, mounted on wall or on its bollard. The light is directed on one side through a glass window.;https://www.simes.it/en/search/?q=7206;1;66;220;220;Ground;MINILOOK BOLLARD H220;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRLOOKPAL2.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;0.4m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Minilook_Bollard_Photometrics : S.7206W;187
S.7206W.20_MINILOOK_3000K_601lm_8.7W_H220_Burnished bronze;S.7206W.20;0;3000;8.7;601;20 Burnished bronze;1.5;3 years;220;240;230;1319;n/a;II;https://www.simes.it/en/overview/93/look-bollard;LOOK has an elegant rectangular body, minimal and compact, mounted on wall or on its bollard. The light is directed on one side through a glass window.;https://www.simes.it/en/search/?q=7206;1;66;220;220;Ground;MINILOOK BOLLARD H220;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRLOOKPAL2.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;0.4m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_20_Burnished bronze;Simes_Minilook_Bollard_Photometrics : S.7206W;187
S.7206W.24_MINILOOK_3000K_601lm_8.7W_H220_Anthracite grey;S.7206W.24;0;3000;8.7;601;24 Anthracite Grey;1.5;3 years;220;240;230;1319;n/a;II;https://www.simes.it/en/overview/93/look-bollard;LOOK has an elegant rectangular body, minimal and compact, mounted on wall or on its bollard. The light is directed on one side through a glass window.;https://www.simes.it/en/search/?q=7206;1;66;220;220;Ground;MINILOOK BOLLARD H220;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRLOOKPAL2.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;0.4m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_24_Anthracyte grey;Simes_Minilook_Bollard_Photometrics : S.7206W;187
S.7206N.01_MINILOOK_4000K_614lm_8.7W_H220_White;S.7206N.01;0;4000;8.7;614;01 White;1.5;3 years;220;240;230;1349;n/a;II;https://www.simes.it/en/overview/93/look-bollard;LOOK has an elegant rectangular body, minimal and compact, mounted on wall or on its bollard. The light is directed on one side through a glass window.;https://www.simes.it/en/search/?q=7206;1;66;220;220;Ground;MINILOOK BOLLARD H220;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRLOOKPAL2.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;0.4m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_01_White;Simes_Minilook_Bollard_Photometrics : S.7206N;187
S.7206N.14_MINILOOK_4000K_614lm_8.7W_H220_Aluminium grey;S.7206N.14;0;4000;8.7;614;14 Aluminium Grey;1.5;3 years;220;240;230;1349;n/a;II;https://www.simes.it/en/overview/93/look-bollard;LOOK has an elegant rectangular body, minimal and compact, mounted on wall or on its bollard. The light is directed on one side through a glass window.;https://www.simes.it/en/search/?q=7206;1;66;220;220;Ground;MINILOOK BOLLARD H220;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRLOOKPAL2.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;0.4m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Minilook_Bollard_Photometrics : S.7206N;187
S.7206N.20_MINILOOK_4000K_614lm_8.7W_H220_Burnished bronze;S.7206N.20;0;4000;8.7;614;20 Burnished bronze;1.5;3 years;220;240;230;1349;n/a;II;https://www.simes.it/en/overview/93/look-bollard;LOOK has an elegant rectangular body, minimal and compact, mounted on wall or on its bollard. The light is directed on one side through a glass window.;https://www.simes.it/en/search/?q=7206;1;66;220;220;Ground;MINILOOK BOLLARD H220;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRLOOKPAL2.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;0.4m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_20_Burnished bronze;Simes_Minilook_Bollard_Photometrics : S.7206N;187
S.7206N.24_MINILOOK_4000K_614lm_8.7W_H220_Anthracite grey;S.7206N.24;0;4000;8.7;614;24 Anthracite Grey;1.5;3 years;220;240;230;1349;n/a;II;https://www.simes.it/en/overview/93/look-bollard;LOOK has an elegant rectangular body, minimal and compact, mounted on wall or on its bollard. The light is directed on one side through a glass window.;https://www.simes.it/en/search/?q=7206;1;66;220;220;Ground;MINILOOK BOLLARD H220;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRLOOKPAL2.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;0.4m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_24_Anthracyte grey;Simes_Minilook_Bollard_Photometrics : S.7206N;187
S.7211H.01_MINILOOK_2700K_584lm_8.7W_H580_White;S.7211H.01;0;2700;8.7;584;01 White;3.6;3 years;220;240;230;1282;n/a;II;https://www.simes.it/en/overview/93/look-bollard;LOOK has an elegant rectangular body, minimal and compact, mounted on wall or on its bollard. The light is directed on one side through a glass window.;https://www.simes.it/en/search/?q=7211;1;66;220;580;Ground;MINILOOK BOLLARD H580;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRLOOKPAL2.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;0.4m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_01_White;Simes_Minilook_Bollard_Photometrics : S.7206H;547
S.7211H.14_MINILOOK_2700K_584lm_8.7W_H580_Aluminium grey;S.7211H.14;0;2700;8.7;584;14 Aluminium Grey;3.6;3 years;220;240;230;1282;n/a;II;https://www.simes.it/en/overview/93/look-bollard;LOOK has an elegant rectangular body, minimal and compact, mounted on wall or on its bollard. The light is directed on one side through a glass window.;https://www.simes.it/en/search/?q=7211;1;66;220;580;Ground;MINILOOK BOLLARD H580;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRLOOKPAL2.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;0.4m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Minilook_Bollard_Photometrics : S.7206H;547
S.7211H.20_MINILOOK_2700K_584lm_8.7W_H580_Burnished bronze;S.7211H.20;0;2700;8.7;584;20 Burnished bronze;3.6;3 years;220;240;230;1282;n/a;II;https://www.simes.it/en/overview/93/look-bollard;LOOK has an elegant rectangular body, minimal and compact, mounted on wall or on its bollard. The light is directed on one side through a glass window.;https://www.simes.it/en/search/?q=7211;1;66;220;580;Ground;MINILOOK BOLLARD H580;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRLOOKPAL2.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;0.4m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_20_Burnished bronze;Simes_Minilook_Bollard_Photometrics : S.7206H;547
S.7211H.24_MINILOOK_2700K_584lm_8.7W_H580_Anthracite grey;S.7211H.24;0;2700;8.7;584;24 Anthracite Grey;3.6;3 years;220;240;230;1282;n/a;II;https://www.simes.it/en/overview/93/look-bollard;LOOK has an elegant rectangular body, minimal and compact, mounted on wall or on its bollard. The light is directed on one side through a glass window.;https://www.simes.it/en/search/?q=7211;1;66;220;580;Ground;MINILOOK BOLLARD H580;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRLOOKPAL2.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;0.4m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_24_Anthracyte grey;Simes_Minilook_Bollard_Photometrics : S.7206H;547
S.7211W.01_MINILOOK_3000K_601lm_8.7W_H580_White;S.7211W.01;0;3000;8.7;601;01 White;3.6;3 years;220;240;230;1319;n/a;II;https://www.simes.it/en/overview/93/look-bollard;LOOK has an elegant rectangular body, minimal and compact, mounted on wall or on its bollard. The light is directed on one side through a glass window.;https://www.simes.it/en/search/?q=7211;1;66;220;580;Ground;MINILOOK BOLLARD H580;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRLOOKPAL2.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;0.4m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_01_White;Simes_Minilook_Bollard_Photometrics : S.7206W;547
S.7211W.14_MINILOOK_3000K_601lm_8.7W_H580_Aluminium grey;S.7211W.14;0;3000;8.7;601;14 Aluminium Grey;3.6;3 years;220;240;230;1319;n/a;II;https://www.simes.it/en/overview/93/look-bollard;LOOK has an elegant rectangular body, minimal and compact, mounted on wall or on its bollard. The light is directed on one side through a glass window.;https://www.simes.it/en/search/?q=7211;1;66;220;580;Ground;MINILOOK BOLLARD H580;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRLOOKPAL2.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;0.4m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Minilook_Bollard_Photometrics : S.7206W;547
S.7211W.20_MINILOOK_3000K_601lm_8.7W_H580_Burnished bronze;S.7211W.20;0;3000;8.7;601;20 Burnished bronze;3.6;3 years;220;240;230;1319;n/a;II;https://www.simes.it/en/overview/93/look-bollard;LOOK has an elegant rectangular body, minimal and compact, mounted on wall or on its bollard. The light is directed on one side through a glass window.;https://www.simes.it/en/search/?q=7211;1;66;220;580;Ground;MINILOOK BOLLARD H580;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRLOOKPAL2.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;0.4m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_20_Burnished bronze;Simes_Minilook_Bollard_Photometrics : S.7206W;547
S.7211W.24_MINILOOK_3000K_601lm_8.7W_H580_Anthracite grey;S.7211W.24;0;3000;8.7;601;24 Anthracite Grey;3.6;3 years;220;240;230;1319;n/a;II;https://www.simes.it/en/overview/93/look-bollard;LOOK has an elegant rectangular body, minimal and compact, mounted on wall or on its bollard. The light is directed on one side through a glass window.;https://www.simes.it/en/search/?q=7211;1;66;220;580;Ground;MINILOOK BOLLARD H580;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRLOOKPAL2.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;0.4m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_24_Anthracyte grey;Simes_Minilook_Bollard_Photometrics : S.7206W;547
S.7211N.01_MINILOOK_4000K_614lm_8.7W_H580_White;S.7211N.01;0;4000;8.7;614;01 White;3.6;3 years;220;240;230;1349;n/a;II;https://www.simes.it/en/overview/93/look-bollard;LOOK has an elegant rectangular body, minimal and compact, mounted on wall or on its bollard. The light is directed on one side through a glass window.;https://www.simes.it/en/search/?q=7211;1;66;220;580;Ground;MINILOOK BOLLARD H580;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRLOOKPAL2.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;0.4m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_01_White;Simes_Minilook_Bollard_Photometrics : S.7206N;547
S.7211N.14_MINILOOK_4000K_614lm_8.7W_H580_Aluminium grey;S.7211N.14;0;4000;8.7;614;14 Aluminium Grey;3.6;3 years;220;240;230;1349;n/a;II;https://www.simes.it/en/overview/93/look-bollard;LOOK has an elegant rectangular body, minimal and compact, mounted on wall or on its bollard. The light is directed on one side through a glass window.;https://www.simes.it/en/search/?q=7211;1;66;220;580;Ground;MINILOOK BOLLARD H580;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRLOOKPAL2.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;0.4m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Minilook_Bollard_Photometrics : S.7206N;547
S.7211N.20_MINILOOK_4000K_614lm_8.7W_H580_Burnished bronze;S.7211N.20;0;4000;8.7;614;20 Burnished bronze;3.6;3 years;220;240;230;1349;n/a;II;https://www.simes.it/en/overview/93/look-bollard;LOOK has an elegant rectangular body, minimal and compact, mounted on wall or on its bollard. The light is directed on one side through a glass window.;https://www.simes.it/en/search/?q=7211;1;66;220;580;Ground;MINILOOK BOLLARD H580;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRLOOKPAL2.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;0.4m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_20_Burnished bronze;Simes_Minilook_Bollard_Photometrics : S.7206N;547
S.7211N.24_MINILOOK_4000K_614lm_8.7W_H580_Anthracite grey;S.7211N.24;0;4000;8.7;614;24 Anthracite Grey;3.6;3 years;220;240;230;1349;n/a;II;https://www.simes.it/en/overview/93/look-bollard;LOOK has an elegant rectangular body, minimal and compact, mounted on wall or on its bollard. The light is directed on one side through a glass window.;https://www.simes.it/en/search/?q=7211;1;66;220;580;Ground;MINILOOK BOLLARD H580;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRLOOKPAL2.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;0.4m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_24_Anthracyte grey;Simes_Minilook_Bollard_Photometrics : S.7206N;547
