;SIMES_Product Code##OTHER##;SIMES_Beam Angle##ANGLE##DEGREES;SIMES_Color Temperature##COLOR_TEMPERATURE##KELVIN;SIMES_Rated Wattage##ELECTRICAL_POWER##WATTS;SIMES_Rated Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;SIMES_Finishes##OTHER##;SIMES_Weigth##MASS##KILOGRAMS;SIMES_Warranty Period##OTHER##;SIMES_Supply Voltage Min##ELECTRICAL_POTENTIAL##VOLTS;SIMES_Supply Voltage Max##ELECTRICAL_POTENTIAL##VOLTS;SIMES_Supply Voltage##ELECTRICAL_POTENTIAL##VOLTS;SIMES_Source Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;SIMES_Remote Power Supply##OTHER##;SIMES_Protection Class##OTHER##;SIMES_Product Page URL##OTHER##;SIMES_Product Description##OTHER##;SIMES_Product Data Sheet URL##OTHER##;SIMES_Number of Poles##OTHER##;SIMES_Nominal Width##LENGTH##MILLIMETERS;SIMES_Nominal Length##LENGTH##MILLIMETERS;SIMES_Nominal Height##LENGTH##MILLIMETERS;SIMES_Mounting Type##OTHER##;SIMES_Model##OTHER##;SIMES_Material Description##OTHER##;SIMES_Manufacturer Comment##OTHER##;SIMES_Luminous Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;SIMES_Light Source Type##OTHER##;SIMES_Lamp Count##OTHER##;SIMES_Installation Note URL##OTHER##;SIMES_IP Rating##OTHER##;SIMES_IK Rating##OTHER##;SIMES_Frequency##OTHER##;SIMES_Energy Efficiency Class##OTHER##;SIMES_Dimmable##OTHER##;SIMES_Current##ELECTRICAL_CURRENT##AMPERES;SIMES_Control Gear##OTHER##;SIMES_Cable Length##OTHER##;SIMES_CRI##OTHER##;SIMES_Approval Mark##OTHER##;LightFixturePlacingType##OTHER##;LightFixtureMountingType##OTHER##;Light Source##OTHER##;HasProtectiveEarth##OTHER##;Ground Stake##OTHER##;Body##OTHER##;Photometric_Type##OTHER##
S.5090H.09_LIFT_4 WINDOWS_60°_2700K_767lm_18.2W_Black;S.5090H.09;60;2700;18.2;767;09 Black;4.7;3 years;220;240;230;1757;n/a;I;https://www.simes.it/en/overview/27/lift;Wall effect of a rigorous geometry design, LIFT fits perfectly in different architectural environments personalizing any context in a clear way.;https://www.simes.it/en/search/?q=5090;1;180;205;180;Wall mounted;LIFT SQUARE 4 WINDOWS 60°;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRLIFTQUAD2.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;0.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_09_Black;Simes_Lift_Photometrics : S.5070H
S.5090H.14_LIFT_4 WINDOWS_60°_2700K_767lm_18.2W_Aluminium grey;S.5090H.14;60;2700;18.2;767;14 Aluminium Grey;4.7;3 years;220;240;230;1757;n/a;I;https://www.simes.it/en/overview/27/lift;Wall effect of a rigorous geometry design, LIFT fits perfectly in different architectural environments personalizing any context in a clear way.;https://www.simes.it/en/search/?q=5090;1;180;205;180;Wall mounted;LIFT SQUARE 4 WINDOWS 60°;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRLIFTQUAD2.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;0.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Lift_Photometrics : S.5070H
S.5090N.09_LIFT_4 WINDOWS_60°_4000K_832lm_18.2W_Black;S.5090N.09;60;4000;18.2;832;09 Black;4.7;3 years;220;240;230;1906;n/a;I;https://www.simes.it/en/overview/27/lift;Wall effect of a rigorous geometry design, LIFT fits perfectly in different architectural environments personalizing any context in a clear way.;https://www.simes.it/en/search/?q=5090;1;180;205;180;Wall mounted;LIFT SQUARE 4 WINDOWS 60°;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRLIFTQUAD2.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;0.0m;CRI80;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_09_Black;Simes_Lift_Photometrics : S.5070N
S.5090N.14_LIFT_4 WINDOWS_60°_4000K_832lm_18.2W_Aluminium grey;S.5090N.14;60;4000;18.2;832;14 Aluminium Grey;4.7;3 years;220;240;230;1906;n/a;I;https://www.simes.it/en/overview/27/lift;Wall effect of a rigorous geometry design, LIFT fits perfectly in different architectural environments personalizing any context in a clear way.;https://www.simes.it/en/search/?q=5090;1;180;205;180;Wall mounted;LIFT SQUARE 4 WINDOWS 60°;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRLIFTQUAD2.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;0.0m;CRI80;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Lift_Photometrics : S.5070N
S.5090W.09_LIFT_4 WINDOWS_60°_3000K_808lm_18.2W_Black;S.5090W.09;60;3000;18.2;808;09 Black;4.7;3 years;220;240;230;1850;n/a;I;https://www.simes.it/en/overview/27/lift;Wall effect of a rigorous geometry design, LIFT fits perfectly in different architectural environments personalizing any context in a clear way.;https://www.simes.it/en/search/?q=5090;1;180;205;180;Wall mounted;LIFT SQUARE 4 WINDOWS 60°;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRLIFTQUAD2.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;0.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_09_Black;Simes_Lift_Photometrics : S.5070W
S.5090W.14_LIFT_4 WINDOWS_60°_3000K_808lm_18.2W_Aluminium grey;S.5090W.14;60;3000;18.2;808;14 Aluminium Grey;4.7;3 years;220;240;230;1850;n/a;I;https://www.simes.it/en/overview/27/lift;Wall effect of a rigorous geometry design, LIFT fits perfectly in different architectural environments personalizing any context in a clear way.;https://www.simes.it/en/search/?q=5090;1;180;205;180;Wall mounted;LIFT SQUARE 4 WINDOWS 60°;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRLIFTQUAD2.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;0.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Lift_Photometrics : S.5070W
S.5080H.09_LIFT_4 WINDOWS_2°_2700K_414lm_18.2W_Black;S.5080H.09;2;2700;18.2;414;09 Black;4.7;3 years;220;240;230;1757;n/a;I;https://www.simes.it/en/overview/27/lift;Wall effect of a rigorous geometry design, LIFT fits perfectly in different architectural environments personalizing any context in a clear way.;https://www.simes.it/en/search/?q=5080;1;180;205;180;Wall mounted;LIFT SQUARE 4 WINDOWS 2°;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRLIFTQUAD2.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;0.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_09_Black;Simes_Lift_Photometrics : S.5075H
S.5080H.14_LIFT_4 WINDOWS_2°_2700K_414lm_18.2W_Aluminium grey;S.5080H.14;2;2700;18.2;414;14 Aluminium Grey;4.7;3 years;220;240;230;1757;n/a;I;https://www.simes.it/en/overview/27/lift;Wall effect of a rigorous geometry design, LIFT fits perfectly in different architectural environments personalizing any context in a clear way.;https://www.simes.it/en/search/?q=5080;1;180;205;180;Wall mounted;LIFT SQUARE 4 WINDOWS 2°;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRLIFTQUAD2.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;0.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Lift_Photometrics : S.5075H
S.5080N.09_LIFT_4 WINDOWS_2°_4000K_449lm_18.2W_Black;S.5080N.09;2;4000;18.2;449;09 Black;4.7;3 years;220;240;230;1906;n/a;I;https://www.simes.it/en/overview/27/lift;Wall effect of a rigorous geometry design, LIFT fits perfectly in different architectural environments personalizing any context in a clear way.;https://www.simes.it/en/search/?q=5080;1;180;205;180;Wall mounted;LIFT SQUARE 4 WINDOWS 2°;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRLIFTQUAD2.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;0.0m;CRI80;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_09_Black;Simes_Lift_Photometrics : S.5075N
S.5080N.14_LIFT_4 WINDOWS_2°_4000K_449lm_18.2W_Aluminium grey;S.5080N.14;2;4000;18.2;449;14 Aluminium Grey;4.7;3 years;220;240;230;1906;n/a;I;https://www.simes.it/en/overview/27/lift;Wall effect of a rigorous geometry design, LIFT fits perfectly in different architectural environments personalizing any context in a clear way.;https://www.simes.it/en/search/?q=5080;1;180;205;180;Wall mounted;LIFT SQUARE 4 WINDOWS 2°;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRLIFTQUAD2.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;0.0m;CRI80;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Lift_Photometrics : S.5075N
S.5080W.09_LIFT_4 WINDOWS_2°_3000K_436lm_18.2W_Black;S.5080W.09;2;3000;18.2;436;09 Black;4.7;3 years;220;240;230;1850;n/a;I;https://www.simes.it/en/overview/27/lift;Wall effect of a rigorous geometry design, LIFT fits perfectly in different architectural environments personalizing any context in a clear way.;https://www.simes.it/en/search/?q=5080;1;180;205;180;Wall mounted;LIFT SQUARE 4 WINDOWS 2°;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRLIFTQUAD2.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;0.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_09_Black;Simes_Lift_Photometrics : S.5075W
S.5080W.14_LIFT_4 WINDOWS_2°_3000K_436lm_18.2W_Aluminium grey;S.5080W.14;2;3000;18.2;436;14 Aluminium Grey;4.7;3 years;220;240;230;1850;n/a;I;https://www.simes.it/en/overview/27/lift;Wall effect of a rigorous geometry design, LIFT fits perfectly in different architectural environments personalizing any context in a clear way.;https://www.simes.it/en/search/?q=5080;1;180;205;180;Wall mounted;LIFT SQUARE 4 WINDOWS 2°;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRLIFTQUAD2.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;0.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Lift_Photometrics : S.5075W
