;SIMES_Product Code##OTHER##;SIMES_Beam Angle##ANGLE##DEGREES;SIMES_Color Temperature##COLOR_TEMPERATURE##KELVIN;SIMES_Rated Wattage##ELECTRICAL_POWER##WATTS;SIMES_Rated Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;SIMES_Finishes##OTHER##;SIMES_Weigth##MASS##KILOGRAMS;SIMES_Warranty Period##OTHER##;SIMES_Supply Voltage Min##ELECTRICAL_POTENTIAL##VOLTS;SIMES_Supply Voltage Max##ELECTRICAL_POTENTIAL##VOLTS;SIMES_Supply Voltage##ELECTRICAL_POTENTIAL##VOLTS;SIMES_Source Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;SIMES_Remote Power Supply##OTHER##;SIMES_Protection Class##OTHER##;SIMES_Product Page URL##OTHER##;SIMES_Product Description##OTHER##;SIMES_Product Data Sheet URL##OTHER##;SIMES_Number of Poles##OTHER##;SIMES_Nominal Width##LENGTH##MILLIMETERS;SIMES_Nominal Length##LENGTH##MILLIMETERS;SIMES_Nominal Height##LENGTH##MILLIMETERS;SIMES_Mounting Type##OTHER##;SIMES_Model##OTHER##;SIMES_Material Description##OTHER##;SIMES_Manufacturer Comment##OTHER##;SIMES_Luminous Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;SIMES_Light Source Type##OTHER##;SIMES_Lamp Count##OTHER##;SIMES_Installation Note URL##OTHER##;SIMES_IP Rating##OTHER##;SIMES_IK Rating##OTHER##;SIMES_Frequency##OTHER##;SIMES_Energy Efficiency Class##OTHER##;SIMES_Dimmable##OTHER##;SIMES_Current##ELECTRICAL_CURRENT##AMPERES;SIMES_Control Gear##OTHER##;SIMES_Cable Length##OTHER##;SIMES_CRI##OTHER##;SIMES_Approval Mark##OTHER##;LightFixturePlacingType##OTHER##;LightFixtureMountingType##OTHER##;Light Source##OTHER##;HasProtectiveEarth##OTHER##;Ground Stake##OTHER##;Body##OTHER##;Photometric_Type##OTHER##
S.5227H.14_REEF_2X90°_2700K_1124lm_35W_Aluminium grey;S.5227H.14;0;2700;35;1124;14 Aluminium Grey;1;3 years;220;240;230;3893;n/a;II;https://www.simes.it/en/overview/62/reef-bollard;REEF is a wide range of bollards and short bollards available in more dimensions and different light configurations.;https://www.simes.it/en/search/?q=5227;1;250;250;220;Ground;REEF 2X90° BOLLARD H220;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRREEF2.pdf;IP65;IK 10;AC 50-60Hz / DC;A+;DALI2/PUSH;0;Electronic ballast;0.4m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Reef_Bollard_Photometrics : S.5227H
S.5227H.20_REEF_2X90°_2700K_1124lm_35W_Burnished bronze_###PHASE-OUT###;S.5227H.20;0;2700;35;1124;20 Burnished bronze;1;3 years;220;240;230;3893;n/a;II;https://www.simes.it/en/overview/62/reef-bollard;REEF is a wide range of bollards and short bollards available in more dimensions and different light configurations.;https://www.simes.it/en/search/?q=5227;1;250;250;220;Ground;REEF 2X90° BOLLARD H220;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRREEF2.pdf;IP65;IK 10;AC 50-60Hz / DC;A+;DALI2/PUSH;0;Electronic ballast;0.4m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_20_Burnished bronze;Simes_Reef_Bollard_Photometrics : S.5227H
S.5227H.24_REEF_2X90°_2700K_1124lm_35W_Anthracite grey;S.5227H.24;0;2700;35;1124;24 Anthracite Grey;1;3 years;220;240;230;3893;n/a;II;https://www.simes.it/en/overview/62/reef-bollard;REEF is a wide range of bollards and short bollards available in more dimensions and different light configurations.;https://www.simes.it/en/search/?q=5227;1;250;250;220;Ground;REEF 2X90° BOLLARD H220;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRREEF2.pdf;IP65;IK 10;AC 50-60Hz / DC;A+;DALI2/PUSH;0;Electronic ballast;0.4m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_24_Anthracyte grey;Simes_Reef_Bollard_Photometrics : S.5227H
S.5227W.14_REEF_2X90°_3000K_1229lm_35W_Aluminium grey;S.5227W.14;0;3000;35;1229;14 Aluminium Grey;1;3 years;220;240;230;4257;n/a;II;https://www.simes.it/en/overview/62/reef-bollard;REEF is a wide range of bollards and short bollards available in more dimensions and different light configurations.;https://www.simes.it/en/search/?q=5227;1;250;250;220;Ground;REEF 2X90° BOLLARD H220;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRREEF2.pdf;IP65;IK 10;AC 50-60Hz / DC;A+;DALI2/PUSH;0;Electronic ballast;0.4m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Reef_Bollard_Photometrics : S.5227W
S.5227W.20_REEF_2X90°_3000K_1229lm_35W_Burnished bronze_###PHASE-OUT###;S.5227W.20;0;3000;35;1229;20 Burnished bronze;1;3 years;220;240;230;4257;n/a;II;https://www.simes.it/en/overview/62/reef-bollard;REEF is a wide range of bollards and short bollards available in more dimensions and different light configurations.;https://www.simes.it/en/search/?q=5227;1;250;250;220;Ground;REEF 2X90° BOLLARD H220;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRREEF2.pdf;IP65;IK 10;AC 50-60Hz / DC;A+;DALI2/PUSH;0;Electronic ballast;0.4m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_20_Burnished bronze;Simes_Reef_Bollard_Photometrics : S.5227W
S.5227W.24_REEF_2X90°_3000K_1229lm_35W_Anthracite grey;S.5227W.24;0;3000;35;1229;24 Anthracite Grey;1;3 years;220;240;230;4257;n/a;II;https://www.simes.it/en/overview/62/reef-bollard;REEF is a wide range of bollards and short bollards available in more dimensions and different light configurations.;https://www.simes.it/en/search/?q=5227;1;250;250;220;Ground;REEF 2X90° BOLLARD H220;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRREEF2.pdf;IP65;IK 10;AC 50-60Hz / DC;A+;DALI2/PUSH;0;Electronic ballast;0.4m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_24_Anthracyte grey;Simes_Reef_Bollard_Photometrics : S.5227W
S.5227N.14_REEF_2X90°_4000K_1292lm_35W_Aluminium grey;S.5227N.14;0;4000;35;1292;14 Aluminium Grey;1;3 years;220;240;230;4473;n/a;II;https://www.simes.it/en/overview/62/reef-bollard;REEF is a wide range of bollards and short bollards available in more dimensions and different light configurations.;https://www.simes.it/en/search/?q=5227;1;250;250;220;Ground;REEF 2X90° BOLLARD H220;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRREEF2.pdf;IP65;IK 10;AC 50-60Hz / DC;A+;DALI2/PUSH;0;Electronic ballast;0.4m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Reef_Bollard_Photometrics : S.5227N
S.5227N.20_REEF_2X90°_4000K_1292lm_35W_Burnished bronze_###PHASE-OUT###;S.5227N.20;0;4000;35;1292;20 Burnished bronze;1;3 years;220;240;230;4473;n/a;II;https://www.simes.it/en/overview/62/reef-bollard;REEF is a wide range of bollards and short bollards available in more dimensions and different light configurations.;https://www.simes.it/en/search/?q=5227;1;250;250;220;Ground;REEF 2X90° BOLLARD H220;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRREEF2.pdf;IP65;IK 10;AC 50-60Hz / DC;A+;DALI2/PUSH;0;Electronic ballast;0.4m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_20_Burnished bronze;Simes_Reef_Bollard_Photometrics : S.5227N
S.5227N.24_REEF_2X90°_4000K_1292lm_35W_Anthracite grey;S.5227N.24;0;4000;35;1292;24 Anthracite Grey;1;3 years;220;240;230;4473;n/a;II;https://www.simes.it/en/overview/62/reef-bollard;REEF is a wide range of bollards and short bollards available in more dimensions and different light configurations.;https://www.simes.it/en/search/?q=5227;1;250;250;220;Ground;REEF 2X90° BOLLARD H220;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRREEF2.pdf;IP65;IK 10;AC 50-60Hz / DC;A+;DALI2/PUSH;0;Electronic ballast;0.4m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_24_Anthracyte grey;Simes_Reef_Bollard_Photometrics : S.5227N
