;SIMES_Product Code##OTHER##;SIMES_Beam Angle##ANGLE##DEGREES;SIMES_Color Temperature##COLOR_TEMPERATURE##KELVIN;SIMES_Rated Wattage##ELECTRICAL_POWER##WATTS;SIMES_Rated Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;SIMES_Finishes##OTHER##;SIMES_Weigth##MASS##KILOGRAMS;SIMES_Warranty Period##OTHER##;SIMES_Supply Voltage Min##ELECTRICAL_POTENTIAL##VOLTS;SIMES_Supply Voltage Max##ELECTRICAL_POTENTIAL##VOLTS;SIMES_Supply Voltage##ELECTRICAL_POTENTIAL##VOLTS;SIMES_Source Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;SIMES_Remote Power Supply##OTHER##;SIMES_Protection Class##OTHER##;SIMES_Product Page URL##OTHER##;SIMES_Product Description##OTHER##;SIMES_Product Data Sheet URL##OTHER##;SIMES_Number of Poles##OTHER##;SIMES_Nominal Width##LENGTH##MILLIMETERS;SIMES_Nominal Length##LENGTH##MILLIMETERS;SIMES_Nominal Height##LENGTH##MILLIMETERS;SIMES_Mounting Type##OTHER##;SIMES_Model##OTHER##;SIMES_Material Description##OTHER##;SIMES_Manufacturer Comment##OTHER##;SIMES_Luminous Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;SIMES_Light Source Type##OTHER##;SIMES_Lamp Count##OTHER##;SIMES_Installation Note URL##OTHER##;SIMES_IP Rating##OTHER##;SIMES_IK Rating##OTHER##;SIMES_Frequency##OTHER##;SIMES_Energy Efficiency Class##OTHER##;SIMES_Dimmable##OTHER##;SIMES_Current##ELECTRICAL_CURRENT##AMPERES;SIMES_Control Gear##OTHER##;SIMES_Cable Length##OTHER##;SIMES_CRI##OTHER##;SIMES_Approval Mark##OTHER##;LightFixturePlacingType##OTHER##;LightFixtureMountingType##OTHER##;Light Source##OTHER##;HasProtectiveEarth##OTHER##;Ground Stake##OTHER##;Body##OTHER##;Photometric_Type##OTHER##
S.5695H.09_MINI SUIT_1 WINDOW_2700K_36lm_2.2W_Black;S.5695H.09;0;2700;2.2;36;09 Black;2.33;3 years;220;240;230;156;n/a;I;https://www.simes.it/en/overview/105/suit;To enlighten driveways without diggings into the paving it is now possible with SUIT, an high performance luminaire that allows an easy and safe installation without recess thanks to its anchor flange.;https://www.simes.it/en/search/?q=5695;1;185;185;41;Surface mounted;MINISUIT DRIVEOVER 1 WINDOW;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRSUIT2.pdf;IP65/IP67;IK 10;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;5.0m;CRI80;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_09_Black;Simes_Minisuit_Photometrics : S.5695H
S.5695H.14_MINI SUIT_1 WINDOW_2700K_36lm_2.2W_Aluminium grey;S.5695H.14;0;2700;2.2;36;14 Aluminium Grey;2.33;3 years;220;240;230;156;n/a;I;https://www.simes.it/en/overview/105/suit;To enlighten driveways without diggings into the paving it is now possible with SUIT, an high performance luminaire that allows an easy and safe installation without recess thanks to its anchor flange.;https://www.simes.it/en/search/?q=5695;1;185;185;41;Surface mounted;MINISUIT DRIVEOVER 1 WINDOW;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRSUIT2.pdf;IP65/IP67;IK 10;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;5.0m;CRI80;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Minisuit_Photometrics : S.5695H
S.5695N.09_MINI SUIT_1 WINDOW_4000K_48lm_2.2W_Black;S.5695N.09;0;4000;2.2;48;09 Black;2.33;3 years;220;240;230;156;n/a;I;https://www.simes.it/en/overview/105/suit;To enlighten driveways without diggings into the paving it is now possible with SUIT, an high performance luminaire that allows an easy and safe installation without recess thanks to its anchor flange.;https://www.simes.it/en/search/?q=5695;1;185;185;41;Surface mounted;MINISUIT DRIVEOVER 1 WINDOW;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRSUIT2.pdf;IP65/IP67;IK 10;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;5.0m;CRI80;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_09_Black;Simes_Minisuit_Photometrics : S.5695N
S.5695N.14_MINI SUIT_1 WINDOW_4000K_48lm_2.2W_Aluminium grey;S.5695N.14;0;4000;2.2;48;14 Aluminium Grey;2.33;3 years;220;240;230;156;n/a;I;https://www.simes.it/en/overview/105/suit;To enlighten driveways without diggings into the paving it is now possible with SUIT, an high performance luminaire that allows an easy and safe installation without recess thanks to its anchor flange.;https://www.simes.it/en/search/?q=5695;1;185;185;41;Surface mounted;MINISUIT DRIVEOVER 1 WINDOW;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRSUIT2.pdf;IP65/IP67;IK 10;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;5.0m;CRI80;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Minisuit_Photometrics : S.5695N
S.5695W.09_MINI SUIT_1 WINDOW_3000K_38lm_2.2W_Black;S.5695W.09;0;3000;2.2;38;09 Black;2.33;3 years;220;240;230;156;n/a;I;https://www.simes.it/en/overview/105/suit;To enlighten driveways without diggings into the paving it is now possible with SUIT, an high performance luminaire that allows an easy and safe installation without recess thanks to its anchor flange.;https://www.simes.it/en/search/?q=5695;1;185;185;41;Surface mounted;MINISUIT DRIVEOVER 1 WINDOW;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRSUIT2.pdf;IP65/IP67;IK 10;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;5.0m;CRI80;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_09_Black;Simes_Minisuit_Photometrics : S.5695W
S.5695W.14_MINI SUIT_1 WINDOW_3000K_38lm_2.2W_Aluminium grey;S.5695W.14;0;3000;2.2;38;14 Aluminium Grey;2.33;3 years;220;240;230;156;n/a;I;https://www.simes.it/en/overview/105/suit;To enlighten driveways without diggings into the paving it is now possible with SUIT, an high performance luminaire that allows an easy and safe installation without recess thanks to its anchor flange.;https://www.simes.it/en/search/?q=5695;1;185;185;41;Surface mounted;MINISUIT DRIVEOVER 1 WINDOW;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRSUIT2.pdf;IP65/IP67;IK 10;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;5.0m;CRI80;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Minisuit_Photometrics : S.5695W
