;SIMES_Product Code##OTHER##;SIMES_Beam Angle##ANGLE##DEGREES;SIMES_Color Temperature##COLOR_TEMPERATURE##KELVIN;SIMES_Rated Wattage##ELECTRICAL_POWER##WATTS;SIMES_Rated Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;SIMES_Finishes##OTHER##;SIMES_Weigth##MASS##KILOGRAMS;SIMES_Warranty Period##OTHER##;SIMES_Supply Voltage Min##ELECTRICAL_POTENTIAL##VOLTS;SIMES_Supply Voltage Max##ELECTRICAL_POTENTIAL##VOLTS;SIMES_Supply Voltage##ELECTRICAL_POTENTIAL##VOLTS;SIMES_Source Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;SIMES_Remote Power Supply##OTHER##;SIMES_Protection Class##OTHER##;SIMES_Product Page URL##OTHER##;SIMES_Product Description##OTHER##;SIMES_Product Data Sheet URL##OTHER##;SIMES_Number of Poles##OTHER##;SIMES_Nominal Width##LENGTH##MILLIMETERS;SIMES_Nominal Length##LENGTH##MILLIMETERS;SIMES_Nominal Height##LENGTH##MILLIMETERS;SIMES_Mounting Type##OTHER##;SIMES_Model##OTHER##;SIMES_Material Description##OTHER##;SIMES_Manufacturer Comment##OTHER##;SIMES_Luminous Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;SIMES_Light Source Type##OTHER##;SIMES_Lamp Count##OTHER##;SIMES_Installation Note URL##OTHER##;SIMES_IP Rating##OTHER##;SIMES_IK Rating##OTHER##;SIMES_Frequency##OTHER##;SIMES_Energy Efficiency Class##OTHER##;SIMES_Dimmable##OTHER##;SIMES_Current##ELECTRICAL_CURRENT##AMPERES;SIMES_Control Gear##OTHER##;SIMES_Cable Length##OTHER##;SIMES_CRI##OTHER##;SIMES_Approval Mark##OTHER##;LightFixturePlacingType##OTHER##;LightFixtureMountingType##OTHER##;Light Source##OTHER##;HasProtectiveEarth##OTHER##;Ground Stake##OTHER##;Body##OTHER##;Photometric_Type##OTHER##
S.6325H.14_MARKER_2700K_92lm_8.3W_Aluminium grey;S.6325H.14;0;2700;8.3;92;14 Aluminium Grey;1.15;3 years;220;240;230;503;n/a;I;https://www.simes.it/en/overview/107/marker;MARKER is a luminaire designed to illuminate stairs and to be recessed in the riser of the steps.;https://www.simes.it/en/search/?q=6325;1;86;310;65;Wall recessed;MARKER WALL RECESSED;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRMARKER2.pdf;IP65;IK 10;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;0.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Marker_Photometrics : S.6325H
S.6325N.14_MARKER_4000K_104lm_8.3W_Aluminium grey;S.6325N.14;0;4000;8.3;104;14 Aluminium Grey;1.15;3 years;220;240;230;572;n/a;I;https://www.simes.it/en/overview/107/marker;MARKER is a luminaire designed to illuminate stairs and to be recessed in the riser of the steps.;https://www.simes.it/en/search/?q=6325;1;86;310;65;Wall recessed;MARKER WALL RECESSED;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRMARKER2.pdf;IP65;IK 10;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;0.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Marker_Photometrics : S.6325N
S.6325W.14_MARKER_3000K_97lm_8.3W_Aluminium grey;S.6325W.14;0;3000;8.3;97;14 Aluminium Grey;1.15;3 years;220;240;230;530;n/a;I;https://www.simes.it/en/overview/107/marker;MARKER is a luminaire designed to illuminate stairs and to be recessed in the riser of the steps.;https://www.simes.it/en/search/?q=6325;1;86;310;65;Wall recessed;MARKER WALL RECESSED;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRMARKER2.pdf;IP65;IK 10;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;0.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Marker_Photometrics : S.6325W
