;SIMES_Product Code##OTHER##;SIMES_Beam Angle##ANGLE##DEGREES;SIMES_Color Temperature##COLOR_TEMPERATURE##KELVIN;SIMES_Rated Wattage##ELECTRICAL_POWER##WATTS;SIMES_Rated Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;SIMES_Finishes##OTHER##;SIMES_Weigth##MASS##KILOGRAMS;SIMES_Warranty Period##OTHER##;SIMES_Supply Voltage Min##ELECTRICAL_POTENTIAL##VOLTS;SIMES_Supply Voltage Max##ELECTRICAL_POTENTIAL##VOLTS;SIMES_Supply Voltage##ELECTRICAL_POTENTIAL##VOLTS;SIMES_Source Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;SIMES_Remote Power Supply##OTHER##;SIMES_Protection Class##OTHER##;SIMES_Product Page URL##OTHER##;SIMES_Product Description##OTHER##;SIMES_Product Data Sheet URL##OTHER##;SIMES_Number of Poles##OTHER##;SIMES_Nominal Width##LENGTH##MILLIMETERS;SIMES_Nominal Length##LENGTH##MILLIMETERS;SIMES_Nominal Height##LENGTH##MILLIMETERS;SIMES_Mounting Type##OTHER##;SIMES_Model##OTHER##;SIMES_Material Description##OTHER##;SIMES_Manufacturer Comment##OTHER##;SIMES_Luminous Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;SIMES_Light Source Type##OTHER##;SIMES_Lamp Count##OTHER##;SIMES_Installation Note URL##OTHER##;SIMES_IP Rating##OTHER##;SIMES_IK Rating##OTHER##;SIMES_Frequency##OTHER##;SIMES_Energy Efficiency Class##OTHER##;SIMES_Dimmable##OTHER##;SIMES_Current##ELECTRICAL_CURRENT##AMPERES;SIMES_Control Gear##OTHER##;SIMES_Cable Length##OTHER##;SIMES_CRI##OTHER##;SIMES_Approval Mark##OTHER##;LightFixturePlacingType##OTHER##;LightFixtureMountingType##OTHER##;Light Source##OTHER##;HasProtectiveEarth##OTHER##;Ground Stake##OTHER##;Body##OTHER##;Photometric_Type##OTHER##
S.1910H.14_OVER-ALL_12°_2700K_1598lm_18.3W_Aluminium grey;S.1910H.14;12;2700;18.3;1598;14 Aluminium Grey;1.8;3 years;0;0;0;1667;need remote power supply type S.3423 230V/700mA 39W;III;https://www.simes.it/en/overview/153/over-all;Over-all is an up-light of easy and immediate application: a special nylon fixing plate isolating it from the ground, is directly fixed to the surface without any recessed in-ground device.;https://www.simes.it/en/search/?q=1910;1;260;260;31;Surface Up-light;Over-all 11°;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTROVERALL.pdf;IP65/IP67;IK 09;DC 0Hz;A+;yes;0.7;n/a;5.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Over-all_Photometrics : S.1910H
S.1910H.24_OVER-ALL_12°_2700K_1598lm_18.3W_Anthracite grey;S.1910H.24;12;2700;18.3;1598;24 Anthracite Grey;1.8;3 years;0;0;0;1667;need remote power supply type S.3423 230V/700mA 39W;III;https://www.simes.it/en/overview/153/over-all;Over-all is an up-light of easy and immediate application: a special nylon fixing plate isolating it from the ground, is directly fixed to the surface without any recessed in-ground device.;https://www.simes.it/en/search/?q=1910;1;260;260;31;Surface Up-light;Over-all 11°;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTROVERALL.pdf;IP65/IP67;IK 09;DC 0Hz;A+;yes;0.7;n/a;5.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_24_Anthracyte grey;Simes_Over-all_Photometrics : S.1910H
S.1910N.14_OVER-ALL_12°_4000K_1888lm_18.3W_Aluminium grey;S.1910N.14;12;4000;18.3;1888;14 Aluminium Grey;1.8;3 years;0;0;0;1895;need remote power supply type S.3423 230V/700mA 39W;III;https://www.simes.it/en/overview/153/over-all;Over-all is an up-light of easy and immediate application: a special nylon fixing plate isolating it from the ground, is directly fixed to the surface without any recessed in-ground device.;https://www.simes.it/en/search/?q=1910;1;260;260;31;Surface Up-light;Over-all 11°;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTROVERALL.pdf;IP65/IP67;IK 08;DC 0Hz;A+;yes;0.7;n/a;5.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Over-all_Photometrics : S.1910N
S.1910N.24_OVER-ALL_12°_4000K_1888lm_18.3W_Anthracite grey;S.1910N.24;12;4000;18.3;1888;24 Anthracite Grey;1.8;3 years;0;0;0;1895;need remote power supply type S.3423 230V/700mA 39W;III;https://www.simes.it/en/overview/153/over-all;Over-all is an up-light of easy and immediate application: a special nylon fixing plate isolating it from the ground, is directly fixed to the surface without any recessed in-ground device.;https://www.simes.it/en/search/?q=1910;1;260;260;31;Surface Up-light;Over-all 11°;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTROVERALL.pdf;IP65/IP67;IK 08;DC 0Hz;A+;yes;0.7;n/a;5.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_24_Anthracyte grey;Simes_Over-all_Photometrics : S.1910N
S.1910W.14_OVER-ALL_12°_3000K_1743lm_18.3W_Aluminium grey;S.1910W.14;12;3000;18.3;1743;14 Aluminium Grey;1.8;3 years;0;0;0;1755;need remote power supply type S.3423 230V/700mA 39W;III;https://www.simes.it/en/overview/153/over-all;Over-all is an up-light of easy and immediate application: a special nylon fixing plate isolating it from the ground, is directly fixed to the surface without any recessed in-ground device.;https://www.simes.it/en/search/?q=1910;1;260;260;31;Surface Up-light;Over-all 11°;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTROVERALL.pdf;IP65/IP67;IK 09;DC 0Hz;A+;yes;0.7;n/a;5.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Over-all_Photometrics : S.1910W
S.1910W.24_OVER-ALL_12°_3000K_1743lm_18.3W_Anthracite grey;S.1910W.24;12;3000;18.3;1743;24 Anthracite Grey;1.8;3 years;0;0;0;1755;need remote power supply type S.3423 230V/700mA 39W;III;https://www.simes.it/en/overview/153/over-all;Over-all is an up-light of easy and immediate application: a special nylon fixing plate isolating it from the ground, is directly fixed to the surface without any recessed in-ground device.;https://www.simes.it/en/search/?q=1910;1;260;260;31;Surface Up-light;Over-all 11°;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTROVERALL.pdf;IP65/IP67;IK 09;DC 0Hz;A+;yes;0.7;n/a;5.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_24_Anthracyte grey;Simes_Over-all_Photometrics : S.1910W
S.1911H.14_OVER-ALL_34°_2700K_1536lm_18.3W_Aluminium grey;S.1911H.14;34;2700;18.3;1536;14 Aluminium Grey;1.8;3 years;0;0;0;1667;need remote power supply type S.3423 230V/700mA 39W;III;https://www.simes.it/en/overview/153/over-all;Over-all is an up-light of easy and immediate application: a special nylon fixing plate isolating it from the ground, is directly fixed to the surface without any recessed in-ground device.;https://www.simes.it/en/search/?q=1911;1;260;260;31;Surface Up-light;Over-all 33°;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTROVERALL.pdf;IP65/IP67;IK 09;DC 0Hz;A+;yes;0.7;n/a;5.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Over-all_Photometrics : S.1911H
S.1911H.24_OVER-ALL_34°_2700K_1536lm_18.3W_Anthracite grey;S.1911H.24;34;2700;18.3;1536;24 Anthracite Grey;1.8;3 years;0;0;0;1667;need remote power supply type S.3423 230V/700mA 39W;III;https://www.simes.it/en/overview/153/over-all;Over-all is an up-light of easy and immediate application: a special nylon fixing plate isolating it from the ground, is directly fixed to the surface without any recessed in-ground device.;https://www.simes.it/en/search/?q=1911;1;260;260;31;Surface Up-light;Over-all 33°;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTROVERALL.pdf;IP65/IP67;IK 09;DC 0Hz;A+;yes;0.7;n/a;5.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_24_Anthracyte grey;Simes_Over-all_Photometrics : S.1911H
S.1911N.14_OVER-ALL_34°_4000K_1816lm_18.3W_Aluminium grey;S.1911N.14;34;4000;18.3;1816;14 Aluminium Grey;1.8;3 years;0;0;0;1895;need remote power supply type S.3423 230V/700mA 39W;III;https://www.simes.it/en/overview/153/over-all;Over-all is an up-light of easy and immediate application: a special nylon fixing plate isolating it from the ground, is directly fixed to the surface without any recessed in-ground device.;https://www.simes.it/en/search/?q=1911;1;260;260;31;Surface Up-light; Over-all 33°;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTROVERALL.pdf;IP65/IP67;IK 08;DC 0Hz;A+;yes;0.7;n/a;5.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Over-all_Photometrics : S.1911N
S.1911N.24_OVER-ALL_34°_4000K_1816lm_18.3W_Anthracite grey;S.1911N.24;34;4000;18.3;1816;24 Anthracite Grey;1.8;3 years;0;0;0;1895;need remote power supply type S.3423 230V/700mA 39W;III;https://www.simes.it/en/overview/153/over-all;Over-all is an up-light of easy and immediate application: a special nylon fixing plate isolating it from the ground, is directly fixed to the surface without any recessed in-ground device.;https://www.simes.it/en/search/?q=1911;1;260;260;31;Surface Up-light; Over-all 33°;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTROVERALL.pdf;IP65/IP67;IK 08;DC 0Hz;A+;yes;0.7;n/a;5.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_24_Anthracyte grey;Simes_Over-all_Photometrics : S.1911N
S.1911W.14_OVER-ALL_34°_3000K_1676lm_18.3W_Aluminium grey;S.1911W.14;34;3000;18.3;1676;14 Aluminium Grey;1.8;3 years;0;0;0;1755;need remote power supply type S.3423 230V/700mA 39W;III;https://www.simes.it/en/overview/153/over-all;Over-all is an up-light of easy and immediate application: a special nylon fixing plate isolating it from the ground, is directly fixed to the surface without any recessed in-ground device.;https://www.simes.it/en/search/?q=1911;1;260;260;31;Surface Up-light;Over-all 33°;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTROVERALL.pdf;IP65/IP67;IK 09;DC 0Hz;A+;yes;0.7;n/a;5.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Over-all_Photometrics : S.1911W
S.1911W.24_OVER-ALL_34°_3000K_1676lm_18.3W_Anthracite grey;S.1911W.24;34;3000;18.3;1676;24 Anthracite Grey;1.8;3 years;0;0;0;1755;need remote power supply type S.3423 230V/700mA 39W;III;https://www.simes.it/en/overview/153/over-all;Over-all is an up-light of easy and immediate application: a special nylon fixing plate isolating it from the ground, is directly fixed to the surface without any recessed in-ground device.;https://www.simes.it/en/search/?q=1911;1;260;260;31;Surface Up-light;Over-all 33°;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTROVERALL.pdf;IP65/IP67;IK 09;DC 0Hz;A+;yes;0.7;n/a;5.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_24_Anthracyte grey;Simes_Over-all_Photometrics : S.1911W
S.1915H.14_OVER-ALL_ASY_2700K_1473lm_18.3W_Aluminium grey;S.1915H.14;0;2700;18.3;1473;14 Aluminium Grey;1.8;3 years;0;0;0;1667;need remote power supply type S.3423 230V/700mA 39W;III;https://www.simes.it/en/overview/153/over-all;Over-all is an up-light of easy and immediate application: a special nylon fixing plate isolating it from the ground, is directly fixed to the surface without any recessed in-ground device.;https://www.simes.it/en/search/?q=1915;1;260;260;31;Surface Up-light;Over-all ASY;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTROVERALL.pdf;IP65/IP67;IK 09;DC 0Hz;A+;yes;0.7;n/a;5.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Over-all_Photometrics : S.1915H
S.1915H.24_OVER-ALL_ASY_2700K_1473lm_18.3W_Anthracite grey;S.1915H.24;0;2700;18.3;1473;24 Anthracite Grey;1.8;3 years;0;0;0;1667;need remote power supply type S.3423 230V/700mA 39W;III;https://www.simes.it/en/overview/153/over-all;Over-all is an up-light of easy and immediate application: a special nylon fixing plate isolating it from the ground, is directly fixed to the surface without any recessed in-ground device.;https://www.simes.it/en/search/?q=1915;1;260;260;31;Surface Up-light;Over-all ASY;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTROVERALL.pdf;IP65/IP67;IK 09;DC 0Hz;A+;yes;0.7;n/a;5.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_24_Anthracyte grey;Simes_Over-all_Photometrics : S.1915H
S.1915N.14_OVER-ALL_ASY_4000K_1741lm_18.3W_Aluminium grey;S.1915N.14;0;4000;18.3;1741;14 Aluminium Grey;1.8;3 years;0;0;0;1895;need remote power supply type S.3423 230V/700mA 39W;III;https://www.simes.it/en/overview/153/over-all;Over-all is an up-light of easy and immediate application: a special nylon fixing plate isolating it from the ground, is directly fixed to the surface without any recessed in-ground device.;https://www.simes.it/en/search/?q=1915;1;260;260;31;Surface Up-light;Over-all ASY;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTROVERALL.pdf;IP65/IP67;IK 08;DC 0Hz;A+;yes;0.7;n/a;5.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Over-all_Photometrics : S.1915N
S.1915N.24_OVER-ALL_ASY_4000K_1741lm_18.3W_Anthracite grey;S.1915N.24;0;4000;18.3;1741;24 Anthracite Grey;1.8;3 years;0;0;0;1895;need remote power supply type S.3423 230V/700mA 39W;III;https://www.simes.it/en/overview/153/over-all;Over-all is an up-light of easy and immediate application: a special nylon fixing plate isolating it from the ground, is directly fixed to the surface without any recessed in-ground device.;https://www.simes.it/en/search/?q=1915;1;260;260;31;Surface Up-light;Over-all ASY;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTROVERALL.pdf;IP65/IP67;IK 08;DC 0Hz;A+;yes;0.7;n/a;5.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_24_Anthracyte grey;Simes_Over-all_Photometrics : S.1915N
S.1915W.14_OVER-ALL_ASY_3000K_1606lm_18.3W_Aluminium grey;S.1915W.14;0;3000;18.3;1606;14 Aluminium Grey;1.8;3 years;0;0;0;1755;need remote power supply type S.3423 230V/700mA 39W;III;https://www.simes.it/en/overview/153/over-all;Over-all is an up-light of easy and immediate application: a special nylon fixing plate isolating it from the ground, is directly fixed to the surface without any recessed in-ground device.;https://www.simes.it/en/search/?q=1915;1;260;260;31;Surface Up-light;Over-all ASY;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTROVERALL.pdf;IP65/IP67;IK 09;DC 0Hz;A+;yes;0.7;n/a;5.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Over-all_Photometrics : S.1915W
S.1915W.24_OVER-ALL_ASY_3000K_1606lm_18.3W_Anthracite grey;S.1915W.24;0;3000;18.3;1606;24 Anthracite Grey;1.8;3 years;0;0;0;1755;need remote power supply type S.3423 230V/700mA 39W;III;https://www.simes.it/en/overview/153/over-all;Over-all is an up-light of easy and immediate application: a special nylon fixing plate isolating it from the ground, is directly fixed to the surface without any recessed in-ground device.;https://www.simes.it/en/search/?q=1915;1;260;260;31;Surface Up-light;Over-all ASY;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTROVERALL.pdf;IP65/IP67;IK 09;DC 0Hz;A+;yes;0.7;n/a;5.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_24_Anthracyte grey;Simes_Over-all_Photometrics : S.1915W
