;SIMES_Product Code##OTHER##;SIMES_Beam Angle##ANGLE##DEGREES;SIMES_Color Temperature##COLOR_TEMPERATURE##KELVIN;SIMES_Rated Wattage##ELECTRICAL_POWER##WATTS;SIMES_Rated Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;SIMES_Finishes##OTHER##;SIMES_Weigth##MASS##KILOGRAMS;SIMES_Warranty Period##OTHER##;SIMES_Supply Voltage Min##ELECTRICAL_POTENTIAL##VOLTS;SIMES_Supply Voltage Max##ELECTRICAL_POTENTIAL##VOLTS;SIMES_Supply Voltage##ELECTRICAL_POTENTIAL##VOLTS;SIMES_Source Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;SIMES_Remote Power Supply##OTHER##;SIMES_Protection Class##OTHER##;SIMES_Product Page URL##OTHER##;SIMES_Product Description##OTHER##;SIMES_Product Data Sheet URL##OTHER##;SIMES_Number of Poles##OTHER##;SIMES_Nominal Width##LENGTH##MILLIMETERS;SIMES_Nominal Length##LENGTH##MILLIMETERS;SIMES_Nominal Height##LENGTH##MILLIMETERS;SIMES_Mounting Type##OTHER##;SIMES_Model##OTHER##;SIMES_Material Description##OTHER##;SIMES_Manufacturer Comment##OTHER##;SIMES_Luminous Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;SIMES_Light Source Type##OTHER##;SIMES_Lamp Count##OTHER##;SIMES_Installation Note URL##OTHER##;SIMES_IP Rating##OTHER##;SIMES_IK Rating##OTHER##;SIMES_Frequency##OTHER##;SIMES_Energy Efficiency Class##OTHER##;SIMES_Dimmable##OTHER##;SIMES_Current##ELECTRICAL_CURRENT##AMPERES;SIMES_Control Gear##OTHER##;SIMES_Cable Length##OTHER##;SIMES_CRI##OTHER##;SIMES_Approval Mark##OTHER##;LightFixturePlacingType##OTHER##;LightFixtureMountingType##OTHER##;Light Source##OTHER##;HasProtectiveEarth##OTHER##;Ground Stake##OTHER##;Body##OTHER##;Photometric_Type##OTHER##
S.3354H.19_NANOLED_WALL RECESSED_45mm_2700K_11lm_0.8W_Stainless Steel;S.3354H.19;0;2700;0.8;11;19 Stainless Steel;0.6;3 years;24;24;24;58;need remote power supply type S.3400 230V/24V DC 10W;III;https://www.simes.it/en/overview/152/nanoled-stainless-steel-wall-recessed;Nanoled Stainless steel is a walk-over in-ground luminaire providing either well defined accent lighting or evocative markers.;https://www.simes.it/en/search/?q=3354;1;45;45;95;Wall recessed;NANOLED 45mm WALL RECESSED STAINLESS STEEL;Stainless steel body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRNANINOX-W.pdf;IP65/IP67;IK 08;DC;A+;yes;0;n/a;5.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_19_Stainless Steel;Simes_Nanoled_Round_Photometrics : S.3354H
S.3354N.19_NANOLED_WALL RECESSED_45mm_4000K_13lm_0.8W_Stainless Steel;S.3354N.19;0;4000;0.8;13;19 Stainless Steel;0.6;3 years;24;24;24;68;need remote power supply type S.3400 230V/24V DC 10W;III;https://www.simes.it/en/overview/152/nanoled-stainless-steel-wall-recessed;Nanoled Stainless steel is a walk-over in-ground luminaire providing either well defined accent lighting or evocative markers.;https://www.simes.it/en/search/?q=3354;1;45;95;95;Wall recessed;NANOLED 45mm WALL RECESSED STAINLESS STEEL;Stainless steel body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRNANINOX-W.pdf;IP65/IP67;IK 08;DC;A+;yes;0;n/a;5.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_19_Stainless Steel;Simes_Nanoled_Round_Photometrics : S.3354N
S.3354W.19_NANOLED_WALL RECESSED_45mm_3000K_12lm_0.8W_Stainless Steel;S.3354W.19;0;3000;0.8;12;19 Stainless Steel;0.6;3 years;24;24;24;62;need remote power supply type S.3400 230V/24V DC 10W;III;https://www.simes.it/en/overview/152/nanoled-stainless-steel-wall-recessed;Nanoled Stainless steel is a walk-over in-ground luminaire providing either well defined accent lighting or evocative markers.;https://www.simes.it/en/search/?q=3354;1;45;45;95;Wall recessed;NANOLED 45mm WALL RECESSED STAINLESS STEEL;Stainless steel body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRNANINOX-W.pdf;IP65/IP67;IK 08;DC;A+;yes;0;n/a;5.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_19_Stainless Steel;Simes_Nanoled_Round_Photometrics : S.3354W
