;SIMES_Product Code##OTHER##;SIMES_Beam Angle##ANGLE##DEGREES;SIMES_Color Temperature##COLOR_TEMPERATURE##KELVIN;SIMES_Rated Wattage##ELECTRICAL_POWER##WATTS;SIMES_Rated Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;SIMES_Finishes##OTHER##;SIMES_Weigth##MASS##KILOGRAMS;SIMES_Warranty Period##OTHER##;SIMES_Supply Voltage Min##ELECTRICAL_POTENTIAL##VOLTS;SIMES_Supply Voltage Max##ELECTRICAL_POTENTIAL##VOLTS;SIMES_Supply Voltage##ELECTRICAL_POTENTIAL##VOLTS;SIMES_Source Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;SIMES_Remote Power Supply##OTHER##;SIMES_Protection Class##OTHER##;SIMES_Product Page URL##OTHER##;SIMES_Product Description##OTHER##;SIMES_Product Data Sheet URL##OTHER##;SIMES_Number of Poles##OTHER##;SIMES_Nominal Width##LENGTH##MILLIMETERS;SIMES_Nominal Length##LENGTH##MILLIMETERS;SIMES_Nominal Height##LENGTH##MILLIMETERS;SIMES_Mounting Type##OTHER##;SIMES_Model##OTHER##;SIMES_Material Description##OTHER##;SIMES_Manufacturer Comment##OTHER##;SIMES_Luminous Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;SIMES_Light Source Type##OTHER##;SIMES_Lamp Count##OTHER##;SIMES_Installation Note URL##OTHER##;SIMES_IP Rating##OTHER##;SIMES_IK Rating##OTHER##;SIMES_Frequency##OTHER##;SIMES_Energy Efficiency Class##OTHER##;SIMES_Dimmable##OTHER##;SIMES_Current##ELECTRICAL_CURRENT##AMPERES;SIMES_Control Gear##OTHER##;SIMES_Cable Length##OTHER##;SIMES_CRI##OTHER##;SIMES_Approval Mark##OTHER##;LightFixturePlacingType##OTHER##;LightFixtureMountingType##OTHER##;Light Source##OTHER##;HasProtectiveEarth##OTHER##;Ground Stake##OTHER##;Body##OTHER##;Photometric_Type##OTHER##
S.2210N.01_5CENTO_RECTANGULAR_4000K_216lm_4.0W_White;S.2210N.01;0;4000;4.0;216;01 White;0.8;3 years;24;24;24;577;need remote power supply type S.2407 230V/24V DC 14.4W;III;https://www.simes.it/en/overview/171/5cento;5cento is a versatile step light with limited dimensions and a slim design that can be installed in plasterboard or brickwork. It can be fixed to the traditional electrical junction box or surface mounted.;https://www.simes.it/en/search/?q=2210;1;22;155;90;Wall mounted;5CENTO RECTANGULAR WALL MOUNTED;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTR5CENTO.pdf;IP65;IK 07;DC;A+;yes;0;n/a;0.5m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_01_White;Simes_5Cento_Photometrics : S.2210N
S.2210N.14_5CENTO_RECTANGULAR_4000K_216lm_4.0W_Aluminium grey;S.2210N.14;0;4000;4.0;216;14 Aluminium Grey;0.8;3 years;24;24;24;577;need remote power supply type S.2407 230V/24V DC 14.4W;III;https://www.simes.it/en/overview/171/5cento;5cento is a versatile step light with limited dimensions and a slim design that can be installed in plasterboard or brickwork. It can be fixed to the traditional electrical junction box or surface mounted.;https://www.simes.it/en/search/?q=2210;1;22;155;90;Wall mounted;5CENTO RECTANGULAR WALL MOUNTED;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTR5CENTO.pdf;IP65;IK 07;DC;A+;yes;0;n/a;0.5m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_5Cento_Photometrics : S.2210N
S.2210N.24_5CENTO_RECTANGULAR_4000K_216lm_4.0W_Antracyte grey;S.2210N.24;0;4000;4.0;216;24 Anthracite Grey;0.8;3 years;24;24;24;577;need remote power supply type S.2407 230V/24V DC 14.4W;III;https://www.simes.it/en/overview/171/5cento;5cento is a versatile step light with limited dimensions and a slim design that can be installed in plasterboard or brickwork. It can be fixed to the traditional electrical junction box or surface mounted.;https://www.simes.it/en/search/?q=2210;1;22;155;90;Wall mounted;5CENTO RECTANGULAR WALL MOUNTED;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTR5CENTO.pdf;IP65;IK 07;DC;A+;yes;0;n/a;0.5m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_24_Anthracyte grey;Simes_5Cento_Photometrics : S.2210N
S.2210H.01_5CENTO_RECTANGULAR_2700K_192lm_4.0W_White;S.2210H.01;0;2700;4.0;192;01 White;0.8;3 years;24;24;24;511;need remote power supply type S.2407 230V/24V DC 14.4W;III;https://www.simes.it/en/overview/171/5cento;5cento is a versatile step light with limited dimensions and a slim design that can be installed in plasterboard or brickwork. It can be fixed to the traditional electrical junction box or surface mounted.;https://www.simes.it/en/search/?q=2210;1;22;155;90;Wall mounted;5CENTO RECTANGULAR WALL MOUNTED;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTR5CENTO.pdf;IP65;IK 07;DC;A+;yes;0;n/a;0.5m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_01_White;Simes_5Cento_Photometrics : S.2210H
S.2210H.14_5CENTO_RECTANGULAR_2700K_192lm_4.0W_Aluminium grey;S.2210H.14;0;2700;4.0;192;14 Aluminium Grey;0.8;3 years;24;24;24;511;need remote power supply type S.2407 230V/24V DC 14.4W;III;https://www.simes.it/en/overview/171/5cento;5cento is a versatile step light with limited dimensions and a slim design that can be installed in plasterboard or brickwork. It can be fixed to the traditional electrical junction box or surface mounted.;https://www.simes.it/en/search/?q=2210;1;22;155;90;Wall mounted;5CENTO RECTANGULAR WALL MOUNTED;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTR5CENTO.pdf;IP65;IK 07;DC;A+;yes;0;n/a;0.5m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_5Cento_Photometrics : S.2210H
S.2210H.24_5CENTO_RECTANGULAR_2700K_192lm_4.0W_Antracyte grey;S.2210H.24;0;2700;4.0;192;24 Anthracite Grey;0.8;3 years;24;24;24;511;need remote power supply type S.2407 230V/24V DC 14.4W;III;https://www.simes.it/en/overview/171/5cento;5cento is a versatile step light with limited dimensions and a slim design that can be installed in plasterboard or brickwork. It can be fixed to the traditional electrical junction box or surface mounted.;https://www.simes.it/en/search/?q=2210;1;22;155;90;Wall mounted;5CENTO RECTANGULAR WALL MOUNTED;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTR5CENTO.pdf;IP65;IK 07;DC;A+;yes;0;n/a;0.5m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_24_Anthracyte grey;Simes_5Cento_Photometrics : S.2210H
S.2210W.01_5CENTO_RECTANGULAR_3000K_201lm_4.0W_White;S.2210W.01;0;3000;4.0;201;01 White;0.8;3 years;24;24;24;536;need remote power supply type S.2407 230V/24V DC 14.4W;III;https://www.simes.it/en/overview/171/5cento;5cento is a versatile step light with limited dimensions and a slim design that can be installed in plasterboard or brickwork. It can be fixed to the traditional electrical junction box or surface mounted.;https://www.simes.it/en/search/?q=2210;1;22;155;90;Wall mounted;5CENTO RECTANGULAR WALL MOUNTED;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTR5CENTO.pdf;IP65;IK 07;DC;A+;yes;0;n/a;0.5m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_01_White;Simes_5Cento_Photometrics : S.2210W
S.2210W.14_5CENTO_RECTANGULAR_3000K_201lm_4.0W_Aluminium grey;S.2210W.14;0;3000;4.0;201;14 Aluminium Grey;0.8;3 years;24;24;24;536;need remote power supply type S.2407 230V/24V DC 14.4W;III;https://www.simes.it/en/overview/171/5cento;5cento is a versatile step light with limited dimensions and a slim design that can be installed in plasterboard or brickwork. It can be fixed to the traditional electrical junction box or surface mounted.;https://www.simes.it/en/search/?q=2210;1;22;155;90;Wall mounted;5CENTO RECTANGULAR WALL MOUNTED;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTR5CENTO.pdf;IP65;IK 07;DC;A+;yes;0;n/a;0.5m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_5Cento_Photometrics : S.2210W
S.2210W.24_5CENTO_RECTANGULAR_3000K_201lm_4.0W_Antracyte grey;S.2210W.24;0;3000;4.0;210;24 Anthracite Grey;0.8;3 years;24;24;24;536;need remote power supply type S.2407 230V/24V DC 14.4W;III;https://www.simes.it/en/overview/171/5cento;5cento is a versatile step light with limited dimensions and a slim design that can be installed in plasterboard or brickwork. It can be fixed to the traditional electrical junction box or surface mounted.;https://www.simes.it/en/search/?q=2210;1;22;155;90;Wall mounted;5CENTO RECTANGULAR WALL MOUNTED;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTR5CENTO.pdf;IP65;IK 07;DC;A+;yes;0;n/a;0.5m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_24_Anthracyte grey;Simes_5Cento_Photometrics : S.2210W
