;SIMES_Product Code##OTHER##;SIMES_Beam Angle##ANGLE##DEGREES;SIMES_Color Temperature##COLOR_TEMPERATURE##KELVIN;SIMES_Rated Wattage##ELECTRICAL_POWER##WATTS;SIMES_Rated Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;SIMES_Finishes##OTHER##;SIMES_Weigth##MASS##KILOGRAMS;SIMES_Warranty Period##OTHER##;SIMES_Supply Voltage Min##ELECTRICAL_POTENTIAL##VOLTS;SIMES_Supply Voltage Max##ELECTRICAL_POTENTIAL##VOLTS;SIMES_Supply Voltage##ELECTRICAL_POTENTIAL##VOLTS;SIMES_Source Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;SIMES_Remote Power Supply##OTHER##;SIMES_Protection Class##OTHER##;SIMES_Product Page URL##OTHER##;SIMES_Product Description##OTHER##;SIMES_Product Data Sheet URL##OTHER##;SIMES_Number of Poles##OTHER##;SIMES_Nominal Width##LENGTH##MILLIMETERS;SIMES_Nominal Length##LENGTH##MILLIMETERS;SIMES_Nominal Height##LENGTH##MILLIMETERS;SIMES_Mounting Type##OTHER##;SIMES_Model##OTHER##;SIMES_Material Description##OTHER##;SIMES_Manufacturer Comment##OTHER##;SIMES_Luminous Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;SIMES_Light Source Type##OTHER##;SIMES_Lamp Count##OTHER##;SIMES_Installation Note URL##OTHER##;SIMES_IP Rating##OTHER##;SIMES_IK Rating##OTHER##;SIMES_Frequency##OTHER##;SIMES_Energy Efficiency Class##OTHER##;SIMES_Dimmable##OTHER##;SIMES_Current##ELECTRICAL_CURRENT##AMPERES;SIMES_Control Gear##OTHER##;SIMES_Cable Length##OTHER##;SIMES_CRI##OTHER##;SIMES_Approval Mark##OTHER##;LightFixturePlacingType##OTHER##;LightFixtureMountingType##OTHER##;Light Source##OTHER##;HasProtectiveEarth##OTHER##;Ground Stake##OTHER##;Body##OTHER##;Photometric_Type##OTHER##
S.5097H.09_MINILIFT_4 WINDOWS_43°_2700K_144lm_11.4W_Black;S.5097H.09;43;2700;11.4;144;09 Black;1.4;3 years;220;240;230;646;n/a;II;https://www.simes.it/en/overview/27/lift;Wall effect of a rigorous geometry design, LIFT fits perfectly in different architectural environments personalizing any context in a clear way.;https://www.simes.it/en/search/?q=5097;1;120;140;120;Wall mounted;MINILIFT SQUARE 4 WINDOW 43°;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTMINILIFT2.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;0.0m;CRI80;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_09_Black;Simes_Lift_Photometrics : S.5077H
S.5097H.14_MINILIFT_4 WINDOWS_43°_2700K_144lm_11.4W_Aluminium grey;S.5097H.14;43;2700;11.4;144;14 Aluminium Grey;1.4;3 years;220;240;230;646;n/a;II;https://www.simes.it/en/overview/27/lift;Wall effect of a rigorous geometry design, LIFT fits perfectly in different architectural environments personalizing any context in a clear way.;https://www.simes.it/en/search/?q=5097;1;120;140;120;Wall mounted;MINILIFT SQUARE 4 WINDOW 43°;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTMINILIFT2.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;0.0m;CRI80;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Lift_Photometrics : S.5077H
S.5097N.09_MINILIFT_4 WINDOWS_43°_4000K_164lm_11.4W_Black;S.5097N.09;43;4000;11.4;164;09 Black;1.4;3 years;220;240;230;736;n/a;II;https://www.simes.it/en/overview/27/lift;Wall effect of a rigorous geometry design, LIFT fits perfectly in different architectural environments personalizing any context in a clear way.;https://www.simes.it/en/search/?q=5097;1;120;140;120;Wall mounted;MINILIFT SQUARE 4 WINDOW 43°;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTMINILIFT2.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;0.0m;CRI80;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_09_Black;Simes_Lift_Photometrics : S.5077N
S.5097N.14_MINILIFT_4 WINDOWS_43°_4000K_164lm_11.4W_Aluminium grey;S.5097N.14;43;4000;11.4;164;14 Aluminium Grey;1.4;3 years;220;240;230;736;n/a;II;https://www.simes.it/en/overview/27/lift;Wall effect of a rigorous geometry design, LIFT fits perfectly in different architectural environments personalizing any context in a clear way.;https://www.simes.it/en/search/?q=5097;1;120;140;120;Wall mounted;MINILIFT SQUARE 4 WINDOW 43°;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTMINILIFT2.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;0.0m;CRI80;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Lift_Photometrics : S.5077N
S.5097W.09_MINILIFT_4 WINDOWS_43°_3000K_152lm_11.4W_Black;S.5097W.09;43;3000;11.4;152;09 Black;1.4;3 years;220;240;230;680;n/a;II;https://www.simes.it/en/overview/27/lift;Wall effect of a rigorous geometry design, LIFT fits perfectly in different architectural environments personalizing any context in a clear way.;https://www.simes.it/en/search/?q=5097;1;120;140;120;Wall mounted;MINILIFT SQUARE 4 WINDOW 43°;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTMINILIFT2.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;0.0m;CRI80;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_09_Black;Simes_Lift_Photometrics : S.5077W
S.5097W.14_MINILIFT_4 WINDOWS_43°_3000K_152lm_11.4W_Aluminium grey;S.5097W.14;43;3000;11.4;152;14 Aluminium Grey;1.4;3 years;220;240;230;680;n/a;II;https://www.simes.it/en/overview/27/lift;Wall effect of a rigorous geometry design, LIFT fits perfectly in different architectural environments personalizing any context in a clear way.;https://www.simes.it/en/search/?q=5097;1;120;140;120;Wall mounted;MINILIFT SQUARE 4 WINDOW 43°;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTMINILIFT2.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;0.0m;CRI80;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Lift_Photometrics : S.5077W
S.5087H.09_MINILIFT_4 WINDOWS_3°_2700K_76lm_11.4W_Black;S.5087H.09;3;2700;11.4;76;09 Black;1.4;3 years;220;240;230;646;n/a;II;https://www.simes.it/en/overview/27/lift;Wall effect of a rigorous geometry design, LIFT fits perfectly in different architectural environments personalizing any context in a clear way.;https://www.simes.it/en/search/?q=5087;1;120;140;120;Wall mounted;MINILIFT SQUARE 4 WINDOW 3°;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTMINILIFT2.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;0.0m;CRI80;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_09_Black;Simes_Lift_Photometrics : S.5067H
S.5087H.14_MINILIFT_4 WINDOWS_3°_2700K_76lm_11.4W_Aluminium grey;S.5087H.14;3;2700;11.4;76;14 Aluminium Grey;1.4;3 years;220;240;230;646;n/a;II;https://www.simes.it/en/overview/27/lift;Wall effect of a rigorous geometry design, LIFT fits perfectly in different architectural environments personalizing any context in a clear way.;https://www.simes.it/en/search/?q=5087;1;120;140;120;Wall mounted;MINILIFT SQUARE 4 WINDOW 3°;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTMINILIFT2.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;0.0m;CRI80;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Lift_Photometrics : S.5067H
S.5087N.09_MINILIFT_4 WINDOWS_3°_4000K_88lm_11.4W_Black;S.5087N.09;3;4000;11.4;88;09 Black;1.4;3 years;220;240;230;736;n/a;II;https://www.simes.it/en/overview/27/lift;Wall effect of a rigorous geometry design, LIFT fits perfectly in different architectural environments personalizing any context in a clear way.;https://www.simes.it/en/search/?q=5087;1;120;140;120;Wall mounted;MINILIFT SQUARE 4 WINDOW 3°;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTMINILIFT2.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;0.0m;CRI80;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_09_Black;Simes_Lift_Photometrics : S.5067N
S.5087N.14_MINILIFT_4 WINDOWS_3°_4000K_88lm_11.4W_Aluminium grey;S.5087N.14;3;4000;11.4;88;14 Aluminium Grey;1.4;3 years;220;240;230;736;n/a;II;https://www.simes.it/en/overview/27/lift;Wall effect of a rigorous geometry design, LIFT fits perfectly in different architectural environments personalizing any context in a clear way.;https://www.simes.it/en/search/?q=5087;1;120;140;120;Wall mounted;MINILIFT SQUARE 4 WINDOW 3°;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTMINILIFT2.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;0.0m;CRI80;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Lift_Photometrics : S.5067N
S.5087W.09_MINILIFT_4 WINDOWS_3°_3000K_80lm_11.4W_Black;S.5087W.09;3;3000;11.4;80;09 Black;1.4;3 years;220;240;230;680;n/a;II;https://www.simes.it/en/overview/27/lift;Wall effect of a rigorous geometry design, LIFT fits perfectly in different architectural environments personalizing any context in a clear way.;https://www.simes.it/en/search/?q=5087;1;120;140;120;Wall mounted;MINILIFT SQUARE 4 WINDOW 3°;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTMINILIFT2.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;0.0m;CRI80;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_09_Black;Simes_Lift_Photometrics : S.5067W
S.5087W.14_MINILIFT_4 WINDOWS_3°_3000K_80lm_11.4W_Aluminium grey;S.5087W.14;3;3000;11.4;80;14 Aluminium Grey;1.4;3 years;220;240;230;680;n/a;II;https://www.simes.it/en/overview/27/lift;Wall effect of a rigorous geometry design, LIFT fits perfectly in different architectural environments personalizing any context in a clear way.;https://www.simes.it/en/search/?q=5087;1;120;140;120;Wall mounted;MINILIFT SQUARE 4 WINDOW 3°;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTMINILIFT2.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;0.0m;CRI80;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Lift_Photometrics : S.5067W
