;SIMES_Product Code##OTHER##;SIMES_Beam Angle##ANGLE##DEGREES;SIMES_Color Temperature##COLOR_TEMPERATURE##KELVIN;SIMES_Rated Wattage##ELECTRICAL_POWER##WATTS;SIMES_Rated Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;SIMES_Finishes##OTHER##;SIMES_Weigth##MASS##KILOGRAMS;SIMES_Warranty Period##OTHER##;SIMES_Supply Voltage Min##ELECTRICAL_POTENTIAL##VOLTS;SIMES_Supply Voltage Max##ELECTRICAL_POTENTIAL##VOLTS;SIMES_Supply Voltage##ELECTRICAL_POTENTIAL##VOLTS;SIMES_Source Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;SIMES_Remote Power Supply##OTHER##;SIMES_Protection Class##OTHER##;SIMES_Product Page URL##OTHER##;SIMES_Product Description##OTHER##;SIMES_Product Data Sheet URL##OTHER##;SIMES_Number of Poles##OTHER##;SIMES_Nominal Width##LENGTH##MILLIMETERS;SIMES_Nominal Length##LENGTH##MILLIMETERS;SIMES_Nominal Height##LENGTH##MILLIMETERS;SIMES_Mounting Type##OTHER##;SIMES_Model##OTHER##;SIMES_Material Description##OTHER##;SIMES_Manufacturer Comment##OTHER##;SIMES_Luminous Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;SIMES_Light Source Type##OTHER##;SIMES_Lamp Count##OTHER##;SIMES_Installation Note URL##OTHER##;SIMES_IP Rating##OTHER##;SIMES_IK Rating##OTHER##;SIMES_Frequency##OTHER##;SIMES_Energy Efficiency Class##OTHER##;SIMES_Dimmable##OTHER##;SIMES_Current##ELECTRICAL_CURRENT##AMPERES;SIMES_Control Gear##OTHER##;SIMES_Cable Length##OTHER##;SIMES_CRI##OTHER##;SIMES_Approval Mark##OTHER##;LightFixturePlacingType##OTHER##;LightFixtureMountingType##OTHER##;Light Source##OTHER##;HasProtectiveEarth##OTHER##;Ground Stake##OTHER##;Body##OTHER##;Photometric_Type##OTHER##
S.6260H.01_SKILL SQUARE WALL_2700K_438lm_8.1W_White;S.6260H.01;0;2700;8.1;438;01 White;1.2;3 years;220;240;230;1319;n/a;I;https://www.simes.it/en/overview/98/skill;"SKILL represents a new concept of outdoor lighting fitting; a recessed/not-recessed luminaire for wall mounting. It concentrates all the advantages of a recessed fitting, but without requiring a housing in the wall.";https://www.simes.it/en/search/?q=6260;1;30;200;200;Wall mounted;SKILL SQUARE WALL MOUNTED;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRSKILL2.pdf;IP65;IK 08;AC 50-60Hz / DC;A+;PHASE-CUT;0;Electronic ballast;0.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_01_White;Simes_Skill_Photometrics : S.6260H
S.6260H.14_SKILL SQUARE WALL_2700K_438lm_8.1W_Aluminium grey;S.6260H.14;0;2700;8.1;438;14 Aluminium Grey;1.2;3 years;220;240;230;1319;n/a;I;https://www.simes.it/en/overview/98/skill;"SKILL represents a new concept of outdoor lighting fitting; a recessed/not-recessed luminaire for wall mounting. It concentrates all the advantages of a recessed fitting, but without requiring a housing in the wall.";https://www.simes.it/en/search/?q=6260;1;30;200;200;Wall mounted;SKILL SQUARE WALL MOUNTED;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRSKILL2.pdf;IP65;IK 08;AC 50-60Hz / DC;A+;PHASE-CUT;0;Electronic ballast;0.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Skill_Photometrics : S.6260H
S.6260H.24_SKILL SQUARE WALL_2700K_438lm_8.1W_Anthracite grey;S.6260H.24;0;2700;8.1;438;24 Anthracite Grey;1.2;3 years;220;240;230;1319;n/a;I;https://www.simes.it/en/overview/98/skill;"SKILL represents a new concept of outdoor lighting fitting; a recessed/not-recessed luminaire for wall mounting. It concentrates all the advantages of a recessed fitting, but without requiring a housing in the wall.";https://www.simes.it/en/search/?q=6260;1;30;200;200;Wall mounted;SKILL SQUARE WALL MOUNTED;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRSKILL2.pdf;IP65;IK 08;AC 50-60Hz / DC;A+;PHASE-CUT;0;Electronic ballast;0.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_24_Anthracyte grey;Simes_Skill_Photometrics : S.6260H
S.6260N.01_SKILL SQUARE WALL_4000K_461lm_8.1W_White;S.6260N.01;0;4000;8.1;461;01 White;1.2;3 years;220;240;230;1764;n/a;I;https://www.simes.it/en/overview/98/skill;"SKILL represents a new concept of outdoor lighting fitting; a recessed/not-recessed luminaire for wall mounting. It concentrates all the advantages of a recessed fitting, but without requiring a housing in the wall.";https://www.simes.it/en/search/?q=6260;1;30;200;200;Wall mounted;SKILL SQUARE WALL MOUNTED;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRSKILL2.pdf;IP65;IK 08;AC 50-60Hz / DC;A+;PHASE-CUT;0;Electronic ballast;0.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_01_White;Simes_Skill_Photometrics : S.6260N
S.6260N.14_SKILL SQUARE WALL_4000K_461lm_8.1W_Aluminium grey;S.6260N.14;0;4000;8.1;461;14 Aluminium Grey;1.2;3 years;220;240;230;1764;n/a;I;https://www.simes.it/en/overview/98/skill;"SKILL represents a new concept of outdoor lighting fitting; a recessed/not-recessed luminaire for wall mounting. It concentrates all the advantages of a recessed fitting, but without requiring a housing in the wall.";https://www.simes.it/en/search/?q=6260;1;30;200;200;Wall mounted;SKILL SQUARE WALL MOUNTED;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRSKILL2.pdf;IP65;IK 08;AC 50-60Hz / DC;A+;PHASE-CUT;0;Electronic ballast;0.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Skill_Photometrics : S.6260N
S.6260N.24_SKILL SQUARE WALL_4000K_461lm_8.1W_Anthracite grey;S.6260N.24;0;4000;8.1;461;24 Anthracite Grey;1.2;3 years;220;240;230;1764;n/a;I;https://www.simes.it/en/overview/98/skill;"SKILL represents a new concept of outdoor lighting fitting; a recessed/not-recessed luminaire for wall mounting. It concentrates all the advantages of a recessed fitting, but without requiring a housing in the wall.";https://www.simes.it/en/search/?q=6260;1;30;200;200;Wall mounted;SKILL SQUARE WALL MOUNTED;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRSKILL2.pdf;IP65;IK 08;AC 50-60Hz / DC;A+;PHASE-CUT;0;Electronic ballast;0.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_24_Anthracyte grey;Simes_Skill_Photometrics : S.6260N
S.6260W.01_SKILL SQUARE WALL_3000K_451lm_8.1W_White;S.6260W.01;0;3000;8.1;451;01 White;1.2;3 years;220;240;230;1357;n/a;I;https://www.simes.it/en/overview/98/skill;"SKILL represents a new concept of outdoor lighting fitting; a recessed/not-recessed luminaire for wall mounting. It concentrates all the advantages of a recessed fitting, but without requiring a housing in the wall.";https://www.simes.it/en/search/?q=6260;1;30;200;200;Wall mounted;SKILL SQUARE WALL MOUNTED;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRSKILL2.pdf;IP65;IK 08;AC 50-60Hz / DC;A+;PHASE-CUT;0;Electronic ballast;0.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_01_White;Simes_Skill_Photometrics : S.6260W
S.6260W.14_SKILL SQUARE WALL_3000K_451lm_8.1W_Aluminium grey;S.6260W.14;0;3000;8.1;451;14 Aluminium Grey;1.2;3 years;220;240;230;1357;n/a;I;https://www.simes.it/en/overview/98/skill;"SKILL represents a new concept of outdoor lighting fitting; a recessed/not-recessed luminaire for wall mounting. It concentrates all the advantages of a recessed fitting, but without requiring a housing in the wall.";https://www.simes.it/en/search/?q=6260;1;30;200;200;Wall mounted;SKILL SQUARE WALL MOUNTED;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRSKILL2.pdf;IP65;IK 08;AC 50-60Hz / DC;A+;PHASE-CUT;0;Electronic ballast;0.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Skill_Photometrics : S.6260W
S.6260W.24_SKILL SQUARE WALL_3000K_451lm_8.1W_Anthracite grey;S.6260W.24;0;3000;8.1;451;24 Anthracite Grey;1.2;3 years;220;240;230;1357;n/a;I;https://www.simes.it/en/overview/98/skill;"SKILL represents a new concept of outdoor lighting fitting; a recessed/not-recessed luminaire for wall mounting. It concentrates all the advantages of a recessed fitting, but without requiring a housing in the wall.";https://www.simes.it/en/search/?q=6260;1;30;200;200;Wall mounted;SKILL SQUARE WALL MOUNTED;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRSKILL2.pdf;IP65;IK 08;AC 50-60Hz / DC;A+;PHASE-CUT;0;Electronic ballast;0.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_24_Anthracyte grey;Simes_Skill_Photometrics : S.6260W
