;SIMES_Product Code##OTHER##;SIMES_Beam Angle##ANGLE##DEGREES;SIMES_Color Temperature##COLOR_TEMPERATURE##KELVIN;SIMES_Rated Wattage##ELECTRICAL_POWER##WATTS;SIMES_Rated Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;SIMES_Finishes##OTHER##;SIMES_Weigth##MASS##KILOGRAMS;SIMES_Warranty Period##OTHER##;SIMES_Supply Voltage Min##ELECTRICAL_POTENTIAL##VOLTS;SIMES_Supply Voltage Max##ELECTRICAL_POTENTIAL##VOLTS;SIMES_Supply Voltage##ELECTRICAL_POTENTIAL##VOLTS;SIMES_Source Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;SIMES_Remote Power Supply##OTHER##;SIMES_Protection Class##OTHER##;SIMES_Product Page URL##OTHER##;SIMES_Product Description##OTHER##;SIMES_Product Data Sheet URL##OTHER##;SIMES_Number of Poles##OTHER##;SIMES_Nominal Width##LENGTH##MILLIMETERS;SIMES_Nominal Length##LENGTH##MILLIMETERS;SIMES_Nominal Height##LENGTH##MILLIMETERS;SIMES_Mounting Type##OTHER##;SIMES_Model##OTHER##;SIMES_Material Description##OTHER##;SIMES_Manufacturer Comment##OTHER##;SIMES_Luminous Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;SIMES_Light Source Type##OTHER##;SIMES_Lamp Count##OTHER##;SIMES_Installation Note URL##OTHER##;SIMES_IP Rating##OTHER##;SIMES_IK Rating##OTHER##;SIMES_Frequency##OTHER##;SIMES_Energy Efficiency Class##OTHER##;SIMES_Dimmable##OTHER##;SIMES_Current##ELECTRICAL_CURRENT##AMPERES;SIMES_Control Gear##OTHER##;SIMES_Cable Length##OTHER##;SIMES_CRI##OTHER##;SIMES_Approval Mark##OTHER##;LightFixturePlacingType##OTHER##;LightFixtureMountingType##OTHER##;Light Source##OTHER##;HasProtectiveEarth##OTHER##;Ground Stake##OTHER##;Body##OTHER##;Photometric_Type##OTHER##
S.6622N.01_MICROLOFT WALL_7°x28°_4000K_80lm_2.2W_White;S.6622N.01;0;4000;2.2;80;01 White;0.5;3 years;220;240;230;113;n/a;II;https://www.simes.it/en/overview/29/loft-round;A complete set of fittings available in three sizes with different light sources allowing for diverse applications.;https://www.simes.it/en/search/?q=6622;1;60;60;60;Wall mounted;MICROLOFT ROUND WALL 7°x28°;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRLOFTTONDO2.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;0.6m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_01_White;Simes_Microloft_Photometrics : S.6622N
S.6622N.14_MICROLOFT WALL_7°x28°_4000K_80lm_2.2W_Aluminium grey;S.6622N.14;0;4000;2.2;80;14 Aluminium Grey;0.5;3 years;220;240;230;113;n/a;II;https://www.simes.it/en/overview/29/loft-round;A complete set of fittings available in three sizes with different light sources allowing for diverse applications.;https://www.simes.it/en/search/?q=6622;1;60;60;60;Wall mounted;MICROLOFT ROUND WALL 7°x28°;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRLOFTTONDO2.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;0.6m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Microloft_Photometrics : S.6622N
S.6622N.24_MICROLOFT WALL_7°x28°_4000K_80lm_2.2W_Anthracite grey;S.6622N.24;0;4000;2.2;80;24 Anthracite Grey;0.5;3 years;220;240;230;113;n/a;II;https://www.simes.it/en/overview/29/loft-round;A complete set of fittings available in three sizes with different light sources allowing for diverse applications.;https://www.simes.it/en/search/?q=6622;1;60;60;60;Wall mounted;MICROLOFT ROUND WALL 7°x28°;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRLOFTTONDO2.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;0.6m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_24_Anthracyte grey;Simes_Microloft_Photometrics : S.6622N
S.6622W.01_MICROLOFT WALL_7°x28°_3000K_74lm_2.2W_White;S.6622W.01;0;3000;2.2;74;01 White;0.5;3 years;220;240;230;105;n/a;II;https://www.simes.it/en/overview/29/loft-round;A complete set of fittings available in three sizes with different light sources allowing for diverse applications.;https://www.simes.it/en/search/?q=6622;1;60;60;60;Wall mounted;MICROLOFT ROUND WALL 7°x28°;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRLOFTTONDO2.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;0.6m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_01_White;Simes_Microloft_Photometrics : S.6622W
S.6622W.14_MICROLOFT WALL_7°x28°_3000K_74lm_2.2W_Aluminium grey;S.6622W.14;0;3000;2.2;74;14 Aluminium Grey;0.5;3 years;220;240;230;105;n/a;II;https://www.simes.it/en/overview/29/loft-round;A complete set of fittings available in three sizes with different light sources allowing for diverse applications.;https://www.simes.it/en/search/?q=6622;1;60;60;60;Wall mounted;MICROLOFT ROUND WALL 7°x28°;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRLOFTTONDO2.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;0.6m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Microloft_Photometrics : S.6622W
S.6622W.24_MICROLOFT WALL_7°x28°_3000K_74lm_2.2W_Anthracite grey;S.6622W.24;0;3000;2.2;74;24 Anthracite Grey;0.5;3 years;220;240;230;105;n/a;II;https://www.simes.it/en/overview/29/loft-round;A complete set of fittings available in three sizes with different light sources allowing for diverse applications.;https://www.simes.it/en/search/?q=6622;1;60;60;60;Wall mounted;MICROLOFT ROUND WALL 7°x28°;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRLOFTTONDO2.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;0.6m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_24_Anthracyte grey;Simes_Microloft_Photometrics : S.6622W
