;SIMES_Product Code##OTHER##;SIMES_Beam Angle##ANGLE##DEGREES;SIMES_Color Temperature##COLOR_TEMPERATURE##KELVIN;SIMES_Rated Wattage##ELECTRICAL_POWER##WATTS;SIMES_Rated Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;SIMES_Finishes##OTHER##;SIMES_Weigth##MASS##KILOGRAMS;SIMES_Warranty Period##OTHER##;SIMES_Supply Voltage Min##ELECTRICAL_POTENTIAL##VOLTS;SIMES_Supply Voltage Max##ELECTRICAL_POTENTIAL##VOLTS;SIMES_Supply Voltage##ELECTRICAL_POTENTIAL##VOLTS;SIMES_Source Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;SIMES_Remote Power Supply##OTHER##;SIMES_Protection Class##OTHER##;SIMES_Product Page URL##OTHER##;SIMES_Product Description##OTHER##;SIMES_Product Data Sheet URL##OTHER##;SIMES_Number of Poles##OTHER##;SIMES_Nominal Width##LENGTH##MILLIMETERS;SIMES_Nominal Length##LENGTH##MILLIMETERS;SIMES_Nominal Height##LENGTH##MILLIMETERS;SIMES_Mounting Type##OTHER##;SIMES_Model##OTHER##;SIMES_Material Description##OTHER##;SIMES_Manufacturer Comment##OTHER##;SIMES_Luminous Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;SIMES_Light Source Type##OTHER##;SIMES_Lamp Count##OTHER##;SIMES_Installation Note URL##OTHER##;SIMES_IP Rating##OTHER##;SIMES_IK Rating##OTHER##;SIMES_Frequency##OTHER##;SIMES_Energy Efficiency Class##OTHER##;SIMES_Dimmable##OTHER##;SIMES_Current##ELECTRICAL_CURRENT##AMPERES;SIMES_Control Gear##OTHER##;SIMES_Cable Length##OTHER##;SIMES_CRI##OTHER##;SIMES_Approval Mark##OTHER##;LightFixturePlacingType##OTHER##;LightFixtureMountingType##OTHER##;Light Source##OTHER##;HasProtectiveEarth##OTHER##;Ground Stake##OTHER##;Body##OTHER##;Photometric_Type##OTHER##
S.7280H.01_COOL WALL_2700K_1545lm_15.3W_White;S.7280H.01;0;2700;15.3;1545;01 White;1.56;3 years;220;240;230;2563;n/a;I;https://www.simes.it/en/overview/104/cool-square;COOL is a simple void volume diffusing light in two directions from a very thin LED circuit right below its protective glass.;https://www.simes.it/en/search/?q=7280;1;85;220;220;Wall mounted;COOL WALL MOUNTED;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRCOOLQUAD2.pdf;IP54;IK 06;AC 50-60Hz / DC;A+;DALI 2 / PUSH;0;Electronic ballast;0.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_01_White;Simes_Cool_Photometrics : S.7280H
S.7280H.09_COOL WALL_2700K_1545lm_15.3W_Black;S.7280H.09;0;2700;15.3;1545;09 Black;1.56;3 years;220;240;230;2563;n/a;I;https://www.simes.it/en/overview/104/cool-square;COOL is a simple void volume diffusing light in two directions from a very thin LED circuit right below its protective glass.;https://www.simes.it/en/search/?q=7280;1;85;220;220;Wall mounted;COOL WALL MOUNTED;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRCOOLQUAD2.pdf;IP54;IK 06;AC 50-60Hz / DC;A+;DALI 2 / PUSH;0;Electronic ballast;0.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_09_Black;Simes_Cool_Photometrics : S.7280H
S.7280H.14_COOL WALL_2700K_1545lm_15.3W_Aluminium grey;S.7280H.14;0;2700;15.3;1545;14 Aluminium Grey;1.56;3 years;220;240;230;2563;n/a;I;https://www.simes.it/en/overview/104/cool-square;COOL is a simple void volume diffusing light in two directions from a very thin LED circuit right below its protective glass.;https://www.simes.it/en/search/?q=7280;1;85;220;220;Wall mounted;COOL WALL MOUNTED;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRCOOLQUAD2.pdf;IP54;IK 06;AC 50-60Hz / DC;A+;DALI 2 / PUSH;0;Electronic ballast;0.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Cool_Photometrics : S.7280H
S.7280N.01_COOL WALL_4000K_1626lm_15.3W_White;S.7280N.01;0;4000;15.3;1626;01 White;1.56;3 years;220;240;230;2699;n/a;I;https://www.simes.it/en/overview/104/cool-square;COOL is a simple void volume diffusing light in two directions from a very thin LED circuit right below its protective glass.;https://www.simes.it/en/search/?q=7280;1;85;220;220;Wall mounted;COOL WALL MOUNTED;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRCOOLQUAD2.pdf;IP54;IK 06;AC 50-60Hz / DC;A+;DALI 2 / PUSH;0;Electronic ballast;0.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_01_White;Simes_Cool_Photometrics : S.7280N
S.7280N.09_COOL WALL_4000K_1626lm_15.3W_Black;S.7280N.09;0;4000;15.3;1626;09 Black;1.56;3 years;220;240;230;2699;n/a;I;https://www.simes.it/en/overview/104/cool-square;COOL is a simple void volume diffusing light in two directions from a very thin LED circuit right below its protective glass.;https://www.simes.it/en/search/?q=7280;1;85;220;220;Wall mounted;COOL WALL MOUNTED;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRCOOLQUAD2.pdf;IP54;IK 06;AC 50-60Hz / DC;A+;DALI 2 / PUSH;0;Electronic ballast;0.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_09_Black;Simes_Cool_Photometrics : S.7280N
S.7280N.14_COOL WALL_4000K_1626lm_15.3W_Aluminium grey;S.7280N.14;0;4000;15.3;1626;14 Aluminium Grey;1.56;3 years;220;240;230;2699;n/a;I;https://www.simes.it/en/overview/104/cool-square;COOL is a simple void volume diffusing light in two directions from a very thin LED circuit right below its protective glass.;https://www.simes.it/en/search/?q=7280;1;85;220;220;Wall mounted;COOL WALL MOUNTED;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRCOOLQUAD2.pdf;IP54;IK 06;AC 50-60Hz / DC;A+;DALI 2 / PUSH;0;Electronic ballast;0.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Cool_Photometrics : S.7280N
S.7280W.01_COOL WALL_3000K_1590lm_15.3W_White;S.7280W.01;0;3000;15.3;1590;01 White;1.56;3 years;220;240;230;2638;n/a;I;https://www.simes.it/en/overview/104/cool-square;COOL is a simple void volume diffusing light in two directions from a very thin LED circuit right below its protective glass.;https://www.simes.it/en/search/?q=7280;1;85;220;220;Wall mounted;COOL WALL MOUNTED;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRCOOLQUAD2.pdf;IP54;IK 06;AC 50-60Hz / DC;A+;DALI 2 / PUSH;0;Electronic ballast;0.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_01_White;Simes_Cool_Photometrics : S.7280W
S.7280W.09_COOL WALL_3000K_1590lm_15.3W_Black;S.7280W.09;0;3000;15.3;1590;09 Black;1.56;3 years;220;240;230;2638;n/a;I;https://www.simes.it/en/overview/104/cool-square;COOL is a simple void volume diffusing light in two directions from a very thin LED circuit right below its protective glass.;https://www.simes.it/en/search/?q=7280;1;85;220;220;Wall mounted;COOL WALL MOUNTED;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRCOOLQUAD2.pdf;IP54;IK 06;AC 50-60Hz / DC;A+;DALI 2 / PUSH;0;Electronic ballast;0.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_09_Black;Simes_Cool_Photometrics : S.7280W
S.7280W.14_COOL WALL_3000K_1590lm_15.3W_Aluminium grey;S.7280W.14;0;3000;15.3;1590;14 Aluminium Grey;1.56;3 years;220;240;230;2638;n/a;I;https://www.simes.it/en/overview/104/cool-square;COOL is a simple void volume diffusing light in two directions from a very thin LED circuit right below its protective glass.;https://www.simes.it/en/search/?q=7280;1;85;220;220;Wall mounted;COOL WALL MOUNTED;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRCOOLQUAD2.pdf;IP54;IK 06;AC 50-60Hz / DC;A+;DALI 2 / PUSH;0;Electronic ballast;0.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Cool_Photometrics : S.7280W
