;SIMES_Product Code##OTHER##;SIMES_Beam Angle##ANGLE##DEGREES;SIMES_Color Temperature##COLOR_TEMPERATURE##KELVIN;SIMES_Rated Wattage##ELECTRICAL_POWER##WATTS;SIMES_Rated Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;SIMES_Finishes##OTHER##;SIMES_Weigth##MASS##KILOGRAMS;SIMES_Warranty Period##OTHER##;SIMES_Supply Voltage Min##ELECTRICAL_POTENTIAL##VOLTS;SIMES_Supply Voltage Max##ELECTRICAL_POTENTIAL##VOLTS;SIMES_Supply Voltage##ELECTRICAL_POTENTIAL##VOLTS;SIMES_Source Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;SIMES_Remote Power Supply##OTHER##;SIMES_Protection Class##OTHER##;SIMES_Product Page URL##OTHER##;SIMES_Product Description##OTHER##;SIMES_Product Data Sheet URL##OTHER##;SIMES_Number of Poles##OTHER##;SIMES_Nominal Width##LENGTH##MILLIMETERS;SIMES_Nominal Length##LENGTH##MILLIMETERS;SIMES_Nominal Height##LENGTH##MILLIMETERS;SIMES_Mounting Type##OTHER##;SIMES_Model##OTHER##;SIMES_Material Description##OTHER##;SIMES_Manufacturer Comment##OTHER##;SIMES_Luminous Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;SIMES_Light Source Type##OTHER##;SIMES_Lamp Count##OTHER##;SIMES_Installation Note URL##OTHER##;SIMES_IP Rating##OTHER##;SIMES_IK Rating##OTHER##;SIMES_Frequency##OTHER##;SIMES_Energy Efficiency Class##OTHER##;SIMES_Dimmable##OTHER##;SIMES_Current##ELECTRICAL_CURRENT##AMPERES;SIMES_Control Gear##OTHER##;SIMES_Cable Length##OTHER##;SIMES_CRI##OTHER##;SIMES_Approval Mark##OTHER##;LightFixturePlacingType##OTHER##;LightFixtureMountingType##OTHER##;Light Source##OTHER##;HasProtectiveEarth##OTHER##;Ground Stake##OTHER##;Body##OTHER##;Photometric_Type##OTHER##
S.1920H.14_MICRO OVER-ALL_12°_2700K_184lm_2.2W_Aluminium grey;S.1920H.14;12;2700;2.2;184;14 Aluminium Grey;0.6;3 years;0;0;0;184;need remote power supply type S.3423 230V/700mA 39W;III;https://www.simes.it/en/overview/153/over-all;Over-all is an up-light of easy and immediate application: a special nylon fixing plate isolating it from the ground, is directly fixed to the surface without any recessed in-ground device.;https://www.simes.it/en/search/?q=1920;1;120;120;27;Surface Up-light;Micro Over-all 12°;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTROVERALL.pdf;IP65/IP67;IK 09;DC 0Hz;A+;yes;0.7;n/a;5.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Micro Over-all_Photometrics : S.1920H
S.1920H.24_MICRO OVER-ALL_12°_2700K_184lm_2.2W_Anthracite grey;S.1920H.24;12;2700;2.2;184;24 Anthracite Grey;0.6;3 years;0;0;0;184;need remote power supply type S.3423 230V/700mA 39W;III;https://www.simes.it/en/overview/153/over-all;Over-all is an up-light of easy and immediate application: a special nylon fixing plate isolating it from the ground, is directly fixed to the surface without any recessed in-ground device.;https://www.simes.it/en/search/?q=1920;1;120;120;27;Surface Up-light;Micro Over-all 12°;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTROVERALL.pdf;IP65/IP67;IK 09;DC 0Hz;A+;yes;0.7;n/a;5.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_24_Anthracyte grey;Simes_Micro Over-all_Photometrics : S.1920H
S.1920N.14_MICRO OVER-ALL_12°_4000K_218lm_2.2W_Aluminium grey;S.1920N.14;12;4000;2.2;218;14 Aluminium Grey;0.6;3 years;0;0;0;218;need remote power supply type S.3423 230V/700mA 39W;III;https://www.simes.it/en/overview/153/over-all;Over-all is an up-light of easy and immediate application: a special nylon fixing plate isolating it from the ground, is directly fixed to the surface without any recessed in-ground device.;https://www.simes.it/en/search/?q=1920;1;120;120;27;Surface Up-light;Micro Over-all 12°;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTROVERALL.pdf;IP65/IP67;IK 08;DC 0Hz;A+;yes;0.7;n/a;5.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Micro Over-all_Photometrics : S.1920N
S.1920N.24_MICRO OVER-ALL_12°_4000K_218lm_2.2W_Anthracite grey;S.1920N.24;12;4000;2.2;218;24 Anthracite Grey;0.6;3 years;0;0;0;218;need remote power supply type S.3423 230V/700mA 39W;III;https://www.simes.it/en/overview/153/over-all;Over-all is an up-light of easy and immediate application: a special nylon fixing plate isolating it from the ground, is directly fixed to the surface without any recessed in-ground device.;https://www.simes.it/en/search/?q=1920;1;120;120;27;Surface Up-light;Micro Over-all 12°;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTROVERALL.pdf;IP65/IP67;IK 08;DC 0Hz;A+;yes;0.7;n/a;5.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_24_Anthracyte grey;Simes_Micro Over-all_Photometrics : S.1920N
S.1920W.14_MICRO OVER-ALL_12°_3000K_200lm_2.2W_Aluminium grey;S.1920W.14;12;3000;2.2;200;14 Aluminium Grey;0.6;3 years;0;0;0;200;need remote power supply type S.3423 230V/700mA 39W;III;https://www.simes.it/en/overview/153/over-all;Over-all is an up-light of easy and immediate application: a special nylon fixing plate isolating it from the ground, is directly fixed to the surface without any recessed in-ground device.;https://www.simes.it/en/search/?q=1920;1;120;120;27;Surface Up-light;Micro Over-all 12°;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTROVERALL.pdf;IP65/IP67;IK 09;DC 0Hz;A+;yes;0.7;n/a;5.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Micro Over-all_Photometrics : S.1920W
S.1920W.24_MICRO OVER-ALL_12°_3000K_200lm_2.2W_Anthracite grey;S.1920W.24;12;3000;2.2;200;24 Anthracite Grey;0.6;3 years;0;0;0;200;need remote power supply type S.3423 230V/700mA 39W;III;https://www.simes.it/en/overview/153/over-all;Over-all is an up-light of easy and immediate application: a special nylon fixing plate isolating it from the ground, is directly fixed to the surface without any recessed in-ground device.;https://www.simes.it/en/search/?q=1920;1;120;120;27;Surface Up-light;Micro Over-all 12°;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTROVERALL.pdf;IP65/IP67;IK 09;DC 0Hz;A+;yes;0.7;n/a;5.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_24_Anthracyte grey;Simes_Micro Over-all_Photometrics : S.1920W
S.1921H.14_MICRO OVER-ALL_32°_2700K_175lm_2.2W_Aluminium grey;S.1921H.14;32;2700;2.2;175;14 Aluminium Grey;0.6;3 years;0;0;0;175;need remote power supply type S.3423 230V/700mA 39W;III;https://www.simes.it/en/overview/153/over-all;Over-all is an up-light of easy and immediate application: a special nylon fixing plate isolating it from the ground, is directly fixed to the surface without any recessed in-ground device.;https://www.simes.it/en/search/?q=1921;1;120;120;27;Surface Up-light;Micro Over-all 32°;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTROVERALL.pdf;IP65/IP67;IK 09;DC 0Hz;A+;yes;0.7;n/a;5.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Micro Over-all_Photometrics : S.1921H
S.1921H.24_MICRO OVER-ALL_32°_2700K_175lm_2.2W_Anthracite grey;S.1921H.24;32;2700;2.2;175;24 Anthracite Grey;0.6;3 years;0;0;0;175;need remote power supply type S.3423 230V/700mA 39W;III;https://www.simes.it/en/overview/153/over-all;Over-all is an up-light of easy and immediate application: a special nylon fixing plate isolating it from the ground, is directly fixed to the surface without any recessed in-ground device.;https://www.simes.it/en/search/?q=1921;1;120;120;27;Surface Up-light;Micro Over-all 32°;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTROVERALL.pdf;IP65/IP67;IK 09;DC 0Hz;A+;yes;0.7;n/a;5.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_24_Anthracyte grey;Simes_Micro Over-all_Photometrics : S.1921H
S.1921N.14_MICRO OVER-ALL_32°_4000K_207lm_2.2W_Aluminium grey;S.1921N.14;32;4000;2.2;207;14 Aluminium Grey;0.6;3 years;0;0;0;207;need remote power supply type S.3423 230V/700mA 39W;III;https://www.simes.it/en/overview/153/over-all;Over-all is an up-light of easy and immediate application: a special nylon fixing plate isolating it from the ground, is directly fixed to the surface without any recessed in-ground device.;https://www.simes.it/en/search/?q=1921;1;120;120;27;Surface Up-light;Micro Over-all 32°;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTROVERALL.pdf;IP65/IP67;IK 08;DC 0Hz;A+;yes;0.7;n/a;5.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Micro Over-all_Photometrics : S.1921N
S.1921N.24_MICRO OVER-ALL_32°_4000K_207lm_2.2W_Anthracite grey;S.1921N.24;32;4000;2.2;207;24 Anthracite Grey;0.6;3 years;0;0;0;207;need remote power supply type S.3423 230V/700mA 39W;III;https://www.simes.it/en/overview/153/over-all;Over-all is an up-light of easy and immediate application: a special nylon fixing plate isolating it from the ground, is directly fixed to the surface without any recessed in-ground device.;https://www.simes.it/en/search/?q=1921;1;120;120;27;Surface Up-light;Micro Over-all 32°;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTROVERALL.pdf;IP65/IP67;IK 08;DC 0Hz;A+;yes;0.7;n/a;5.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_24_Anthracyte grey;Simes_Micro Over-all_Photometrics : S.1921N
S.1921W.14_MICRO OVER-ALL_32°_3000K_191lm_2.2W_Aluminium grey;S.1921W.14;32;3000;2.2;191;14 Aluminium Grey;0.6;3 years;0;0;0;191;need remote power supply type S.3423 230V/700mA 39W;III;https://www.simes.it/en/overview/153/over-all;Over-all is an up-light of easy and immediate application: a special nylon fixing plate isolating it from the ground, is directly fixed to the surface without any recessed in-ground device.;https://www.simes.it/en/search/?q=1921;1;120;120;27;Surface Up-light;Micro Over-all 32°;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTROVERALL.pdf;IP65/IP67;IK 09;DC 0Hz;A+;yes;0.7;n/a;5.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Micro Over-all_Photometrics : S.1921W
S.1921W.24_MICRO OVER-ALL_32°_3000K_191lm_2.2W_Anthracite grey;S.1921W.24;32;3000;2.2;191;24 Anthracite Grey;0.6;3 years;0;0;0;191;need remote power supply type S.3423 230V/700mA 39W;III;https://www.simes.it/en/overview/153/over-all;Over-all is an up-light of easy and immediate application: a special nylon fixing plate isolating it from the ground, is directly fixed to the surface without any recessed in-ground device.;https://www.simes.it/en/search/?q=1921;1;120;120;27;Surface Up-light;Micro Over-all 32°;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTROVERALL.pdf;IP65/IP67;IK 09;DC 0Hz;A+;yes;0.7;n/a;5.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_24_Anthracyte grey;Simes_Micro Over-all_Photometrics : S.1921W
S.1925H.14_MICRO OVER-ALL_ASY_2700K_170lm_2.2W_Aluminium grey;S.1925H.14;0;2700;2.2;170;14 Aluminium Grey;0.6;3 years;0;0;0;170;need remote power supply type S.3423 230V/700mA 39W;III;https://www.simes.it/en/overview/153/over-all;Over-all is an up-light of easy and immediate application: a special nylon fixing plate isolating it from the ground, is directly fixed to the surface without any recessed in-ground device.;https://www.simes.it/en/search/?q=1925;1;120;120;27;Surface Up-light;Micro Over-all ASY;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTROVERALL.pdf;IP65/IP67;IK 09;DC 0Hz;A+;yes;0.7;n/a;5.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Micro Over-all_Photometrics : S.1925H
S.1925H.24_MICRO OVER-ALL_ASY_2700K_170lm_2.2W_Anthracite grey;S.1925H.24;0;2700;2.2;170;24 Anthracite Grey;0.6;3 years;0;0;0;170;need remote power supply type S.3423 230V/700mA 39W;III;https://www.simes.it/en/overview/153/over-all;Over-all is an up-light of easy and immediate application: a special nylon fixing plate isolating it from the ground, is directly fixed to the surface without any recessed in-ground device.;https://www.simes.it/en/search/?q=1925;1;120;120;27;Surface Up-light;Micro Over-all ASY;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTROVERALL.pdf;IP65/IP67;IK 09;DC 0Hz;A+;yes;0.7;n/a;5.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_24_Anthracyte grey;Simes_Micro Over-all_Photometrics : S.1925H
S.1925N.14_MICRO OVER-ALL_ASY_4000K_200lm_2.2W_Aluminium grey;S.1925N.14;0;4000;2.2;200;14 Aluminium Grey;0.6;3 years;0;0;0;200;need remote power supply type S.3423 230V/700mA 39W;III;https://www.simes.it/en/overview/153/over-all;Over-all is an up-light of easy and immediate application: a special nylon fixing plate isolating it from the ground, is directly fixed to the surface without any recessed in-ground device.;https://www.simes.it/en/search/?q=1925;1;120;120;27;Surface Up-light;Micro Over-all ASY;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTROVERALL.pdf;IP65/IP67;IK 08;DC 0Hz;A+;yes;0.7;n/a;5.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Micro Over-all_Photometrics : S.1925N
S.1925N.24_MICRO OVER-ALL_ASY_4000K_200lm_2.2W_Anthracite grey;S.1925N.24;0;4000;2.2;200;24 Anthracite Grey;0.6;3 years;0;0;0;200;need remote power supply type S.3423 230V/700mA 39W;III;https://www.simes.it/en/overview/153/over-all;Over-all is an up-light of easy and immediate application: a special nylon fixing plate isolating it from the ground, is directly fixed to the surface without any recessed in-ground device.;https://www.simes.it/en/search/?q=1925;1;120;120;27;Surface Up-light;Micro Over-all ASY;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTROVERALL.pdf;IP65/IP67;IK 08;DC 0Hz;A+;yes;0.7;n/a;5.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_24_Anthracyte grey;Simes_Micro Over-all_Photometrics : S.1925N
S.1925W.14_MICRO OVER-ALL_ASY_3000K_185lm_2.2W_Aluminium grey;S.1925W.14;0;3000;2.2;185;14 Aluminium Grey;0.6;3 years;0;0;0;185;need remote power supply type S.3423 230V/700mA 39W;III;https://www.simes.it/en/overview/153/over-all;Over-all is an up-light of easy and immediate application: a special nylon fixing plate isolating it from the ground, is directly fixed to the surface without any recessed in-ground device.;https://www.simes.it/en/search/?q=1925;1;120;120;27;Surface Up-light;Micro Over-all ASY;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTROVERALL.pdf;IP65/IP67;IK 09;DC 0Hz;A+;yes;0.7;n/a;5.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Micro Over-all_Photometrics : S.1925W
S.1925W.24_MICRO OVER-ALL_ASY_3000K_185lm_2.2W_Anthracite grey;S.1925W.24;0;3000;2.2;185;24 Anthracite Grey;0.6;3 years;0;0;0;185;need remote power supply type S.3423 230V/700mA 39W;III;https://www.simes.it/en/overview/153/over-all;Over-all is an up-light of easy and immediate application: a special nylon fixing plate isolating it from the ground, is directly fixed to the surface without any recessed in-ground device.;https://www.simes.it/en/search/?q=1925;1;120;120;27;Surface Up-light;Micro Over-all ASY;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTROVERALL.pdf;IP65/IP67;IK 09;DC 0Hz;A+;yes;0.7;n/a;5.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_24_Anthracyte grey;Simes_Micro Over-all_Photometrics : S.1925W
