;SIMES_Product Code##OTHER##;SIMES_Beam Angle##ANGLE##DEGREES;SIMES_Color Temperature##COLOR_TEMPERATURE##KELVIN;SIMES_Rated Wattage##ELECTRICAL_POWER##WATTS;SIMES_Rated Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;SIMES_Finishes##OTHER##;SIMES_Weigth##MASS##KILOGRAMS;SIMES_Warranty Period##OTHER##;SIMES_Supply Voltage Min##ELECTRICAL_POTENTIAL##VOLTS;SIMES_Supply Voltage Max##ELECTRICAL_POTENTIAL##VOLTS;SIMES_Supply Voltage##ELECTRICAL_POTENTIAL##VOLTS;SIMES_Source Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;SIMES_Remote Power Supply##OTHER##;SIMES_Protection Class##OTHER##;SIMES_Product Page URL##OTHER##;SIMES_Product Description##OTHER##;SIMES_Product Data Sheet URL##OTHER##;SIMES_Number of Poles##OTHER##;SIMES_Nominal Width##LENGTH##MILLIMETERS;SIMES_Nominal Length##LENGTH##MILLIMETERS;SIMES_Nominal Height##LENGTH##MILLIMETERS;SIMES_Mounting Type##OTHER##;SIMES_Model##OTHER##;SIMES_Material Description##OTHER##;SIMES_Manufacturer Comment##OTHER##;SIMES_Luminous Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;SIMES_Light Source Type##OTHER##;SIMES_Lamp Count##OTHER##;SIMES_Installation Note URL##OTHER##;SIMES_IP Rating##OTHER##;SIMES_IK Rating##OTHER##;SIMES_Frequency##OTHER##;SIMES_Energy Efficiency Class##OTHER##;SIMES_Dimmable##OTHER##;SIMES_Current##ELECTRICAL_CURRENT##AMPERES;SIMES_Control Gear##OTHER##;SIMES_Cable Length##OTHER##;SIMES_CRI##OTHER##;SIMES_Approval Mark##OTHER##;LightFixturePlacingType##OTHER##;LightFixtureMountingType##OTHER##;Light Source##OTHER##;HasProtectiveEarth##OTHER##;Ground Stake##OTHER##;Body##OTHER##;Photometric_Type##OTHER##;SIMES_AltezzaTraf##LENGTH##MILLIMETERS
S.7265H.01_LOOK_2700K_1725lm_21,6W_H290_White;S.7265H.01;0;2700;21.6;1725;01 White;1.5;3 years;220;240;230;3534;n/a;II;https://www.simes.it/en/overview/93/look-bollard;LOOK has an elegant rectangular body, minimal and compact, mounted on wall or on its bollard. The light is directed on one side through a glass window.;https://www.simes.it/en/search/?q=7265;1;130;290;290;Ground;LOOK BOLLARD H290;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRLOOKPAL.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;DALI2 / PUSH;0;Electronic ballast;0.4m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_01_White;Simes_Look_Bollard_Photometrics : S.7260H;247
S.7265H.14_LOOK_2700K_1725lm_21,6W_H290_Aluminium grey;S.7265H.14;0;2700;21.6;1725;14 Aluminium Grey;1.5;3 years;220;240;230;3534;n/a;II;https://www.simes.it/en/overview/93/look-bollard;LOOK has an elegant rectangular body, minimal and compact, mounted on wall or on its bollard. The light is directed on one side through a glass window.;https://www.simes.it/en/search/?q=7265;1;130;290;290;Ground;LOOK BOLLARD H290;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRLOOKPAL.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;DALI2 / PUSH;0;Electronic ballast;0.4m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Look_Bollard_Photometrics : S.7260H;247
S.7265H.20_LOOK_2700K_1725lm_21,6W_H290_Burnished bronze;S.7265H.20;0;2700;21.6;1725;20 Burnished bronze;1.5;3 years;220;240;230;3534;n/a;II;https://www.simes.it/en/overview/93/look-bollard;LOOK has an elegant rectangular body, minimal and compact, mounted on wall or on its bollard. The light is directed on one side through a glass window.;https://www.simes.it/en/search/?q=7265;1;130;290;290;Ground;LOOK BOLLARD H290;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRLOOKPAL.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;DALI2 / PUSH;0;Electronic ballast;0.4m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_20_Burnished bronze;Simes_Look_Bollard_Photometrics : S.7260H;247
S.7265H.24_LOOK_2700K_1725lm_21,6W_H290_Anthracite grey;S.7265H.24;0;2700;21.6;1725;24 Anthracite Grey;1.5;3 years;220;240;230;3534;n/a;II;https://www.simes.it/en/overview/93/look-bollard;LOOK has an elegant rectangular body, minimal and compact, mounted on wall or on its bollard. The light is directed on one side through a glass window.;https://www.simes.it/en/search/?q=7265;1;130;290;290;Ground;LOOK BOLLARD H290;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRLOOKPAL.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;DALI2 / PUSH;0;Electronic ballast;0.4m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_24_Anthracyte grey;Simes_Look_Bollard_Photometrics : S.7260H;247
S.7265W.01_LOOK_3000K_1774lm_21,6W_H290_White;S.7265W.01;0;3000;21.6;1774;01 White;1.5;3 years;220;240;230;3720;n/a;II;https://www.simes.it/en/overview/93/look-bollard;LOOK has an elegant rectangular body, minimal and compact, mounted on wall or on its bollard. The light is directed on one side through a glass window.;https://www.simes.it/en/search/?q=7265;1;130;290;290;Ground;LOOK BOLLARD H290;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRLOOKPAL.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;DALI2 / PUSH;0;Electronic ballast;0.4m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_01_White;Simes_Look_Bollard_Photometrics : S.7260W;247
S.7265W.14_LOOK_3000K_1774lm_21,6W_H290_Aluminium grey;S.7265W.14;0;3000;21.6;1774;14 Aluminium Grey;1.5;3 years;220;240;230;3720;n/a;II;https://www.simes.it/en/overview/93/look-bollard;LOOK has an elegant rectangular body, minimal and compact, mounted on wall or on its bollard. The light is directed on one side through a glass window.;https://www.simes.it/en/search/?q=7265;1;130;290;290;Ground;LOOK BOLLARD H290;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRLOOKPAL.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;DALI2 / PUSH;0;Electronic ballast;0.4m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Look_Bollard_Photometrics : S.7260W;247
S.7265W.20_LOOK_3000K_1774lm_21,6W_H290_Burnished bronze;S.7265W.20;0;3000;21.6;1774;20 Burnished bronze;1.5;3 years;220;240;230;3720;n/a;II;https://www.simes.it/en/overview/93/look-bollard;LOOK has an elegant rectangular body, minimal and compact, mounted on wall or on its bollard. The light is directed on one side through a glass window.;https://www.simes.it/en/search/?q=7265;1;130;290;290;Ground;LOOK BOLLARD H290;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRLOOKPAL.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;DALI2 / PUSH;0;Electronic ballast;0.4m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_20_Burnished bronze;Simes_Look_Bollard_Photometrics : S.7260W;247
S.7265W.24_LOOK_3000K_1774lm_21,6W_H290_Anthracite grey;S.7265W.24;0;3000;21.6;1774;24 Anthracite Grey;1.5;3 years;220;240;230;3720;n/a;II;https://www.simes.it/en/overview/93/look-bollard;LOOK has an elegant rectangular body, minimal and compact, mounted on wall or on its bollard. The light is directed on one side through a glass window.;https://www.simes.it/en/search/?q=7265;1;130;290;290;Ground;LOOK BOLLARD H290;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRLOOKPAL.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;DALI2 / PUSH;0;Electronic ballast;0.4m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_24_Anthracyte grey;Simes_Look_Bollard_Photometrics : S.7260W;247
S.7265N.01_LOOK_4000K_1813lm_21,6W_H290_White;S.7265N.01;0;4000;21.6;1813;01 White;1.5;3 years;220;240;230;4018;n/a;II;https://www.simes.it/en/overview/93/look-bollard;LOOK has an elegant rectangular body, minimal and compact, mounted on wall or on its bollard. The light is directed on one side through a glass window.;https://www.simes.it/en/search/?q=7265;1;130;290;290;Ground;LOOK BOLLARD H290;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRLOOKPAL.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;DALI2 / PUSH;0;Electronic ballast;0.4m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_01_White;Simes_Look_Bollard_Photometrics : S.7260N;247
S.7265N.14_LOOK_4000K_1813lm_21,6W_H290_Aluminium grey;S.7265N.14;0;4000;21.6;1813;14 Aluminium Grey;1.5;3 years;220;240;230;4018;n/a;II;https://www.simes.it/en/overview/93/look-bollard;LOOK has an elegant rectangular body, minimal and compact, mounted on wall or on its bollard. The light is directed on one side through a glass window.;https://www.simes.it/en/search/?q=7265;1;130;290;290;Ground;LOOK BOLLARD H290;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRLOOKPAL.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;DALI2 / PUSH;0;Electronic ballast;0.4m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Look_Bollard_Photometrics : S.7260N;247
S.7265N.20_LOOK_4000K_1813lm_21,6W_H290_Burnished bronze;S.7265N.20;0;4000;21.6;1813;20 Burnished bronze;1.5;3 years;220;240;230;4018;n/a;II;https://www.simes.it/en/overview/93/look-bollard;LOOK has an elegant rectangular body, minimal and compact, mounted on wall or on its bollard. The light is directed on one side through a glass window.;https://www.simes.it/en/search/?q=7265;1;130;290;290;Ground;LOOK BOLLARD H290;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRLOOKPAL.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;DALI2 / PUSH;0;Electronic ballast;0.4m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_20_Burnished bronze;Simes_Look_Bollard_Photometrics : S.7260N;247
S.7265N.24_LOOK_4000K_1813lm_21,6W_H290_Anthracite grey;S.7265N.24;0;4000;21.6;1813;24 Anthracite Grey;1.5;3 years;220;240;230;4018;n/a;II;https://www.simes.it/en/overview/93/look-bollard;LOOK has an elegant rectangular body, minimal and compact, mounted on wall or on its bollard. The light is directed on one side through a glass window.;https://www.simes.it/en/search/?q=7265;1;130;290;290;Ground;LOOK BOLLARD H290;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRLOOKPAL.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;DALI2 / PUSH;0;Electronic ballast;0.4m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_24_Anthracyte grey;Simes_Look_Bollard_Photometrics : S.7260N;247
S.7266H.01_LOOK_2700K_1725lm_21,6W_H580_White;S.7266H.01;0;2700;21.6;1725;01 White;3.6;3 years;220;240;230;3534;n/a;II;https://www.simes.it/en/overview/93/look-bollard;LOOK has an elegant rectangular body, minimal and compact, mounted on wall or on its bollard. The light is directed on one side through a glass window.;https://www.simes.it/en/search/?q=7266;1;130;290;580;Ground;LOOK BOLLARD H580;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRLOOKPAL.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;DALI2 / PUSH;0;Electronic ballast;0.4m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_01_White;Simes_Look_Bollard_Photometrics : S.7260H;537
S.7266H.14_LOOK_2700K_1725lm_21,6W_H580_Aluminium grey;S.7266H.14;0;2700;21.6;1725;14 Aluminium Grey;3.6;3 years;220;240;230;3534;n/a;II;https://www.simes.it/en/overview/93/look-bollard;LOOK has an elegant rectangular body, minimal and compact, mounted on wall or on its bollard. The light is directed on one side through a glass window.;https://www.simes.it/en/search/?q=7266;1;130;290;580;Ground;LOOK BOLLARD H580;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRLOOKPAL.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;DALI2 / PUSH;0;Electronic ballast;0.4m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Look_Bollard_Photometrics : S.7260H;537
S.7266H.20_LOOK_2700K_1725lm_21,6W_H580_Burnished bronze;S.7266H.20;0;2700;21.6;1725;20 Burnished bronze;3.6;3 years;220;240;230;3534;n/a;II;https://www.simes.it/en/overview/93/look-bollard;LOOK has an elegant rectangular body, minimal and compact, mounted on wall or on its bollard. The light is directed on one side through a glass window.;https://www.simes.it/en/search/?q=7266;1;130;290;580;Ground;LOOK BOLLARD H580;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRLOOKPAL.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;DALI2 / PUSH;0;Electronic ballast;0.4m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_20_Burnished bronze;Simes_Look_Bollard_Photometrics : S.7260H;537
S.7266H.24_LOOK_2700K_1725lm_21,6W_H580_Anthracite grey;S.7266H.24;0;2700;21.6;1725;24 Anthracite Grey;3.6;3 years;220;240;230;3534;n/a;II;https://www.simes.it/en/overview/93/look-bollard;LOOK has an elegant rectangular body, minimal and compact, mounted on wall or on its bollard. The light is directed on one side through a glass window.;https://www.simes.it/en/search/?q=7266;1;130;290;580;Ground;LOOK BOLLARD H580;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRLOOKPAL.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;DALI2 / PUSH;0;Electronic ballast;0.4m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_24_Anthracyte grey;Simes_Look_Bollard_Photometrics : S.7260H;537
S.7266W.01_LOOK_3000K_1774lm_21,6W_H580_White;S.7266W.01;0;3000;21.6;1774;01 White;3.6;3 years;220;240;230;3720;n/a;II;https://www.simes.it/en/overview/93/look-bollard;LOOK has an elegant rectangular body, minimal and compact, mounted on wall or on its bollard. The light is directed on one side through a glass window.;https://www.simes.it/en/search/?q=7266;1;130;290;580;Ground;LOOK BOLLARD H580;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRLOOKPAL.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;DALI2 / PUSH;0;Electronic ballast;0.4m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_01_White;Simes_Look_Bollard_Photometrics : S.7260W;537
S.7266W.14_LOOK_3000K_1774lm_21,6W_H580_Aluminium grey;S.7266W.14;0;3000;21.6;1774;14 Aluminium Grey;3.6;3 years;220;240;230;3720;n/a;II;https://www.simes.it/en/overview/93/look-bollard;LOOK has an elegant rectangular body, minimal and compact, mounted on wall or on its bollard. The light is directed on one side through a glass window.;https://www.simes.it/en/search/?q=7266;1;130;290;580;Ground;LOOK BOLLARD H580;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRLOOKPAL.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;DALI2 / PUSH;0;Electronic ballast;0.4m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Look_Bollard_Photometrics : S.7260W;537
S.7266W.20_LOOK_3000K_1774lm_21,6W_H580_Burnished bronze;S.7266W.20;0;3000;21.6;1774;20 Burnished bronze;3.6;3 years;220;240;230;3720;n/a;II;https://www.simes.it/en/overview/93/look-bollard;LOOK has an elegant rectangular body, minimal and compact, mounted on wall or on its bollard. The light is directed on one side through a glass window.;https://www.simes.it/en/search/?q=7266;1;130;290;580;Ground;LOOK BOLLARD H580;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRLOOKPAL.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;DALI2 / PUSH;0;Electronic ballast;0.4m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_20_Burnished bronze;Simes_Look_Bollard_Photometrics : S.7260W;537
S.7266W.24_LOOK_3000K_1774lm_21,6W_H580_Anthracite grey;S.7266W.24;0;3000;21.6;1774;24 Anthracite Grey;3.6;3 years;220;240;230;3720;n/a;II;https://www.simes.it/en/overview/93/look-bollard;LOOK has an elegant rectangular body, minimal and compact, mounted on wall or on its bollard. The light is directed on one side through a glass window.;https://www.simes.it/en/search/?q=7266;1;130;290;580;Ground;LOOK BOLLARD H580;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRLOOKPAL.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;DALI2 / PUSH;0;Electronic ballast;0.4m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_24_Anthracyte grey;Simes_Look_Bollard_Photometrics : S.7260W;537
S.7266N.01_LOOK_4000K_1813lm_21,6W_H580_White;S.7266N.01;0;4000;21.6;1813;01 White;3.6;3 years;220;240;230;4018;n/a;II;https://www.simes.it/en/overview/93/look-bollard;LOOK has an elegant rectangular body, minimal and compact, mounted on wall or on its bollard. The light is directed on one side through a glass window.;https://www.simes.it/en/search/?q=7266;1;130;290;580;Ground;LOOK BOLLARD H580;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRLOOKPAL.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;DALI2 / PUSH;0;Electronic ballast;0.4m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_01_White;Simes_Look_Bollard_Photometrics : S.7260N;537
S.7266N.14_LOOK_4000K_1813lm_21,6W_H580_Aluminium grey;S.7266N.14;0;4000;21.6;1813;14 Aluminium Grey;3.6;3 years;220;240;230;4018;n/a;II;https://www.simes.it/en/overview/93/look-bollard;LOOK has an elegant rectangular body, minimal and compact, mounted on wall or on its bollard. The light is directed on one side through a glass window.;https://www.simes.it/en/search/?q=7266;1;130;290;580;Ground;LOOK BOLLARD H580;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRLOOKPAL.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;DALI2 / PUSH;0;Electronic ballast;0.4m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Look_Bollard_Photometrics : S.7260N;537
S.7266N.20_LOOK_4000K_1813lm_21,6W_H580_Burnished bronze;S.7266N.20;0;4000;21.6;1813;20 Burnished bronze;3.6;3 years;220;240;230;4018;n/a;II;https://www.simes.it/en/overview/93/look-bollard;LOOK has an elegant rectangular body, minimal and compact, mounted on wall or on its bollard. The light is directed on one side through a glass window.;https://www.simes.it/en/search/?q=7266;1;130;290;580;Ground;LOOK BOLLARD H580;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRLOOKPAL.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;DALI2 / PUSH;0;Electronic ballast;0.4m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_20_Burnished bronze;Simes_Look_Bollard_Photometrics : S.7260N;537
S.7266N.24_LOOK_4000K_1813lm_21,6W_H580_Anthracite grey;S.7266N.24;0;4000;21.6;1813;24 Anthracite Grey;3.6;3 years;220;240;230;4018;n/a;II;https://www.simes.it/en/overview/93/look-bollard;LOOK has an elegant rectangular body, minimal and compact, mounted on wall or on its bollard. The light is directed on one side through a glass window.;https://www.simes.it/en/search/?q=7266;1;130;290;580;Ground;LOOK BOLLARD H580;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRLOOKPAL.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;DALI2 / PUSH;0;Electronic ballast;0.4m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_24_Anthracyte grey;Simes_Look_Bollard_Photometrics : S.7260N;537
S.7267H.01_LOOK_2700K_1725lm_21,6W_H870_White;S.7267H.01;0;2700;21.6;1725;01 White;4.5;3 years;220;240;230;3534;n/a;II;https://www.simes.it/en/overview/93/look-bollard;LOOK has an elegant rectangular body, minimal and compact, mounted on wall or on its bollard. The light is directed on one side through a glass window.;https://www.simes.it/en/search/?q=7267;1;130;290;870;Ground;LOOK BOLLARD H870;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRLOOKPAL.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;DALI2 / PUSH;0;Electronic ballast;0.4m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_01_White;Simes_Look_Bollard_Photometrics : S.7260H;827
S.7267H.14_LOOK_2700K_1725lm_21,6W_H870_Aluminium grey;S.7267H.14;0;2700;21.6;1725;14 Aluminium Grey;4.5;3 years;220;240;230;3534;n/a;II;https://www.simes.it/en/overview/93/look-bollard;LOOK has an elegant rectangular body, minimal and compact, mounted on wall or on its bollard. The light is directed on one side through a glass window.;https://www.simes.it/en/search/?q=7267;1;130;290;870;Ground;LOOK BOLLARD H870;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRLOOKPAL.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;DALI2 / PUSH;0;Electronic ballast;0.4m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Look_Bollard_Photometrics : S.7260H;827
S.7267H.20_LOOK_2700K_1725lm_21,6W_H870_Burnished bronze;S.7267H.20;0;2700;21.6;1725;20 Burnished bronze;4.5;3 years;220;240;230;3534;n/a;II;https://www.simes.it/en/overview/93/look-bollard;LOOK has an elegant rectangular body, minimal and compact, mounted on wall or on its bollard. The light is directed on one side through a glass window.;https://www.simes.it/en/search/?q=7267;1;130;290;870;Ground;LOOK BOLLARD H870;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRLOOKPAL.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;DALI2 / PUSH;0;Electronic ballast;0.4m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_20_Burnished bronze;Simes_Look_Bollard_Photometrics : S.7260H;827
S.7267H.24_LOOK_2700K_1725lm_21,6W_H870_Anthracite grey;S.7267H.24;0;2700;21.6;1725;24 Anthracite Grey;4.5;3 years;220;240;230;3534;n/a;II;https://www.simes.it/en/overview/93/look-bollard;LOOK has an elegant rectangular body, minimal and compact, mounted on wall or on its bollard. The light is directed on one side through a glass window.;https://www.simes.it/en/search/?q=7267;1;130;290;870;Ground;LOOK BOLLARD H870;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRLOOKPAL.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;DALI2 / PUSH;0;Electronic ballast;0.4m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_24_Anthracyte grey;Simes_Look_Bollard_Photometrics : S.7260H;827
S.7267W.01_LOOK_3000K_1774lm_21,6W_H870_White;S.7267W.01;0;3000;21.6;1774;01 White;4.5;3 years;220;240;230;3720;n/a;II;https://www.simes.it/en/overview/93/look-bollard;LOOK has an elegant rectangular body, minimal and compact, mounted on wall or on its bollard. The light is directed on one side through a glass window.;https://www.simes.it/en/search/?q=7267;1;130;290;870;Ground;LOOK BOLLARD H870;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRLOOKPAL.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;DALI2 / PUSH;0;Electronic ballast;0.4m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_01_White;Simes_Look_Bollard_Photometrics : S.7260W;827
S.7267W.14_LOOK_3000K_1774lm_21,6W_H870_Aluminium grey;S.7267W.14;0;3000;21.6;1774;14 Aluminium Grey;4.5;3 years;220;240;230;3720;n/a;II;https://www.simes.it/en/overview/93/look-bollard;LOOK has an elegant rectangular body, minimal and compact, mounted on wall or on its bollard. The light is directed on one side through a glass window.;https://www.simes.it/en/search/?q=7267;1;130;290;870;Ground;LOOK BOLLARD H870;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRLOOKPAL.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;DALI2 / PUSH;0;Electronic ballast;0.4m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Look_Bollard_Photometrics : S.7260W;827
S.7267W.20_LOOK_3000K_1774lm_21,6W_H870_Burnished bronze;S.7267W.20;0;3000;21.6;1774;20 Burnished bronze;4.5;3 years;220;240;230;3720;n/a;II;https://www.simes.it/en/overview/93/look-bollard;LOOK has an elegant rectangular body, minimal and compact, mounted on wall or on its bollard. The light is directed on one side through a glass window.;https://www.simes.it/en/search/?q=7267;1;130;290;870;Ground;LOOK BOLLARD H870;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRLOOKPAL.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;DALI2 / PUSH;0;Electronic ballast;0.4m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_20_Burnished bronze;Simes_Look_Bollard_Photometrics : S.7260W;827
S.7267W.24_LOOK_3000K_1774lm_21,6W_H870_Anthracite grey;S.7267W.24;0;3000;21.6;1774;24 Anthracite Grey;4.5;3 years;220;240;230;3720;n/a;II;https://www.simes.it/en/overview/93/look-bollard;LOOK has an elegant rectangular body, minimal and compact, mounted on wall or on its bollard. The light is directed on one side through a glass window.;https://www.simes.it/en/search/?q=7267;1;130;290;870;Ground;LOOK BOLLARD H870;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRLOOKPAL.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;DALI2 / PUSH;0;Electronic ballast;0.4m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_24_Anthracyte grey;Simes_Look_Bollard_Photometrics : S.7260W;827
S.7267N.01_LOOK_4000K_1813lm_21,6W_H870_White;S.7267N.01;0;4000;21.6;1813;01 White;4.5;3 years;220;240;230;4018;n/a;II;https://www.simes.it/en/overview/93/look-bollard;LOOK has an elegant rectangular body, minimal and compact, mounted on wall or on its bollard. The light is directed on one side through a glass window.;https://www.simes.it/en/search/?q=7267;1;130;290;870;Ground;LOOK BOLLARD H870;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRLOOKPAL.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;DALI2 / PUSH;0;Electronic ballast;0.4m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_01_White;Simes_Look_Bollard_Photometrics : S.7260N;827
S.7267N.14_LOOK_4000K_1813lm_21,6W_H870_Aluminium grey;S.7267N.14;0;4000;21.6;1813;14 Aluminium Grey;4.5;3 years;220;240;230;4018;n/a;II;https://www.simes.it/en/overview/93/look-bollard;LOOK has an elegant rectangular body, minimal and compact, mounted on wall or on its bollard. The light is directed on one side through a glass window.;https://www.simes.it/en/search/?q=7267;1;130;290;870;Ground;LOOK BOLLARD H870;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRLOOKPAL.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;DALI2 / PUSH;0;Electronic ballast;0.4m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Look_Bollard_Photometrics : S.7260N;827
S.7267N.20_LOOK_4000K_1813lm_21,6W_H870_Burnished bronze;S.7267N.20;0;4000;21.6;1813;20 Burnished bronze;4.5;3 years;220;240;230;4018;n/a;II;https://www.simes.it/en/overview/93/look-bollard;LOOK has an elegant rectangular body, minimal and compact, mounted on wall or on its bollard. The light is directed on one side through a glass window.;https://www.simes.it/en/search/?q=7267;1;130;290;870;Ground;LOOK BOLLARD H870;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRLOOKPAL.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;DALI2 / PUSH;0;Electronic ballast;0.4m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_20_Burnished bronze;Simes_Look_Bollard_Photometrics : S.7260N;827
S.7267N.24_LOOK_4000K_1813lm_21,6W_H870_Anthracite grey;S.7267N.24;0;4000;21.6;1813;24 Anthracite Grey;4.5;3 years;220;240;230;4018;n/a;II;https://www.simes.it/en/overview/93/look-bollard;LOOK has an elegant rectangular body, minimal and compact, mounted on wall or on its bollard. The light is directed on one side through a glass window.;https://www.simes.it/en/search/?q=7267;1;130;290;870;Ground;LOOK BOLLARD H870;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRLOOKPAL.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;DALI2 / PUSH;0;Electronic ballast;0.4m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_24_Anthracyte grey;Simes_Look_Bollard_Photometrics : S.7260N;827
