;SIMES_Product Code##OTHER##;SIMES_Beam Angle##ANGLE##DEGREES;SIMES_Color Temperature##COLOR_TEMPERATURE##KELVIN;SIMES_Rated Wattage##ELECTRICAL_POWER##WATTS;SIMES_Rated Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;SIMES_Finishes##OTHER##;SIMES_Weigth##MASS##KILOGRAMS;SIMES_Warranty Period##OTHER##;SIMES_Supply Voltage Min##ELECTRICAL_POTENTIAL##VOLTS;SIMES_Supply Voltage Max##ELECTRICAL_POTENTIAL##VOLTS;SIMES_Supply Voltage##ELECTRICAL_POTENTIAL##VOLTS;SIMES_Source Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;SIMES_Remote Power Supply##OTHER##;SIMES_Protection Class##OTHER##;SIMES_Product Page URL##OTHER##;SIMES_Product Description##OTHER##;SIMES_Product Data Sheet URL##OTHER##;SIMES_Number of Poles##OTHER##;SIMES_Nominal Width##LENGTH##MILLIMETERS;SIMES_Nominal Length##LENGTH##MILLIMETERS;SIMES_Nominal Height##LENGTH##MILLIMETERS;SIMES_Mounting Type##OTHER##;SIMES_Model##OTHER##;SIMES_Material Description##OTHER##;SIMES_Manufacturer Comment##OTHER##;SIMES_Luminous Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;SIMES_Light Source Type##OTHER##;SIMES_Lamp Count##OTHER##;SIMES_Installation Note URL##OTHER##;SIMES_IP Rating##OTHER##;SIMES_IK Rating##OTHER##;SIMES_Frequency##OTHER##;SIMES_Energy Efficiency Class##OTHER##;SIMES_Dimmable##OTHER##;SIMES_Current##ELECTRICAL_CURRENT##AMPERES;SIMES_Control Gear##OTHER##;SIMES_Cable Length##OTHER##;SIMES_CRI##OTHER##;SIMES_Approval Mark##OTHER##;LightFixturePlacingType##OTHER##;LightFixtureMountingType##OTHER##;Light Source##OTHER##;HasProtectiveEarth##OTHER##;Ground Stake##OTHER##;Body##OTHER##;Photometric_Type##OTHER##
C.8034H_LINEAR GHOST _L240_2700K_253lm_4W;C.8034H;0;2700;4;253;;1.85;3 years;220;240;230;363;n/a;II;https://www.simes.it/en/overview/127/ghost-for-cast-concrete;Ghost for cast concrete is a luminous void created through a specific recessed housing fixed to the shutters before casting.;https://www.simes.it/en/search/?q=8034;1;90;240;88;Wall recessed;LINEAR GHOST L240 WALL RECESSED;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRGHOST-LINEA2.pdf;IP65;IK 08;AC 50/60Hz;A+;n/a;0;Electronic ballast;6.0m;CRI80;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Ghost_Photometrics : C.8034H
C.8034N_LINEAR GHOST _L240_4000K_287lm_4W;C.8034N;0;4000;4;287;;1.85;3 years;220;240;230;412;n/a;II;https://www.simes.it/en/overview/127/ghost-for-cast-concrete;Ghost for cast concrete is a luminous void created through a specific recessed housing fixed to the shutters before casting.;https://www.simes.it/en/search/?q=8034;1;90;240;88;Wall recessed;LINEAR GHOST L240 WALL RECESSED;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRGHOST-LINEA2.pdf;IP65;IK 08;AC 50/60Hz;A+;n/a;0;Electronic ballast;6.0m;CRI80;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Ghost_Photometrics : C.8034N
C.8034W_LINEAR GHOST _L240_3000K_266lm_4W;C.8034W;0;3000;4;266;;1.85;3 years;220;240;230;382;n/a;II;https://www.simes.it/en/overview/127/ghost-for-cast-concrete;Ghost for cast concrete is a luminous void created through a specific recessed housing fixed to the shutters before casting.;https://www.simes.it/en/search/?q=8034;1;90;240;88;Wall recessed;LINEAR GHOST L240 WALL RECESSED;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRGHOST-LINEA2.pdf;IP65;IK 08;AC 50/60Hz;A+;n/a;0;Electronic ballast;6.0m;CRI80;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Ghost_Photometrics : C.8034W
C.8036H_LINEAR GHOST _L430_2700K_505lm_7.5W;C.8036H;0;2700;7.5;505;;2.52;3 years;220;240;230;726;n/a;II;https://www.simes.it/en/overview/127/ghost-for-cast-concrete;Ghost for cast concrete is a luminous void created through a specific recessed housing fixed to the shutters before casting.;https://www.simes.it/en/search/?q=8036;1;90;340;88;Wall recessed;LINEAR GHOST L430 WALL RECESSED;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRGHOST-LINEA2.pdf;IP65;IK 08;AC 50/60Hz;A+;n/a;0;Electronic ballast;6.0m;CRI80;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Ghost_Photometrics : C.8036H
C.8036N_LINEAR GHOST _L430_4000K_555lm_7.5W;C.8036N;0;4000;7.5;555;;2.52;3 years;220;240;230;825;n/a;II;https://www.simes.it/en/overview/127/ghost-for-cast-concrete;Ghost for cast concrete is a luminous void created through a specific recessed housing fixed to the shutters before casting.;https://www.simes.it/en/search/?q=8036;1;90;340;88;Wall recessed;LINEAR GHOST L430 WALL RECESSED;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRGHOST-LINEA2.pdf;IP65;IK 08;AC 50/60Hz;A+;n/a;0;Electronic ballast;6.0m;CRI80;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Ghost_Photometrics : C.8036N
C.8036W_LINEAR GHOST _L430_3000K_532lm_7.5W;C.8036W;0;3000;7.5;532;;2.52;3 years;220;240;230;764;n/a;II;https://www.simes.it/en/overview/127/ghost-for-cast-concrete;Ghost for cast concrete is a luminous void created through a specific recessed housing fixed to the shutters before casting.;https://www.simes.it/en/search/?q=8036;1;90;340;88;Wall recessed;LINEAR GHOST L430 WALL RECESSED;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRGHOST-LINEA2.pdf;IP65;IK 08;AC 50/60Hz;A+;n/a;0;Electronic ballast;6.0m;CRI80;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Ghost_Photometrics : C.8036W
C.8038H_LINEAR GHOST _L810_2700K_992lm_14W;C.8038H;0;2700;14;992;;4.26;3 years;220;240;230;1451;n/a;II;https://www.simes.it/en/overview/127/ghost-for-cast-concrete;Ghost for cast concrete is a luminous void created through a specific recessed housing fixed to the shutters before casting.;https://www.simes.it/en/search/?q=8038;1;90;810;88;Wall recessed;LINEAR GHOST L810 WALL RECESSED;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRGHOST-LINEA2.pdf;IP65;IK 08;AC 50/60Hz;A+;n/a;0;Electronic ballast;6.0m;CRI80;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Ghost_Photometrics : C.8038H
C.8038N_LINEAR GHOST _L810_4000K_1127lm_14W;C.8038N;0;4000;14;1127;;4.26;3 years;220;240;230;1650;n/a;II;https://www.simes.it/en/overview/127/ghost-for-cast-concrete;Ghost for cast concrete is a luminous void created through a specific recessed housing fixed to the shutters before casting.;https://www.simes.it/en/search/?q=8038;1;90;810;88;Wall recessed;LINEAR GHOST L810 WALL RECESSED;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRGHOST-LINEA2.pdf;IP65;IK 08;AC 50/60Hz;A+;n/a;0;Electronic ballast;6.0m;CRI80;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Ghost_Photometrics : C.8038N
C.8038W_LINEAR GHOST _L810_3000K_1044lm_14W;C.8038W;0;3000;14;1044;;4.26;3 years;220;240;230;1528;n/a;II;https://www.simes.it/en/overview/127/ghost-for-cast-concrete;Ghost for cast concrete is a luminous void created through a specific recessed housing fixed to the shutters before casting.;https://www.simes.it/en/search/?q=8038;1;90;810;88;Wall recessed;LINEAR GHOST L810 WALL RECESSED;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRGHOST-LINEA2.pdf;IP65;IK 08;AC 50/60Hz;A+;n/a;0;Electronic ballast;6.0m;CRI80;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Ghost_Photometrics : C.8038W
C.8040H_LINEAR GHOST _L1570_2700K_1973lm_28W;C.8040H;0;2700;28;1973;;7.44;3 years;220;240;230;2903;n/a;II;https://www.simes.it/en/overview/127/ghost-for-cast-concrete;Ghost for cast concrete is a luminous void created through a specific recessed housing fixed to the shutters before casting.;https://www.simes.it/en/search/?q=8040;1;90;1570;88;Wall recessed;LINEAR GHOST L1570 WALL RECESSED;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRGHOST-LINEA2.pdf;IP65;IK 08;AC 50/60Hz;A+;n/a;0;Electronic ballast;6.0m;CRI80;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Ghost_Photometrics : C.8040H
C.8040N_LINEAR GHOST _L1570_4000K_2243lm_28W;C.8040N;0;4000;28;2243;;7.44;3 years;220;240;230;3300;n/a;II;https://www.simes.it/en/overview/127/ghost-for-cast-concrete;Ghost for cast concrete is a luminous void created through a specific recessed housing fixed to the shutters before casting.;https://www.simes.it/en/search/?q=8040;1;90;1570;88;Wall recessed;LINEAR GHOST L1570 WALL RECESSED;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRGHOST-LINEA2.pdf;IP65;IK 08;AC 50/60Hz;A+;n/a;0;Electronic ballast;6.0m;CRI80;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Ghost_Photometrics : C.8040N
C.8040W_LINEAR GHOST _L1570_3000K_2077lm_28W;C.8040W;0;3000;28;2077;;7.44;3 years;220;240;230;3056;n/a;II;https://www.simes.it/en/overview/127/ghost-for-cast-concrete;Ghost for cast concrete is a luminous void created through a specific recessed housing fixed to the shutters before casting.;https://www.simes.it/en/search/?q=8040;1;90;1570;88;Wall recessed;LINEAR GHOST L1570 WALL RECESSED;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRGHOST-LINEA2.pdf;IP65;IK 08;AC 50/60Hz;A+;n/a;0;Electronic ballast;6.0m;CRI80;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Ghost_Photometrics : C.8040W
