;SIMES_Product Code##OTHER##;SIMES_Beam Angle##ANGLE##DEGREES;SIMES_Color Temperature##COLOR_TEMPERATURE##KELVIN;SIMES_Rated Wattage##ELECTRICAL_POWER##WATTS;SIMES_Rated Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;SIMES_Finishes##OTHER##;SIMES_Weigth##MASS##KILOGRAMS;SIMES_Warranty Period##OTHER##;SIMES_Supply Voltage Min##ELECTRICAL_POTENTIAL##VOLTS;SIMES_Supply Voltage Max##ELECTRICAL_POTENTIAL##VOLTS;SIMES_Supply Voltage##ELECTRICAL_POTENTIAL##VOLTS;SIMES_Source Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;SIMES_Remote Power Supply##OTHER##;SIMES_Protection Class##OTHER##;SIMES_Product Page URL##OTHER##;SIMES_Product Description##OTHER##;SIMES_Product Data Sheet URL##OTHER##;SIMES_Number of Poles##OTHER##;SIMES_Nominal Width##LENGTH##MILLIMETERS;SIMES_Nominal Length##LENGTH##MILLIMETERS;SIMES_Nominal Height##LENGTH##MILLIMETERS;SIMES_Mounting Type##OTHER##;SIMES_Model##OTHER##;SIMES_Material Description##OTHER##;SIMES_Manufacturer Comment##OTHER##;SIMES_Luminous Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;SIMES_Light Source Type##OTHER##;SIMES_Lamp Count##OTHER##;SIMES_Installation Note URL##OTHER##;SIMES_IP Rating##OTHER##;SIMES_IK Rating##OTHER##;SIMES_Frequency##OTHER##;SIMES_Energy Efficiency Class##OTHER##;SIMES_Dimmable##OTHER##;SIMES_Current##ELECTRICAL_CURRENT##AMPERES;SIMES_Control Gear##OTHER##;SIMES_Cable Length##OTHER##;SIMES_CRI##OTHER##;SIMES_Approval Mark##OTHER##;LightFixturePlacingType##OTHER##;LightFixtureMountingType##OTHER##;Light Source##OTHER##;HasProtectiveEarth##OTHER##;Ground Stake##OTHER##;Body##OTHER##;Photometric_Type##OTHER##
S.3976N.14_SLOT DOUBLE_POST TOP_4000K_7550lm_79,2W_Aluminium grey;S.3976N.14;0;4000;79.2;7550;14 Aluminium Grey;16.7;3 years;220;240;230;11520;n/a;II;https://www.simes.it/en/overview/66/slot-pole;SLOT POLE is a minimalist pole-top luminaire for urban illumination and direct refletor. Its asymmetric optic is directed downwards allowing optimum light distribution.;https://www.simes.it/en/search/?q=3976;1;250;842;550;Post Top;SLOT POST TOP DOUBLE;Aluminium body;n/a;0;LED;1; https://www.simes.it/download/montaggio/ISTMEGSLPALOD2P.pdf;IP65;IK 09;AC 50-60Hz / DC;A+;DALI2/PUSH;0;Electronic ballast;0.4m;CRI80;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Slot_Pole_Photometrics : S.3973N
S.3976N.24_SLOT DOUBLE_POST TOP_4000K_7550lm_79,2W_Anthracite grey;S.3976N.24;0;4000;79.2;7550;24 Anthracite Grey;16.7;3 years;220;240;230;11520;n/a;II;https://www.simes.it/en/overview/66/slot-pole;SLOT POLE is a minimalist pole-top luminaire for urban illumination and direct refletor. Its asymmetric optic is directed downwards allowing optimum light distribution.;https://www.simes.it/en/search/?q=3976;1;250;842;550;Post Top;SLOT POST TOP DOUBLE;Aluminium body;n/a;0;LED;1; https://www.simes.it/download/montaggio/ISTMEGSLPALOD2P.pdf;IP65;IK 09;AC 50-60Hz / DC;A+;DALI2/PUSH;0;Electronic ballast;0.4m;CRI80;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_24_Anthracyte grey;Simes_Slot_Pole_Photometrics : S.3973N
S.3976W.14_SLOT DOUBLE_POST TOP_3000K_7074lm_79,2W_Aluminium grey;S.3976W.14;0;3000;79.2;7074;14 Aluminium Grey;16.7;3 years;220;240;230;10800;n/a;II;https://www.simes.it/en/overview/66/slot-pole;SLOT POLE is a minimalist pole-top luminaire for urban illumination and direct refletor. Its asymmetric optic is directed downwards allowing optimum light distribution.;https://www.simes.it/en/search/?q=3976;1;250;842;550;Post Top;SLOT POST TOP DOUBLE;Aluminium body;n/a;0;LED;1; https://www.simes.it/download/montaggio/ISTMEGSLPALOD2P.pdf;IP65;IK 09;AC 50-60Hz / DC;A+;DALI2/PUSH;0;Electronic ballast;0.4m;CRI80;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Slot_Pole_Photometrics : S.3973W
S.3976W.24_SLOT DOUBLE_POST TOP_3000K_7074lm_79,2W_Anthracite grey;S.3976W.24;0;3000;79.2;7074;24 Anthracite Grey;16.7;3 years;220;240;230;10800;n/a;II;https://www.simes.it/en/overview/66/slot-pole;SLOT POLE is a minimalist pole-top luminaire for urban illumination and direct refletor. Its asymmetric optic is directed downwards allowing optimum light distribution.;https://www.simes.it/en/search/?q=3976;1;250;842;550;Post Top;SLOT POST TOP DOUBLE;Aluminium body;n/a;0;LED;1; https://www.simes.it/download/montaggio/ISTMEGSLPALOD2P.pdf;IP65;IK 09;AC 50-60Hz / DC;A+;DALI2/PUSH;0;Electronic ballast;0.4m;CRI80;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_24_Anthracyte grey;Simes_Slot_Pole_Photometrics : S.3973W
S.3976H.14_SLOT DOUBLE_POST TOP_2700K_6602lm_79,2W_Aluminium grey;S.3976H.14;0;2700;79.2;6602;14 Aluminium Grey;16.7;3 years;220;240;230;10080;n/a;II;https://www.simes.it/en/overview/66/slot-pole;SLOT POLE is a minimalist pole-top luminaire for urban illumination and direct refletor. Its asymmetric optic is directed downwards allowing optimum light distribution.;https://www.simes.it/en/search/?q=3976;1;250;842;550;Post Top;SLOT POST TOP DOUBLE;Aluminium body;n/a;0;LED;1; https://www.simes.it/download/montaggio/ISTMEGSLPALOD2P.pdf;IP65;IK 09;AC 50-60Hz / DC;A+;DALI2/PUSH;0;Electronic ballast;0.4m;CRI80;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Slot_Pole_Photometrics : S.3973H
S.3976H.24_SLOT DOUBLE_POST TOP_2700K_6602lm_79,2W_Anthracite grey;S.3976H.24;0;2700;79.2;6602;24 Anthracite Grey;16.7;3 years;220;240;230;10080;n/a;II;https://www.simes.it/en/overview/66/slot-pole;SLOT POLE is a minimalist pole-top luminaire for urban illumination and direct refletor. Its asymmetric optic is directed downwards allowing optimum light distribution.;https://www.simes.it/en/search/?q=3976;1;250;842;550;Post Top;SLOT POST TOP DOUBLE;Aluminium body;n/a;0;LED;1; https://www.simes.it/download/montaggio/ISTMEGSLPALOD2P.pdf;IP65;IK 09;AC 50-60Hz / DC;A+;DALI2/PUSH;0;Electronic ballast;0.4m;CRI80;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_24_Anthracyte grey;Simes_Slot_Pole_Photometrics : S.3973H
