;SIMES_Product Code##OTHER##;SIMES_Beam Angle##ANGLE##DEGREES;SIMES_Color Temperature##COLOR_TEMPERATURE##KELVIN;SIMES_Rated Wattage##ELECTRICAL_POWER##WATTS;SIMES_Rated Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;SIMES_Finishes##OTHER##;SIMES_Weigth##MASS##KILOGRAMS;SIMES_Warranty Period##OTHER##;SIMES_Supply Voltage Min##ELECTRICAL_POTENTIAL##VOLTS;SIMES_Supply Voltage Max##ELECTRICAL_POTENTIAL##VOLTS;SIMES_Supply Voltage##ELECTRICAL_POTENTIAL##VOLTS;SIMES_Source Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;SIMES_Remote Power Supply##OTHER##;SIMES_Protection Class##OTHER##;SIMES_Product Page URL##OTHER##;SIMES_Product Description##OTHER##;SIMES_Product Data Sheet URL##OTHER##;SIMES_Number of Poles##OTHER##;SIMES_Nominal Width##LENGTH##MILLIMETERS;SIMES_Nominal Length##LENGTH##MILLIMETERS;SIMES_Nominal Height##LENGTH##MILLIMETERS;SIMES_Mounting Type##OTHER##;SIMES_Model##OTHER##;SIMES_Material Description##OTHER##;SIMES_Manufacturer Comment##OTHER##;SIMES_Luminous Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;SIMES_Light Source Type##OTHER##;SIMES_Lamp Count##OTHER##;SIMES_Installation Note URL##OTHER##;SIMES_IP Rating##OTHER##;SIMES_IK Rating##OTHER##;SIMES_Frequency##OTHER##;SIMES_Energy Efficiency Class##OTHER##;SIMES_Dimmable##OTHER##;SIMES_Current##ELECTRICAL_CURRENT##AMPERES;SIMES_Control Gear##OTHER##;SIMES_Cable Length##OTHER##;SIMES_CRI##OTHER##;SIMES_Approval Mark##OTHER##;LightFixturePlacingType##OTHER##;LightFixtureMountingType##OTHER##;Light Source##OTHER##;HasProtectiveEarth##OTHER##;Ground Stake##OTHER##;Body##OTHER##;Photometric_Type##OTHER##
S.1510H.01_KEEN_12°_2700K_1109lm_16.5W_White;S.1510H.01;12;2700;16.5;1109;01 White;2.0;3 years;220;240;230;1121;n/a;II;https://www.simes.it/en/overview/103/keen;Keen represents the evolution of outdoor lighting projectors. A special double joint allows the projector to take infinite positions for different light effects. Its minimal design makes it suitable for a wide range of architectural project applications.;https://www.simes.it/en/search/?q=1510;1;45;140;185;Surface mounted;KEEN 9° PROJECTOR;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRKEEN2.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;DALI2 / PUSH;0;Electronic ballast;0.15m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_01_White;Simes_Keen_Photometrics : S.1510H
S.1510H.14_KEEN_12°_2700K_1109lm_16.5W_Aluminium grey;S.1510H.14;12;2700;16.5;1109;14 Aluminium Grey;2.0;3 years;220;240;230;1121;n/a;II;https://www.simes.it/en/overview/103/keen;Keen represents the evolution of outdoor lighting projectors. A special double joint allows the projector to take infinite positions for different light effects. Its minimal design makes it suitable for a wide range of architectural project applications.;https://www.simes.it/en/search/?q=1510;1;45;140;185;Surface mounted;KEEN 9° PROJECTOR;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRKEEN2.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;DALI2 / PUSH;0;Electronic ballast;0.15m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Keen_Photometrics : S.1510H
S.1510N.01_KEEN_12°_4000K_1398lm_16.5W_White;S.1510N.01;12;4000;16.5;1398;01 White;2.0;3 years;220;240;230;1274;n/a;II;https://www.simes.it/en/overview/103/keen;Keen represents the evolution of outdoor lighting projectors. A special double joint allows the projector to take infinite positions for different light effects. Its minimal design makes it suitable for a wide range of architectural project applications.;https://www.simes.it/en/search/?q=1510;1;45;140;185;Surface mounted;KEEN 9° PROJECTOR;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRKEEN2.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;DALI2 / PUSH;0;Electronic ballast;0.15m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_01_White;Simes_Keen_Photometrics : S.1510N
S.1510N.14_KEEN_12°_4000K_1398lm_16.5W_Aluminium grey;S.1510N.14;12;4000;16.5;1398;14 Aluminium Grey;2.0;3 years;220;240;230;1274;n/a;II;https://www.simes.it/en/overview/103/keen;Keen represents the evolution of outdoor lighting projectors. A special double joint allows the projector to take infinite positions for different light effects. Its minimal design makes it suitable for a wide range of architectural project applications.;https://www.simes.it/en/search/?q=1510;1;45;140;185;Surface mounted;KEEN 9° PROJECTOR;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRKEEN2.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;DALI2 / PUSH;0;Electronic ballast;0.15m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Keen_Photometrics : S.1510N
S.1510W.01_KEEN_12°_3000K_1302lm_16.5W_White;S.1510W.01;12;3000;16.5;1302;01 White;2.0;3 years;220;240;230;1180;n/a;II;https://www.simes.it/en/overview/103/keen;Keen represents the evolution of outdoor lighting projectors. A special double joint allows the projector to take infinite positions for different light effects. Its minimal design makes it suitable for a wide range of architectural project applications.;https://www.simes.it/en/search/?q=1510;1;45;140;185;Surface mounted;KEEN 9° PROJECTOR;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRKEEN2.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;DALI2 / PUSH;0;Electronic ballast;0.15m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_01_White;Simes_Keen_Photometrics : S.1510W
S.1510W.14_KEEN_12°_3000K_1302lm_16.5W_Aluminium grey;S.1510W.14;12;3000;16.5;1302;14 Aluminium Grey;2.0;3 years;220;240;230;1180;n/a;II;https://www.simes.it/en/overview/103/keen;Keen represents the evolution of outdoor lighting projectors. A special double joint allows the projector to take infinite positions for different light effects. Its minimal design makes it suitable for a wide range of architectural project applications.;https://www.simes.it/en/search/?q=1510;1;45;140;185;Surface mounted;KEEN 9° PROJECTOR;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRKEEN2.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;DALI2 / PUSH;0;Electronic ballast;0.15m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Keen_Photometrics : S.1510W
S.1511H.01_KEEN_24°_2700K_1047lm_16.5W_White;S.1511H.01;24;2700;16.5;1047;01 White;2.0;3 years;220;240;230;1121;n/a;II;https://www.simes.it/en/overview/103/keen;Keen represents the evolution of outdoor lighting projectors. A special double joint allows the projector to take infinite positions for different light effects. Its minimal design makes it suitable for a wide range of architectural project applications.;https://www.simes.it/en/search/?q=1511;1;45;140;185;Surface mounted;KEEN 24° PROJECTOR;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRKEEN2.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;DALI2 / PUSH;0;Electronic ballast;0.15m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_01_White;Simes_Keen_Photometrics : S.1511H
S.1511H.14_KEEN_24°_2700K_1047lm_16.5W_Aluminium grey;S.1511H.14;24;2700;16.5;1047;14 Aluminium Grey;2.0;3 years;220;240;230;1121;n/a;II;https://www.simes.it/en/overview/103/keen;Keen represents the evolution of outdoor lighting projectors. A special double joint allows the projector to take infinite positions for different light effects. Its minimal design makes it suitable for a wide range of architectural project applications.;https://www.simes.it/en/search/?q=1511;1;45;140;185;Surface mounted;KEEN 24° PROJECTOR;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRKEEN2.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;DALI2 / PUSH;0;Electronic ballast;0.15m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Keen_Photometrics : S.1511H
S.1511N.01_KEEN_24°_4000K_1320lm_16.5W_White;S.1511N.01;24;4000;16.5;1320;01 White;2.0;3 years;220;240;230;1274;n/a;II;https://www.simes.it/en/overview/103/keen;Keen represents the evolution of outdoor lighting projectors. A special double joint allows the projector to take infinite positions for different light effects. Its minimal design makes it suitable for a wide range of architectural project applications.;https://www.simes.it/en/search/?q=1511;1;45;140;185;Surface mounted;KEEN 24° PROJECTOR;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRKEEN2.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;DALI2 / PUSH;0;Electronic ballast;0.15m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_01_White;Simes_Keen_Photometrics : S.1511N
S.1511N.14_KEEN_24°_4000K_1320lm_16.5W_Aluminium grey;S.1511N.14;24;4000;16.5;1320;14 Aluminium Grey;2.0;3 years;220;240;230;1274;n/a;II;https://www.simes.it/en/overview/103/keen;Keen represents the evolution of outdoor lighting projectors. A special double joint allows the projector to take infinite positions for different light effects. Its minimal design makes it suitable for a wide range of architectural project applications.;https://www.simes.it/en/search/?q=1511;1;45;140;185;Surface mounted;KEEN 24° PROJECTOR;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRKEEN2.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;DALI2 / PUSH;0;Electronic ballast;0.15m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Keen_Photometrics : S.1511N
S.1511W.01_KEEN_24°_3000K_1229lm_16.5W_White;S.1511W.01;24;3000;16.5;1229;01 White;2.0;3 years;220;240;230;1180;n/a;II;https://www.simes.it/en/overview/103/keen;Keen represents the evolution of outdoor lighting projectors. A special double joint allows the projector to take infinite positions for different light effects. Its minimal design makes it suitable for a wide range of architectural project applications.;https://www.simes.it/en/search/?q=1511;1;45;140;185;Surface mounted;KEEN 24° PROJECTOR;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRKEEN2.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;DALI2 / PUSH;0;Electronic ballast;0.15m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_01_White;Simes_Keen_Photometrics : S.1511W
S.1511W.14_KEEN_24°_3000K_1229lm_16.5W_Aluminium grey;S.1511W.14;24;3000;16.5;1229;14 Aluminium Grey;2.0;3 years;220;240;230;1180;n/a;II;https://www.simes.it/en/overview/103/keen;Keen represents the evolution of outdoor lighting projectors. A special double joint allows the projector to take infinite positions for different light effects. Its minimal design makes it suitable for a wide range of architectural project applications.;https://www.simes.it/en/search/?q=1511;1;45;140;185;Surface mounted;KEEN 24° PROJECTOR;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRKEEN2.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;DALI2 / PUSH;0;Electronic ballast;0.15m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Keen_Photometrics : S.1511W
S.1513H.01_KEEN_13°x44°_2700K_1008lm_16.5W_White;S.1513H.01;0;2700;16.5;1008;01 White;2.0;3 years;220;240;230;1121;n/a;II;https://www.simes.it/en/overview/103/keen;Keen represents the evolution of outdoor lighting projectors. A special double joint allows the projector to take infinite positions for different light effects. Its minimal design makes it suitable for a wide range of architectural project applications.;https://www.simes.it/en/search/?q=1513;1;45;140;185;Surface mounted;KEEN 12°x43° PROJECTOR;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRKEEN2.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;DALI2 / PUSH;0;Electronic ballast;0.15m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_01_White;Simes_Keen_Photometrics : S.1513H
S.1513H.14_KEEN_13°x44°_2700K_1008lm_16.5W_Aluminium grey;S.1513H.14;0;2700;16.5;1008;14 Aluminium Grey;2.0;3 years;220;240;230;1121;n/a;II;https://www.simes.it/en/overview/103/keen;Keen represents the evolution of outdoor lighting projectors. A special double joint allows the projector to take infinite positions for different light effects. Its minimal design makes it suitable for a wide range of architectural project applications.;https://www.simes.it/en/search/?q=1513;1;45;140;185;Surface mounted;KEEN 12°x43° PROJECTOR;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRKEEN2.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;DALI2 / PUSH;0;Electronic ballast;0.15m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Keen_Photometrics : S.1513H
S.1513N.01_KEEN_13°x44°_4000K_1271lm_16.5W_White;S.1513N.01;0;4000;16.5;1271;01 White;2.0;3 years;220;240;230;1274;n/a;II;https://www.simes.it/en/overview/103/keen;Keen represents the evolution of outdoor lighting projectors. A special double joint allows the projector to take infinite positions for different light effects. Its minimal design makes it suitable for a wide range of architectural project applications.;https://www.simes.it/en/search/?q=1513;1;45;140;185;Surface mounted;KEEN 12°x43° PROJECTOR;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRKEEN2.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;DALI2 / PUSH;0;Electronic ballast;0.15m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_01_White;Simes_Keen_Photometrics : S.1513N
S.1513N.14_KEEN_13°x44°_4000K_1271lm_16.5W_Aluminium grey;S.1513N.14;0;4000;16.5;1271;14 Aluminium Grey;2.0;3 years;220;240;230;1274;n/a;II;https://www.simes.it/en/overview/103/keen;Keen represents the evolution of outdoor lighting projectors. A special double joint allows the projector to take infinite positions for different light effects. Its minimal design makes it suitable for a wide range of architectural project applications.;https://www.simes.it/en/search/?q=1513;1;45;140;185;Surface mounted;KEEN 12°x43° PROJECTOR;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRKEEN2.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;DALI2 / PUSH;0;Electronic ballast;0.15m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Keen_Photometrics : S.1513N
S.1513W.01_KEEN_13°x44°_3000K_1183lm_16.5W_White;S.1513W.01;0;3000;16.5;1183;01 White;2.0;3 years;220;240;230;1180;n/a;II;https://www.simes.it/en/overview/103/keen;Keen represents the evolution of outdoor lighting projectors. A special double joint allows the projector to take infinite positions for different light effects. Its minimal design makes it suitable for a wide range of architectural project applications.;https://www.simes.it/en/search/?q=1513;1;45;140;185;Surface mounted;KEEN 12°x43° PROJECTOR;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRKEEN2.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;DALI2 / PUSH;0;Electronic ballast;0.15m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_01_White;Simes_Keen_Photometrics : S.1513W
S.1513W.14_KEEN_13°x44°_3000K_1183lm_16.5W_Aluminium grey;S.1513W.14;0;3000;16.5;1183;14 Aluminium Grey;2.0;3 years;220;240;230;1180;n/a;II;https://www.simes.it/en/overview/103/keen;Keen represents the evolution of outdoor lighting projectors. A special double joint allows the projector to take infinite positions for different light effects. Its minimal design makes it suitable for a wide range of architectural project applications.;https://www.simes.it/en/search/?q=1513;1;45;140;185;Surface mounted;KEEN 12°x43° PROJECTOR;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRKEEN2.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;DALI2 / PUSH;0;Electronic ballast;0.15m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Keen_Photometrics : S.1513W
