;SIMES_Product Code##OTHER##;SIMES_Beam Angle##ANGLE##DEGREES;SIMES_Color Temperature##COLOR_TEMPERATURE##KELVIN;SIMES_Rated Wattage##ELECTRICAL_POWER##WATTS;SIMES_Rated Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;SIMES_Finishes##OTHER##;SIMES_Weigth##MASS##KILOGRAMS;SIMES_Warranty Period##OTHER##;SIMES_Supply Voltage Min##ELECTRICAL_POTENTIAL##VOLTS;SIMES_Supply Voltage Max##ELECTRICAL_POTENTIAL##VOLTS;SIMES_Supply Voltage##ELECTRICAL_POTENTIAL##VOLTS;SIMES_Source Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;SIMES_Remote Power Supply##OTHER##;SIMES_Protection Class##OTHER##;SIMES_Product Page URL##OTHER##;SIMES_Product Description##OTHER##;SIMES_Product Data Sheet URL##OTHER##;SIMES_Number of Poles##OTHER##;SIMES_Nominal Width##LENGTH##MILLIMETERS;SIMES_Nominal Length##LENGTH##MILLIMETERS;SIMES_Nominal Height##LENGTH##MILLIMETERS;SIMES_Mounting Type##OTHER##;SIMES_Model##OTHER##;SIMES_Material Description##OTHER##;SIMES_Manufacturer Comment##OTHER##;SIMES_Luminous Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;SIMES_Light Source Type##OTHER##;SIMES_Lamp Count##OTHER##;SIMES_Installation Note URL##OTHER##;SIMES_IP Rating##OTHER##;SIMES_IK Rating##OTHER##;SIMES_Frequency##OTHER##;SIMES_Energy Efficiency Class##OTHER##;SIMES_Dimmable##OTHER##;SIMES_Current##ELECTRICAL_CURRENT##AMPERES;SIMES_Control Gear##OTHER##;SIMES_Cable Length##OTHER##;SIMES_CRI##OTHER##;SIMES_Approval Mark##OTHER##;LightFixturePlacingType##OTHER##;LightFixtureMountingType##OTHER##;Light Source##OTHER##;HasProtectiveEarth##OTHER##;Ground Stake##OTHER##;Body##OTHER##;Photometric_Type##OTHER##
S.6270H.01_MINISKILL ROUND WALL_2700K_180lm_3,7W_White;S.6270H.01;0;2700;3.7;180;01 White;0.5;3 years;24;24;24;549;need remote power supply type S.3400 230V/24V DC 10W;III;https://www.simes.it/en/overview/98/skill;"SKILL represents a new concept of outdoor lighting fitting; a recessed/not-recessed luminaire for wall mounting. It concentrates all the advantages of a recessed fitting, but without requiring a housing in the wall.";https://www.simes.it/en/search/?q=6270;1;28;105;105;Wall mounted;MINISKILL ROUND WALL MOUNTED;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRMSKILL2.pdf;IP65;IK 08;DC;A+;yes;0;n/a;1.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_01_White;Simes_Skill_Photometrics : S.6270H
S.6270H.14_MINISKILL ROUND WALL_2700K_180lm_3,7W_Aluminium grey;S.6270H.14;0;2700;3.7;180;14 Aluminium Grey;0.5;3 years;24;24;24;549;need remote power supply type S.3400 230V/24V DC 10W;III;https://www.simes.it/en/overview/98/skill;"SKILL represents a new concept of outdoor lighting fitting; a recessed/not-recessed luminaire for wall mounting. It concentrates all the advantages of a recessed fitting, but without requiring a housing in the wall.";https://www.simes.it/en/search/?q=6270;1;28;105;105;Wall mounted;MINISKILL ROUND WALL MOUNTED;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRMSKILL2.pdf;IP65;IK 08;DC;A+;yes;0;n/a;1.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Skill_Photometrics : S.6270H
S.6270H.24_MINISKILL ROUND WALL_2700K_180lm_3,7W_Anthracite grey;S.6270H.24;0;2700;3.7;180;24 Anthracite Grey;0.5;3 years;24;24;24;549;need remote power supply type S.3400 230V/24V DC 10W;III;https://www.simes.it/en/overview/98/skill;"SKILL represents a new concept of outdoor lighting fitting; a recessed/not-recessed luminaire for wall mounting. It concentrates all the advantages of a recessed fitting, but without requiring a housing in the wall.";https://www.simes.it/en/search/?q=6270;1;28;105;105;Wall mounted;MINISKILL ROUND WALL MOUNTED;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRMSKILL2.pdf;IP65;IK 08;DC;A+;yes;0;n/a;1.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_24_Anthracyte grey;Simes_Skill_Photometrics : S.6270H
S.6270N.01_MINISKILL ROUND WALL_4000K_189lm_3,7W_White;S.6270N.01;0;4000;3.7;189;01 White;0.5;3 years;24;24;24;734;need remote power supply type S.3400 230V/24V DC 10W;III;https://www.simes.it/en/overview/98/skill;"SKILL represents a new concept of outdoor lighting fitting; a recessed/not-recessed luminaire for wall mounting. It concentrates all the advantages of a recessed fitting, but without requiring a housing in the wall.";https://www.simes.it/en/search/?q=6270;1;28;105;105;Wall mounted;MINISKILL ROUND WALL MOUNTED;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRMSKILL2.pdf;IP65;IK 08;DC;A+;yes;0;n/a;1.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_01_White;Simes_Skill_Photometrics : S.6270N
S.6270N.14_MINISKILL ROUND WALL_4000K_189lm_3,7W_Aluminium grey;S.6270N.14;0;4000;3.7;189;14 Aluminium Grey;0.5;3 years;24;24;24;734;need remote power supply type S.3400 230V/24V DC 10W;III;https://www.simes.it/en/overview/98/skill;"SKILL represents a new concept of outdoor lighting fitting; a recessed/not-recessed luminaire for wall mounting. It concentrates all the advantages of a recessed fitting, but without requiring a housing in the wall.";https://www.simes.it/en/search/?q=6270;1;28;105;105;Wall mounted;MINISKILL ROUND WALL MOUNTED;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRMSKILL2.pdf;IP65;IK 08;DC;A+;yes;0;n/a;1.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Skill_Photometrics : S.6270N
S.6270N.24_MINISKILL ROUND WALL_4000K_189lm_3,7W_Anthracite grey;S.6270N.24;0;4000;3.7;189;24 Anthracite Grey;0.5;3 years;24;24;24;734;need remote power supply type S.3400 230V/24V DC 10W;III;https://www.simes.it/en/overview/98/skill;"SKILL represents a new concept of outdoor lighting fitting; a recessed/not-recessed luminaire for wall mounting. It concentrates all the advantages of a recessed fitting, but without requiring a housing in the wall.";https://www.simes.it/en/search/?q=6270;1;28;105;105;Wall mounted;MINISKILL ROUND WALL MOUNTED;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRMSKILL2.pdf;IP65;IK 08;DC;A+;yes;0;n/a;1.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_24_Anthracyte grey;Simes_Skill_Photometrics : S.6270N
S.6270W.01_MINISKILL ROUND WALL_3000K_185lm_3,7W_White;S.6270W.01;0;3000;3.7;185;01 White;0.5;3 years;24;24;24;565;need remote power supply type S.3400 230V/24V DC 10W;III;https://www.simes.it/en/overview/98/skill;"SKILL represents a new concept of outdoor lighting fitting; a recessed/not-recessed luminaire for wall mounting. It concentrates all the advantages of a recessed fitting, but without requiring a housing in the wall.";https://www.simes.it/en/search/?q=6270;1;28;105;105;Wall mounted;MINISKILL ROUND WALL MOUNTED;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRMSKILL2.pdf;IP65;IK 08;DC;A+;yes;0;n/a;1.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_01_White;Simes_Skill_Photometrics : S.6270W
S.6270W.14_MINISKILL ROUND WALL_3000K_185lm_3,7W_Aluminium grey;S.6270W.14;0;3000;3.7;185;14 Aluminium Grey;0.5;3 years;24;24;24;565;need remote power supply type S.3400 230V/24V DC 10W;III;https://www.simes.it/en/overview/98/skill;"SKILL represents a new concept of outdoor lighting fitting; a recessed/not-recessed luminaire for wall mounting. It concentrates all the advantages of a recessed fitting, but without requiring a housing in the wall.";https://www.simes.it/en/search/?q=6270;1;28;105;105;Wall mounted;MINISKILL ROUND WALL MOUNTED;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRMSKILL2.pdf;IP65;IK 08;DC;A+;yes;0;n/a;1.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Skill_Photometrics : S.6270W
S.6270W.24_MINISKILL ROUND WALL_3000K_185lm_3,7W_Anthracite grey;S.6270W.24;0;3000;3.7;185;24 Anthracite Grey;0.5;3 years;24;24;24;565;need remote power supply type S.3400 230V/24V DC 10W;III;https://www.simes.it/en/overview/98/skill;"SKILL represents a new concept of outdoor lighting fitting; a recessed/not-recessed luminaire for wall mounting. It concentrates all the advantages of a recessed fitting, but without requiring a housing in the wall.";https://www.simes.it/en/search/?q=6270;1;28;105;105;Wall mounted;MINISKILL ROUND WALL MOUNTED;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRMSKILL2.pdf;IP65;IK 08;DC;A+;yes;0;n/a;1.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_24_Anthracyte grey;Simes_Skill_Photometrics : S.6270W
