;SIMES_Product Code##OTHER##;SIMES_Beam Angle##ANGLE##DEGREES;SIMES_Color Temperature##COLOR_TEMPERATURE##KELVIN;SIMES_Rated Wattage##ELECTRICAL_POWER##WATTS;SIMES_Rated Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;SIMES_Finishes##OTHER##;SIMES_Weigth##MASS##KILOGRAMS;SIMES_Warranty Period##OTHER##;SIMES_Supply Voltage Min##ELECTRICAL_POTENTIAL##VOLTS;SIMES_Supply Voltage Max##ELECTRICAL_POTENTIAL##VOLTS;SIMES_Supply Voltage##ELECTRICAL_POTENTIAL##VOLTS;SIMES_Source Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;SIMES_Remote Power Supply##OTHER##;SIMES_Protection Class##OTHER##;SIMES_Product Page URL##OTHER##;SIMES_Product Description##OTHER##;SIMES_Product Data Sheet URL##OTHER##;SIMES_Number of Poles##OTHER##;SIMES_Nominal Width##LENGTH##MILLIMETERS;SIMES_Nominal Length##LENGTH##MILLIMETERS;SIMES_Nominal Height##LENGTH##MILLIMETERS;SIMES_Mounting Type##OTHER##;SIMES_Model##OTHER##;SIMES_Material Description##OTHER##;SIMES_Manufacturer Comment##OTHER##;SIMES_Luminous Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;SIMES_Light Source Type##OTHER##;SIMES_Lamp Count##OTHER##;SIMES_Installation Note URL##OTHER##;SIMES_IP Rating##OTHER##;SIMES_IK Rating##OTHER##;SIMES_Frequency##OTHER##;SIMES_Energy Efficiency Class##OTHER##;SIMES_Dimmable##OTHER##;SIMES_Current##ELECTRICAL_CURRENT##AMPERES;SIMES_Control Gear##OTHER##;SIMES_Cable Length##OTHER##;SIMES_CRI##OTHER##;SIMES_Approval Mark##OTHER##;LightFixturePlacingType##OTHER##;LightFixtureMountingType##OTHER##;Light Source##OTHER##;HasProtectiveEarth##OTHER##;Ground Stake##OTHER##;Body##OTHER##;Photometric_Type##OTHER##
S.8884N.19_ZIP_COMFORT_ACIDETCHEDGLASS_SQUARE_4000K_101lm_7.5W_Stainless Steel;S.8884N.19;80;4000;7.5;101;19 Stainless Steel;3.4;3 years;220;240;230;605;n/a;I;https://www.simes.it/en/overview/167/zip-comfort;It has constantly evolved to achieve greater and more precise lighting control and high performance in terms of flux and efficiency. ZIP COMFORT is the right answer to the most difficult architectural challenges thanks to the availability of many different combinations.;https://www.simes.it/en/search/?q=8884;1;200;200;240;Inground;ZIP SQUARE WALKOVER STAINLESS STEEL ACID-ETCHED GLASS;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRZIPCOMF-IN2.pdf;IP65/IP67;IK 09;AC 50-60Hz / DC;A+;DALI2/PUSH;0;Electronic ballast;0.5m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_19_Stainless Steel;Simes_Zip_Comfort_Square_Photometrics : S.8884N
S.8884W.19_ZIP_COMFORT_ACIDETCHEDGLASS_SQUARE_3000K_92lm_7.5W_Stainless Steel;S.8884W.19;80;3000;7.5;92;19 Stainless Steel;3.4;3 years;220;240;230;560;n/a;I;https://www.simes.it/en/overview/167/zip-comfort;It has constantly evolved to achieve greater and more precise lighting control and high performance in terms of flux and efficiency. ZIP COMFORT is the right answer to the most difficult architectural challenges thanks to the availability of many different combinations.;https://www.simes.it/en/search/?q=8884;1;200;200;240;Inground;ZIP SQUARE WALKOVER STAINLESS STEEL ACID-ETCHED GLASS;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRZIPCOMF-IN2.pdf;IP65/IP67;IK 09;AC 50-60Hz / DC;A+;DALI2/PUSH;0;Electronic ballast;0.5m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_19_Stainless Steel;Simes_Zip_Comfort_Square_Photometrics : S.8884W
S.8884H.19_ZIP_COMFORT_ACIDETCHEDGLASS_SQUARE_2700K_57lm_7.5W_Stainless Steel;S.8884H.19;80;2700;7.5;57;19 Stainless Steel;3.4;3 years;220;240;230;532;n/a;I;https://www.simes.it/en/overview/167/zip-comfort;It has constantly evolved to achieve greater and more precise lighting control and high performance in terms of flux and efficiency. ZIP COMFORT is the right answer to the most difficult architectural challenges thanks to the availability of many different combinations.;https://www.simes.it/en/search/?q=8884;1;200;200;240;Inground;ZIP SQUARE WALKOVER STAINLESS STEEL ACID-ETCHED GLASS;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRZIPCOMF-IN2.pdf;IP65/IP67;IK 09;AC 50-60Hz / DC;A+;DALI2/PUSH;0;Electronic ballast;0.5m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_19_Stainless Steel;Simes_Zip_Comfort_Square_Photometrics : S.8884H
S.8895N.19_ZIP_COMFORT_12°_SQUARE_4000K_1179lm_16.6W_Stainless Steel;S.8895N.19;11;4000;16.6;1179;19 Stainless Steel;3.4;3 years;220;240;230;1660;n/a;I;https://www.simes.it/en/overview/167/zip-comfort;It has constantly evolved to achieve greater and more precise lighting control and high performance in terms of flux and efficiency. ZIP COMFORT is the right answer to the most difficult architectural challenges thanks to the availability of many different combinations.;https://www.simes.it/en/search/?q=8895;1;200;200;240;Inground;ZIP SQUARE WALKOVER STAINLESS STEEL 12°;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRZIPCOMF-IN2.pdf;IP65/IP67;IK 09;AC 50-60Hz / DC;A+;DALI2/PUSH;0;Electronic ballast;0.5m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_19_Stainless Steel;Simes_Zip_Comfort_Square_Photometrics : S.8895N
S.8895W.19_ZIP_COMFORT_12°_SQUARE_3000K_1143lm_16.6W_Stainless Steel;S.8895W.19;11;3000;16.6;1143;19 Stainless Steel;3.4;3 years;220;240;230;1520;n/a;I;https://www.simes.it/en/overview/167/zip-comfort;It has constantly evolved to achieve greater and more precise lighting control and high performance in terms of flux and efficiency. ZIP COMFORT is the right answer to the most difficult architectural challenges thanks to the availability of many different combinations.;https://www.simes.it/en/search/?q=8895;1;200;200;240;Inground;ZIP SQUARE WALKOVER STAINLESS STEEL 12°;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRZIPCOMF-IN2.pdf;IP65/IP67;IK 09;AC 50-60Hz / DC;A+;DALI2/PUSH;0;Electronic ballast;0.5m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_19_Stainless Steel;Simes_Zip_Comfort_Square_Photometrics : S.8895W
S.8895H.19_ZIP_COMFORT_12°_SQUARE_2700K_1011lm_16.6W_Stainless Steel;S.8895H.19;11;2700;16.6;1011;19 Stainless Steel;3.4;3 years;220;240;230;1450;n/a;I;https://www.simes.it/en/overview/167/zip-comfort;It has constantly evolved to achieve greater and more precise lighting control and high performance in terms of flux and efficiency. ZIP COMFORT is the right answer to the most difficult architectural challenges thanks to the availability of many different combinations.;https://www.simes.it/en/search/?q=8895;1;200;200;240;Inground;ZIP SQUARE WALKOVER STAINLESS STEEL 12°;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRZIPCOMF-IN2.pdf;IP65/IP67;IK 09;AC 50-60Hz / DC;A+;DALI2/PUSH;0;Electronic ballast;0.5m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_19_Stainless Steel;Simes_Zip_Comfort_Square_Photometrics : S.8895H
S.8896N.19_ZIP_COMFORT_ASY_SQUARE_4000K_1250lm_16.6W_Stainless Steel;S.8896N.19;0;4000;16.6;1250;19 Stainless Steel;3.4;3 years;220;240;230;1660;n/a;I;https://www.simes.it/en/overview/167/zip-comfort;It has constantly evolved to achieve greater and more precise lighting control and high performance in terms of flux and efficiency. ZIP COMFORT is the right answer to the most difficult architectural challenges thanks to the availability of many different combinations.;https://www.simes.it/en/search/?q=8896;1;200;200;240;Inground;ZIP SQUARE WALKOVER STAINLESS STEEL ASY;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRZIPCOMF-IN2.pdf;IP65/IP67;IK 09;AC 50-60Hz / DC;A+;DALI2/PUSH;0;Electronic ballast;0.5m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_19_Stainless Steel;Simes_Zip_Comfort_Square_Photometrics : S.8896N
S.8896W.19_ZIP_COMFORT_ASY_SQUARE_3000K_1188lm_16.6W_Stainless Steel;S.8896W.19;0;3000;16.6;1188;19 Stainless Steel;3.4;3 years;220;240;230;1520;n/a;I;https://www.simes.it/en/overview/167/zip-comfort;It has constantly evolved to achieve greater and more precise lighting control and high performance in terms of flux and efficiency. ZIP COMFORT is the right answer to the most difficult architectural challenges thanks to the availability of many different combinations.;https://www.simes.it/en/search/?q=8896;1;200;200;240;Inground;ZIP SQUARE WALKOVER STAINLESS STEEL ASY;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRZIPCOMF-IN2.pdf;IP65/IP67;IK 09;AC 50-60Hz / DC;A+;DALI2/PUSH;0;Electronic ballast;0.5m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_19_Stainless Steel;Simes_Zip_Comfort_Square_Photometrics : S.8896W
S.8896H.19_ZIP_COMFORT_ASY_SQUARE_2700K_1083lm_16.6W_Stainless Steel;S.8896H.19;0;2700;16.6;1083;19 Stainless Steel;3.4;3 years;220;240;230;1450;n/a;I;https://www.simes.it/en/overview/167/zip-comfort;It has constantly evolved to achieve greater and more precise lighting control and high performance in terms of flux and efficiency. ZIP COMFORT is the right answer to the most difficult architectural challenges thanks to the availability of many different combinations.;https://www.simes.it/en/search/?q=8896;1;200;200;240;Inground;ZIP SQUARE WALKOVER STAINLESS STEEL ASY;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRZIPCOMF-IN2.pdf;IP65/IP67;IK 09;AC 50-60Hz / DC;A+;DALI2/PUSH;0;Electronic ballast;0.5m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_19_Stainless Steel;Simes_Zip_Comfort_Square_Photometrics : S.8896H
S.8897N.19_ZIP_COMFORT_33°_SQUARE_4000K_1023lm_15.2W_Stainless Steel;S.8897N.19;25;4000;15.2;1023;19 Stainless Steel;3.4;3 years;220;240;230;1544;n/a;I;https://www.simes.it/en/overview/167/zip-comfort;It has constantly evolved to achieve greater and more precise lighting control and high performance in terms of flux and efficiency. ZIP COMFORT is the right answer to the most difficult architectural challenges thanks to the availability of many different combinations.;https://www.simes.it/en/search/?q=8897;1;200;200;240;Inground;ZIP SQUARE WALKOVER STAINLESS STEEL 33°;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRZIPCOMF-IN2.pdf;IP65/IP67;IK 09;AC 50-60Hz / DC;A+;DALI2/PUSH;0;Electronic ballast;0.5m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_19_Stainless Steel;Simes_Zip_Comfort_Square_Photometrics : S.8897N
S.8897W.19_ZIP_COMFORT_33°_SQUARE_3000K_973lm_15.2W_Stainless Steel;S.8897W.19;25;3000;15.2;973;19 Stainless Steel;3.4;3 years;220;240;230;1522;n/a;I;https://www.simes.it/en/overview/167/zip-comfort;It has constantly evolved to achieve greater and more precise lighting control and high performance in terms of flux and efficiency. ZIP COMFORT is the right answer to the most difficult architectural challenges thanks to the availability of many different combinations.;https://www.simes.it/en/search/?q=8897;1;200;200;240;Inground;ZIP SQUARE WALKOVER STAINLESS STEEL 33°;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRZIPCOMF-IN2.pdf;IP65/IP67;IK 09;AC 50-60Hz / DC;A+;DALI2/PUSH;0;Electronic ballast;0.5m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_19_Stainless Steel;Simes_Zip_Comfort_Square_Photometrics : S.8897W
S.8897H.19_ZIP_COMFORT_33°_SQUARE_2700K_940lm_15.2W_Stainless Steel;S.8897H.19;25;2700;15.2;940;19 Stainless Steel;3.4;3 years;220;240;230;1449;n/a;I;https://www.simes.it/en/overview/167/zip-comfort;It has constantly evolved to achieve greater and more precise lighting control and high performance in terms of flux and efficiency. ZIP COMFORT is the right answer to the most difficult architectural challenges thanks to the availability of many different combinations.;https://www.simes.it/en/search/?q=8897;1;200;200;240;Inground;ZIP SQUARE WALKOVER STAINLESS STEEL 33°;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRZIPCOMF-IN2.pdf;IP65/IP67;IK 09;AC 50-60Hz / DC;A+;DALI2/PUSH;0;Electronic ballast;0.5m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_19_Stainless Steel;Simes_Zip_Comfort_Square_Photometrics : S.8897H
S.8899.19_ZIP_COMFORT_33°_SQUARE_RGBW (W=3000K)_-lm_15W_Stainless Steel;S.8899.19;33;0;15;0;19 Stainless Steel;3.4;3 years;24;24;24;0;need remote power supply type S.3411 230V/24V PWM 60W & DMX RGBW CONTROLLER type S.2450;III;https://www.simes.it/en/overview/167/zip-comfort;It has constantly evolved to achieve greater and more precise lighting control and high performance in terms of flux and efficiency. ZIP COMFORT is the right answer to the most difficult architectural challenges thanks to the availability of many different combinations.;https://www.simes.it/en/search/?q=8899;1;200;200;240;Inground;ZIP SQUARE WALKOVER STAINLESS STEEL 33° RGBW;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRZIPIRGBW24.pdf;IP65/IP67;IK 09;AC 50-60Hz / DC;A+;RGBW DMX;0;Electronic ballast;0.5m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_19_Stainless Steel;Simes_Zip_Comfort_Square_Photometrics : S.8899
S.7884N.09_ZIP_COMFORT_ACIDETCHEDGLASS_SQUARE_4000K_101lm_7.5W_Black;S.7884N.09;80;4000;7.5;101;09 Black;3.4;3 years;220;240;230;605;n/a;I;https://www.simes.it/en/overview/167/zip-comfort;It has constantly evolved to achieve greater and more precise lighting control and high performance in terms of flux and efficiency. ZIP COMFORT is the right answer to the most difficult architectural challenges thanks to the availability of many different combinations.;https://www.simes.it/en/search/?q=7884;1;200;200;240;Inground;ZIP SQUARE WALKOVER  ACID-ETCHED GLASS;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRZIPCOMF-IN2.pdf;IP65/IP67;IK 09;AC 50-60Hz / DC;A+;DALI2/PUSH;0;Electronic ballast;0.5m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_09_Black;Simes_Zip_Comfort_Square_Photometrics : S.8884N
S.7884W.09_ZIP_COMFORT_ACIDETCHEDGLASS_SQUARE_3000K_92lm_7.5W_Black;S.7884W.09;80;3000;7.5;92;09 Black;3.4;3 years;220;240;230;560;n/a;I;https://www.simes.it/en/overview/167/zip-comfort;It has constantly evolved to achieve greater and more precise lighting control and high performance in terms of flux and efficiency. ZIP COMFORT is the right answer to the most difficult architectural challenges thanks to the availability of many different combinations.;https://www.simes.it/en/search/?q=7884;1;200;200;240;Inground;ZIP SQUARE WALKOVER ACID-ETCHED GLASS;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRZIPCOMF-IN2.pdf;IP65/IP67;IK 09;AC 50-60Hz / DC;A+;DALI2/PUSH;0;Electronic ballast;0.5m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_09_Black;Simes_Zip_Comfort_Square_Photometrics : S.8884W
S.7884H.09_ZIP_COMFORT_ACIDETCHEDGLASS_SQUARE_2700K_57lm_7.5W_Black;S.7884H.09;80;2700;7.5;57;09 Black;3.4;3 years;220;240;230;532;n/a;I;https://www.simes.it/en/overview/167/zip-comfort;It has constantly evolved to achieve greater and more precise lighting control and high performance in terms of flux and efficiency. ZIP COMFORT is the right answer to the most difficult architectural challenges thanks to the availability of many different combinations.;https://www.simes.it/en/search/?q=7884;1;200;200;240;Inground;ZIP SQUARE WALKOVER  ACID-ETCHED GLASS;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRZIPCOMF-IN2.pdf;IP65/IP67;IK 09;AC 50-60Hz / DC;A+;DALI2/PUSH;0;Electronic ballast;0.5m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_09_Black;Simes_Zip_Comfort_Square_Photometrics : S.8884H
S.7895N.09_ZIP_COMFORT_12°_SQUARE_4000K_1179lm_16.6W_Black;S.7895N.09;11;4000;16.6;1179;09 Black;3.4;3 years;220;240;230;1660;n/a;I;https://www.simes.it/en/overview/167/zip-comfort;It has constantly evolved to achieve greater and more precise lighting control and high performance in terms of flux and efficiency. ZIP COMFORT is the right answer to the most difficult architectural challenges thanks to the availability of many different combinations.;https://www.simes.it/en/search/?q=7895;1;200;200;240;Inground;ZIP SQUARE WALKOVER  12°;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRZIPCOMF-IN2.pdf;IP65/IP67;IK 09;AC 50-60Hz / DC;A+;DALI2/PUSH;0;Electronic ballast;0.5m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_09_Black;Simes_Zip_Comfort_Square_Photometrics : S.8895N
S.7895W.09_ZIP_COMFORT_12°_SQUARE_3000K_1143lm_16.6W_Black;S.7895W.09;11;3000;16.6;1143;09 Black;3.4;3 years;220;240;230;1520;n/a;I;https://www.simes.it/en/overview/167/zip-comfort;It has constantly evolved to achieve greater and more precise lighting control and high performance in terms of flux and efficiency. ZIP COMFORT is the right answer to the most difficult architectural challenges thanks to the availability of many different combinations.;https://www.simes.it/en/search/?q=7895;1;200;200;240;Inground;ZIP SQUARE WALKOVER 12°;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRZIPCOMF-IN2.pdf;IP65/IP67;IK 09;AC 50-60Hz / DC;A+;DALI2/PUSH;0;Electronic ballast;0.5m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_09_Black;Simes_Zip_Comfort_Square_Photometrics : S.8895W
S.7895H.09_ZIP_COMFORT_12°_SQUARE_2700K_1011lm_16.6W_Black;S.7895H.09;11;2700;16.6;1011;09 Black;3.4;3 years;220;240;230;1450;n/a;I;https://www.simes.it/en/overview/167/zip-comfort;It has constantly evolved to achieve greater and more precise lighting control and high performance in terms of flux and efficiency. ZIP COMFORT is the right answer to the most difficult architectural challenges thanks to the availability of many different combinations.;https://www.simes.it/en/search/?q=7895;1;200;200;240;Inground;ZIP SQUARE WALKOVER  12°;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRZIPCOMF-IN2.pdf;IP65/IP67;IK 09;AC 50-60Hz / DC;A+;DALI2/PUSH;0;Electronic ballast;0.5m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_09_Black;Simes_Zip_Comfort_Square_Photometrics : S.8895H
S.7896N.09_ZIP_COMFORT_ASY_SQUARE_4000K_1250lm_16.6W_Black;S.7896N.09;0;4000;16.6;1250;09 Black;3.4;3 years;220;240;230;1660;n/a;I;https://www.simes.it/en/overview/167/zip-comfort;It has constantly evolved to achieve greater and more precise lighting control and high performance in terms of flux and efficiency. ZIP COMFORT is the right answer to the most difficult architectural challenges thanks to the availability of many different combinations.;https://www.simes.it/en/search/?q=7896;1;200;200;240;Inground;ZIP SQUARE WALKOVER ASY;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRZIPCOMF-IN2.pdf;IP65/IP67;IK 09;AC 50-60Hz / DC;A+;DALI2/PUSH;0;Electronic ballast;0.5m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_09_Black;Simes_Zip_Comfort_Square_Photometrics : S.8896N
S.7896W.09_ZIP_COMFORT_ASY_SQUARE_3000K_1188lm_16.6W_Black;S.7896W.09;0;3000;16.6;1188;09 Black;3.4;3 years;220;240;230;1520;n/a;I;https://www.simes.it/en/overview/167/zip-comfort;It has constantly evolved to achieve greater and more precise lighting control and high performance in terms of flux and efficiency. ZIP COMFORT is the right answer to the most difficult architectural challenges thanks to the availability of many different combinations.;https://www.simes.it/en/search/?q=7896;1;200;200;240;Inground;ZIP SQUARE WALKOVER  ASY;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRZIPCOMF-IN2.pdf;IP65/IP67;IK 09;AC 50-60Hz / DC;A+;DALI2/PUSH;0;Electronic ballast;0.5m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_09_Black;Simes_Zip_Comfort_Square_Photometrics : S.8896W
S.7896H.09_ZIP_COMFORT_ASY_SQUARE_2700K_1083lm_16.6W_Black;S.7896H.09;0;2700;16.6;1083;09 Black;3.4;3 years;220;240;230;1450;n/a;I;https://www.simes.it/en/overview/167/zip-comfort;It has constantly evolved to achieve greater and more precise lighting control and high performance in terms of flux and efficiency. ZIP COMFORT is the right answer to the most difficult architectural challenges thanks to the availability of many different combinations.;https://www.simes.it/en/search/?q=7896;1;200;200;240;Inground;ZIP SQUARE WALKOVER ASY;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRZIPCOMF-IN2.pdf;IP65/IP67;IK 09;AC 50-60Hz / DC;A+;DALI2/PUSH;0;Electronic ballast;0.5m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_09_Black;Simes_Zip_Comfort_Square_Photometrics : S.8896H
S.7897N.09_ZIP_COMFORT_33°_SQUARE_4000K_1023lm_15.2W_Black;S.7897N.09;25;4000;15.2;1023;09 Black;3.4;3 years;220;240;230;1544;n/a;I;https://www.simes.it/en/overview/167/zip-comfort;It has constantly evolved to achieve greater and more precise lighting control and high performance in terms of flux and efficiency. ZIP COMFORT is the right answer to the most difficult architectural challenges thanks to the availability of many different combinations.;https://www.simes.it/en/search/?q=7897;1;200;200;240;Inground;ZIP SQUARE WALKOVER  33°;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRZIPCOMF-IN2.pdf;IP65/IP67;IK 09;AC 50-60Hz / DC;A+;DALI2/PUSH;0;Electronic ballast;0.5m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_09_Black;Simes_Zip_Comfort_Square_Photometrics : S.8897N
S.7897W.09_ZIP_COMFORT_33°_SQUARE_3000K_973lm_15.2W_Black;S.7897W.09;25;3000;15.2;973;09 Black;3.4;3 years;220;240;230;1522;n/a;I;https://www.simes.it/en/overview/167/zip-comfort;It has constantly evolved to achieve greater and more precise lighting control and high performance in terms of flux and efficiency. ZIP COMFORT is the right answer to the most difficult architectural challenges thanks to the availability of many different combinations.;https://www.simes.it/en/search/?q=7897;1;200;200;240;Inground;ZIP SQUARE WALKOVER 33°;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRZIPCOMF-IN2.pdf;IP65/IP67;IK 09;AC 50-60Hz / DC;A+;DALI2/PUSH;0;Electronic ballast;0.5m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_09_Black;Simes_Zip_Comfort_Square_Photometrics : S.8897W
S.7897H.09_ZIP_COMFORT_33°_SQUARE_2700K_940lm_15.2W_Black;S.7897H.09;25;2700;15.2;940;09 Black;3.4;3 years;220;240;230;1449;n/a;I;https://www.simes.it/en/overview/167/zip-comfort;It has constantly evolved to achieve greater and more precise lighting control and high performance in terms of flux and efficiency. ZIP COMFORT is the right answer to the most difficult architectural challenges thanks to the availability of many different combinations.;https://www.simes.it/en/search/?q=7897;1;200;200;240;Inground;ZIP SQUARE WALKOVER 33°;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRZIPCOMF-IN2.pdf;IP65/IP67;IK 09;AC 50-60Hz / DC;A+;DALI2/PUSH;0;Electronic ballast;0.5m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_09_Black;Simes_Zip_Comfort_Square_Photometrics : S.8897H
