;SIMES_Product Code##OTHER##;SIMES_Beam Angle##ANGLE##DEGREES;SIMES_Color Temperature##COLOR_TEMPERATURE##KELVIN;SIMES_Rated Wattage##ELECTRICAL_POWER##WATTS;SIMES_Rated Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;SIMES_Finishes##OTHER##;SIMES_Weigth##MASS##KILOGRAMS;SIMES_Warranty Period##OTHER##;SIMES_Supply Voltage Min##ELECTRICAL_POTENTIAL##VOLTS;SIMES_Supply Voltage Max##ELECTRICAL_POTENTIAL##VOLTS;SIMES_Supply Voltage##ELECTRICAL_POTENTIAL##VOLTS;SIMES_Source Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;SIMES_Remote Power Supply##OTHER##;SIMES_Protection Class##OTHER##;SIMES_Product Page URL##OTHER##;SIMES_Product Description##OTHER##;SIMES_Product Data Sheet URL##OTHER##;SIMES_Number of Poles##OTHER##;SIMES_Nominal Width##LENGTH##MILLIMETERS;SIMES_Nominal Length##LENGTH##MILLIMETERS;SIMES_Nominal Height##LENGTH##MILLIMETERS;SIMES_Mounting Type##OTHER##;SIMES_Model##OTHER##;SIMES_Material Description##OTHER##;SIMES_Manufacturer Comment##OTHER##;SIMES_Luminous Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;SIMES_Light Source Type##OTHER##;SIMES_Lamp Count##OTHER##;SIMES_Installation Note URL##OTHER##;SIMES_IP Rating##OTHER##;SIMES_IK Rating##OTHER##;SIMES_Frequency##OTHER##;SIMES_Energy Efficiency Class##OTHER##;SIMES_Dimmable##OTHER##;SIMES_Current##ELECTRICAL_CURRENT##AMPERES;SIMES_Control Gear##OTHER##;SIMES_Cable Length##OTHER##;SIMES_CRI##OTHER##;SIMES_Approval Mark##OTHER##;LightFixturePlacingType##OTHER##;LightFixtureMountingType##OTHER##;Light Source##OTHER##;HasProtectiveEarth##OTHER##;Ground Stake##OTHER##;Body##OTHER##;Photometric_Type##OTHER##
L.9260H.01_SKILL SQUARE WOOD WALL_2700K_438lm_8.1W_White;L.9260H.01;0;2700;8.1;438;01 White;1.2;3 years;220;240;230;1319;n/a;I;https://www.simes.it/en/overview/126/skill-wood;Design Matteo Thun A non-recessed wall installation, SKILL WOOD represents a new concept of outdoor light fitting where aluminum is combined with the natural character of teak wood, assuring warmth and emotion. Eco sustainability, absence of glare and visual comfort make SKILL WOOD an extremely contemporary light fitting.;https://www.simes.it/en/search/?q=9260;1;33;200;200;Wall mounted;SKILL SQUARE WOOD WALL MOUNTED;Aluminium body + Teak;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRSKILL2.pdf;IP65;IK 08;AC 50-60Hz / DC;A+;Phase cut;0;Electronic ballast;0.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_01_White;Simes_Skill_Photometrics : L.9260H
L.9260H.20_SKILL SQUARE WOOD WALL_2700K_438lm_8.1W_Burnished bronze;L.9260H.20;0;2700;8.1;438;20 Burnished bronze;1.2;3 years;220;240;230;1319;n/a;I;https://www.simes.it/en/overview/126/skill-wood;Design Matteo Thun A non-recessed wall installation, SKILL WOOD represents a new concept of outdoor light fitting where aluminum is combined with the natural character of teak wood, assuring warmth and emotion. Eco sustainability, absence of glare and visual comfort make SKILL WOOD an extremely contemporary light fitting.;https://www.simes.it/en/search/?q=9260;1;33;200;200;Wall mounted;SKILL SQUARE WOOD WALL MOUNTED;Aluminium body + Teak;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRSKILL2.pdf;IP65;IK 08;AC 50-60Hz / DC;A+;Phase cut;0;Electronic ballast;0.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_20_Burnished bronze;Simes_Skill_Photometrics : L.9260H
L.9260N.01_SKILL SQUARE WOOD WALL_4000K_461lm_8.1W_White;L.9260N.01;0;4000;8.1;461;01 White;1.2;3 years;220;240;230;1764;n/a;I;https://www.simes.it/en/overview/126/skill-wood;Design Matteo Thun A non-recessed wall installation, SKILL WOOD represents a new concept of outdoor light fitting where aluminum is combined with the natural character of teak wood, assuring warmth and emotion. Eco sustainability, absence of glare and visual comfort make SKILL WOOD an extremely contemporary light fitting.;https://www.simes.it/en/search/?q=9260;1;33;200;200;Wall mounted;SKILL SQUARE WOOD WALL MOUNTED;Aluminium body + Teak;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRSKILL2.pdf;IP65;IK 08;AC 50-60Hz / DC;A+;Phase cut;0;Electronic ballast;0.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_01_White;Simes_Skill_Photometrics : L.9260N
L.9260N.20_SKILL SQUARE WOOD WALL_4000K_461lm_8.1W_Burnished bronze;L.9260N.20;0;4000;8.1;461;20 Burnished bronze;1.2;3 years;220;240;230;1764;n/a;I;https://www.simes.it/en/overview/126/skill-wood;Design Matteo Thun A non-recessed wall installation, SKILL WOOD represents a new concept of outdoor light fitting where aluminum is combined with the natural character of teak wood, assuring warmth and emotion. Eco sustainability, absence of glare and visual comfort make SKILL WOOD an extremely contemporary light fitting.;https://www.simes.it/en/search/?q=9260;1;33;200;200;Wall mounted;SKILL SQUARE WOOD WALL MOUNTED;Aluminium body + Teak;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRSKILL2.pdf;IP65;IK 08;AC 50-60Hz / DC;A+;Phase cut;0;Electronic ballast;0.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_20_Burnished bronze;Simes_Skill_Photometrics : L.9260N
L.9260W.01_SKILL SQUARE WOOD WALL_3000K_451lm_8.1W_White;L.9260W.01;0;3000;8.1;451;01 White;1.2;3 years;220;240;230;1357;n/a;I;https://www.simes.it/en/overview/126/skill-wood;Design Matteo Thun A non-recessed wall installation, SKILL WOOD represents a new concept of outdoor light fitting where aluminum is combined with the natural character of teak wood, assuring warmth and emotion. Eco sustainability, absence of glare and visual comfort make SKILL WOOD an extremely contemporary light fitting.;https://www.simes.it/en/search/?q=9260;1;33;200;200;Wall mounted;SKILL SQUARE WOOD WALL MOUNTED;Aluminium body + Teak;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRSKILL2.pdf;IP65;IK 08;AC 50-60Hz / DC;A+;Phase cut;0;Electronic ballast;0.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_01_White;Simes_Skill_Photometrics : L.9260W
L.9260W.20_SKILL SQUARE WOOD WALL_3000K_451lm_8.1W_Burnished bronze;L.9260W.20;0;3000;8.1;451;20 Burnished bronze;1.2;3 years;220;240;230;1357;n/a;I;https://www.simes.it/en/overview/126/skill-wood;Design Matteo Thun A non-recessed wall installation, SKILL WOOD represents a new concept of outdoor light fitting where aluminum is combined with the natural character of teak wood, assuring warmth and emotion. Eco sustainability, absence of glare and visual comfort make SKILL WOOD an extremely contemporary light fitting.;https://www.simes.it/en/search/?q=9260;1;33;200;200;Wall mounted;SKILL SQUARE WOOD WALL MOUNTED;Aluminium body + Teak;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRSKILL2.pdf;IP65;IK 08;AC 50-60Hz / DC;A+;Phase cut;0;Electronic ballast;0.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_20_Burnished bronze;Simes_Skill_Photometrics : L.9260W
