;SIMES_Product Code##OTHER##;SIMES_Beam Angle##ANGLE##DEGREES;SIMES_Color Temperature##COLOR_TEMPERATURE##KELVIN;SIMES_Rated Wattage##ELECTRICAL_POWER##WATTS;SIMES_Rated Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;SIMES_Finishes##OTHER##;SIMES_Weigth##MASS##KILOGRAMS;SIMES_Warranty Period##OTHER##;SIMES_Supply Voltage Min##ELECTRICAL_POTENTIAL##VOLTS;SIMES_Supply Voltage Max##ELECTRICAL_POTENTIAL##VOLTS;SIMES_Supply Voltage##ELECTRICAL_POTENTIAL##VOLTS;SIMES_Source Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;SIMES_Remote Power Supply##OTHER##;SIMES_Protection Class##OTHER##;SIMES_Product Page URL##OTHER##;SIMES_Product Description##OTHER##;SIMES_Product Data Sheet URL##OTHER##;SIMES_Number of Poles##OTHER##;SIMES_Nominal Width##LENGTH##MILLIMETERS;SIMES_Nominal Length##LENGTH##MILLIMETERS;SIMES_Nominal Height##LENGTH##MILLIMETERS;SIMES_Mounting Type##OTHER##;SIMES_Model##OTHER##;SIMES_Material Description##OTHER##;SIMES_Manufacturer Comment##OTHER##;SIMES_Luminous Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;SIMES_Light Source Type##OTHER##;SIMES_Lamp Count##OTHER##;SIMES_Installation Note URL##OTHER##;SIMES_IP Rating##OTHER##;SIMES_IK Rating##OTHER##;SIMES_Frequency##OTHER##;SIMES_Energy Efficiency Class##OTHER##;SIMES_Dimmable##OTHER##;SIMES_Current##ELECTRICAL_CURRENT##AMPERES;SIMES_Control Gear##OTHER##;SIMES_Cable Length##OTHER##;SIMES_CRI##OTHER##;SIMES_Approval Mark##OTHER##;LightFixturePlacingType##OTHER##;LightFixtureMountingType##OTHER##;Light Source##OTHER##;HasProtectiveEarth##OTHER##;Ground Stake##OTHER##;Body##OTHER##;Photometric_Type##OTHER##
S.6160H.09_MOAI_2700K_1460lm_33.9W_H1150_Black;S.6160H.09;0;2700;33.9;1460;09 Black;11.9;3 years;220;240;230;3574;n/a;II;https://www.simes.it/en/overview/60/moai;MOAI is a bollard with a strong personality and design.;https://www.simes.it/en/search/?q=6160;1;180;180;1150;Ground;MOAI BOLLARD H1150;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRMOAI2.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;DALI2/PUSH;0;Electronic ballast;0.4m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_09_Black;SIMES_Moai_Bollard_Photometrics : S.6160H
S.6160H.14_MOAI_2700K_1460lm_33.9W_H1150_Aluminium grey;S.6160H.14;0;2700;33.9;1460;14 Aluminium Grey;11.9;3 years;220;240;230;3574;n/a;II;https://www.simes.it/en/overview/60/moai;MOAI is a bollard with a strong personality and design.;https://www.simes.it/en/search/?q=6160;1;180;180;1150;Ground;MOAI BOLLARD H1150;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRMOAI2.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;DALI2/PUSH;0;Electronic ballast;0.4m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;SIMES_Moai_Bollard_Photometrics : S.6160H
S.6160H.20_MOAI_2700K_1460lm_33.9W_H1150_Burnished bronze_###PHASE-OUT###;S.6160H.20;0;2700;33.9;1460;20 Burnished bronze;11.9;3 years;220;240;230;3574;n/a;II;https://www.simes.it/en/overview/60/moai;MOAI is a bollard with a strong personality and design.;https://www.simes.it/en/search/?q=6160;1;180;180;1150;Ground;MOAI BOLLARD H1150;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRMOAI2.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;DALI2/PUSH;0;Electronic ballast;0.4m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_20_Burnished bronze;SIMES_Moai_Bollard_Photometrics : S.6160H
S.6160W.09_MOAI_3000K_1538lm_33.9W_H1150_Black;S.6160W.09;0;3000;33.9;1538;09 Black;11.9;3 years;220;240;230;3763;n/a;II;https://www.simes.it/en/overview/60/moai;MOAI is a bollard with a strong personality and design.;https://www.simes.it/en/search/?q=6160;1;180;180;1150;Ground;MOAI BOLLARD H1150;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRMOAI2.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;DALI2/PUSH;0;Electronic ballast;0.4m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_09_Black;SIMES_Moai_Bollard_Photometrics : S.6160W
S.6160W.14_MOAI_3000K_1538lm_33.9W_H1150_Aluminium grey;S.6160W.14;0;3000;33.9;1538;14 Aluminium Grey;11.9;3 years;220;240;230;3763;n/a;II;https://www.simes.it/en/overview/60/moai;MOAI is a bollard with a strong personality and design.;https://www.simes.it/en/search/?q=6160;1;180;180;1150;Ground;MOAI BOLLARD H1150;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRMOAI2.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;DALI2/PUSH;0;Electronic ballast;0.4m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;SIMES_Moai_Bollard_Photometrics : S.6160W
S.6160W.20_MOAI_3000K_1538lm_33.9W_H1150_Burnished bronze_###PHASE-OUT###;S.6160W.20;0;3000;33.9;1538;20 Burnished bronze;11.9;3 years;220;240;230;3763;n/a;II;https://www.simes.it/en/overview/60/moai;MOAI is a bollard with a strong personality and design.;https://www.simes.it/en/search/?q=6160;1;180;180;1150;Ground;MOAI BOLLARD H1150;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRMOAI2.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;DALI2/PUSH;0;Electronic ballast;0.4m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_20_Burnished bronze;SIMES_Moai_Bollard_Photometrics : S.6160W
S.6160N.09_MOAI_4000K_1875lm_33.9W_H1150_Black;S.6160N.09;0;4000;33.9;1875;09 Black;11.9;3 years;220;240;230;3875;n/a;II;https://www.simes.it/en/overview/60/moai;MOAI is a bollard with a strong personality and design.;https://www.simes.it/en/search/?q=6160;1;180;180;1150;Ground;MOAI BOLLARD H1150;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRMOAI2.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;DALI2/PUSH;0;Electronic ballast;0.4m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_09_Black;SIMES_Moai_Bollard_Photometrics : S.6160N
S.6160N.14_MOAI_4000K_1875lm_33.9W_H1150_Aluminium grey;S.6160N.14;0;4000;33.9;1875;14 Aluminium Grey;11.9;3 years;220;240;230;3875;n/a;II;https://www.simes.it/en/overview/60/moai;MOAI is a bollard with a strong personality and design.;https://www.simes.it/en/search/?q=6160;1;180;180;1150;Ground;MOAI BOLLARD H1150;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRMOAI2.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;DALI2/PUSH;0;Electronic ballast;0.4m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;SIMES_Moai_Bollard_Photometrics : S.6160N
S.6160N.20_MOAI_4000K_1875lm_33.9W_H1150_Burnished bronze_###PHASE-OUT###;S.6160N.20;0;4000;33.9;1875;20 Burnished bronze;11.9;3 years;220;240;230;3875;n/a;II;https://www.simes.it/en/overview/60/moai;MOAI is a bollard with a strong personality and design.;https://www.simes.it/en/search/?q=6160;1;180;180;1150;Ground;MOAI BOLLARD H1150;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRMOAI2.pdf;IP65;IK 06;AC 50-60Hz / DC;A+;DALI2/PUSH;0;Electronic ballast;0.4m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_20_Burnished bronze;SIMES_Moai_Bollard_Photometrics : S.6160N
