 ;SIMES_Product Code##OTHER##;SIMES_Beam Angle##ANGLE##DEGREES;SIMES_Color Temperature##COLOR_TEMPERATURE##KELVIN;SIMES_Rated Wattage##ELECTRICAL_POWER##WATTS;SIMES_Rated Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;SIMES_Finishes##OTHER##;SIMES_Weigth##MASS##KILOGRAMS;SIMES_Warranty Period##OTHER##;SIMES_Supply Voltage Min##ELECTRICAL_POTENTIAL##VOLTS;SIMES_Supply Voltage Max##ELECTRICAL_POTENTIAL##VOLTS;SIMES_Supply Voltage##ELECTRICAL_POTENTIAL##VOLTS;SIMES_Source Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;SIMES_Remote Power Supply##OTHER##;SIMES_Protection Class##OTHER##;SIMES_Product Page URL##OTHER##;SIMES_Product Description##OTHER##;SIMES_Product Data Sheet URL##OTHER##;SIMES_Number of Poles##OTHER##;SIMES_Nominal Width##LENGTH##MILLIMETERS;SIMES_Nominal Length##LENGTH##MILLIMETERS;SIMES_Nominal Height##LENGTH##MILLIMETERS;SIMES_Mounting Type##OTHER##;SIMES_Model##OTHER##;SIMES_Material Description##OTHER##;SIMES_Manufacturer Comment##OTHER##;SIMES_Luminous Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;SIMES_Light Source Type##OTHER##;SIMES_Lamp Count##OTHER##;SIMES_Installation Note URL##OTHER##;SIMES_IP Rating##OTHER##;SIMES_IK Rating##OTHER##;SIMES_Frequency##OTHER##;SIMES_Energy Efficiency Class##OTHER##;SIMES_Dimmable##OTHER##;SIMES_Current##ELECTRICAL_CURRENT##AMPERES;SIMES_Control Gear##OTHER##;SIMES_Cable Length##OTHER##;SIMES_CRI##OTHER##;SIMES_Approval Mark##OTHER##;LightFixturePlacingType##OTHER##;LightFixtureMountingType##OTHER##;Light Source##OTHER##;HasProtectiveEarth##OTHER##;Ground Stake##OTHER##;Body##OTHER##;Photometric_Type##OTHER##
S.1810N.01_PETIT_4000K_598lm_14.5W_White;S.1810N.01;0;4000;14.5;598;01 White;1.2;3 years;220;240;230;1384;n/a;I;https://www.simes.it/en/overview/182/petit-applique;Petit applique is conceived to design a precise light effect on the vertical surface.;https://www.simes.it/en/search/?q=1810;1;71;102;145;Applique;PETIT APPLIQUE;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRPETIT.pdf;IP65;IK 07;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;5.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_01_White;Simes_Petit_Photometrics : S.1810N
S.1810N.14_PETIT_4000K_598lm_14.5W_Aluminium grey;S.1810N.14;0;4000;14.5;598;14 Aluminium Grey;1.2;3 years;220;240;230;1384;n/a;I;https://www.simes.it/en/overview/182/petit-applique;Petit applique is conceived to design a precise light effect on the vertical surface.;https://www.simes.it/en/search/?q=1810;1;71;102;145;Applique;PETIT APPLIQUE;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRPETIT.pdf;IP65;IK 07;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;5.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Petit_Photometrics : S.1810N
S.1810N.24_PETIT_4000K_598lm_14.5W_Antracyte grey;S.1810N.24;0;4000;14.5;598;24 Anthracite Grey;1.2;3 years;220;240;230;1384;n/a;I;https://www.simes.it/en/overview/182/petit-applique;Petit applique is conceived to design a precise light effect on the vertical surface.;https://www.simes.it/en/search/?q=1810;1;71;102;145;Applique;PETIT APPLIQUE;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRPETIT.pdf;IP65;IK 07;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;5.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_24_Anthracyte grey;Simes_Petit_Photometrics : S.1810N
S.1810H.01_PETIT_2700K_528lm_14.5W_White;S.1810H.01;0;2700;14.5;528;01 White;1.2;3 years;220;240;230;1225;n/a;I;https://www.simes.it/en/overview/182/petit-applique;Petit applique is conceived to design a precise light effect on the vertical surface.;https://www.simes.it/en/search/?q=1810;1;71;102;145;Applique;PETIT APPLIQUE;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRPETIT.pdf;IP65;IK 07;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;5.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_01_White;Simes_Petit_Photometrics : S.1810H
S.1810H.14_PETIT_2700K_528lm_14.5W_Aluminium grey;S.1810H.14;0;2700;14.5;528;14 Aluminium Grey;1.2;3 years;220;240;230;1225;n/a;I;https://www.simes.it/en/overview/182/petit-applique;Petit applique is conceived to design a precise light effect on the vertical surface.;https://www.simes.it/en/search/?q=1810;1;71;102;145;Applique;PETIT APPLIQUE;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRPETIT.pdf;IP65;IK 07;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;5.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Petit_Photometrics : S.1810H
S.1810H.24_PETIT_2700K_528lm_14.5W_Antracyte grey;S.1810H.24;0;2700;14.5;528;24 Anthracite Grey;1.2;3 years;220;240;230;1225;n/a;I;https://www.simes.it/en/overview/182/petit-applique;Petit applique is conceived to design a precise light effect on the vertical surface.;https://www.simes.it/en/search/?q=1810;1;71;102;145;Applique;PETIT APPLIQUE;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRPETIT.pdf;IP65;IK 07;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;5.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_24_Anthracyte grey;Simes_Petit_Photometrics : S.1810H
S.1810W.01_PETIT_3000K_568lm_14.5W_White;S.1810W.01;0;3000;14.5;568;01 White;1.2;3 years;220;240;230;1290;n/a;I;https://www.simes.it/en/overview/182/petit-applique;Petit applique is conceived to design a precise light effect on the vertical surface.;https://www.simes.it/en/search/?q=1810;1;71;102;145;Applique;PETIT APPLIQUE;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRPETIT.pdf;IP65;IK 07;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;5.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_01_White;Simes_Petit_Photometrics : S.1810W
S.1810W.14_PETIT_3000K_568lm_14.5W_Aluminium grey;S.1810W.14;0;3000;14.5;568;14 Aluminium Grey;1.2;3 years;220;240;230;1290;n/a;I;https://www.simes.it/en/overview/182/petit-applique;Petit applique is conceived to design a precise light effect on the vertical surface.;https://www.simes.it/en/search/?q=1810;1;71;102;145;Applique;PETIT APPLIQUE;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRPETIT.pdf;IP65;IK 07;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;5.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Petit_Photometrics : S.1810W
S.1810W.24_PETIT_3000K_568lm_14.5W_Antracyte grey;S.1810W.24;0;3000;14.5;568;24 Anthracite Grey;1.2;3 years;220;240;230;1290;n/a;I;https://www.simes.it/en/overview/182/petit-applique;Petit applique is conceived to design a precise light effect on the vertical surface.;https://www.simes.it/en/search/?q=1810;1;71;102;145;Applique;PETIT APPLIQUE;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRPETIT.pdf;IP65;IK 07;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;5.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_24_Anthracyte grey;Simes_Petit_Photometrics : S.1810W
