;SIMES_Product Code##OTHER##;SIMES_Beam Angle##ANGLE##DEGREES;SIMES_Color Temperature##COLOR_TEMPERATURE##KELVIN;SIMES_Rated Wattage##ELECTRICAL_POWER##WATTS;SIMES_Rated Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;SIMES_Finishes##OTHER##;SIMES_Weigth##MASS##KILOGRAMS;SIMES_Warranty Period##OTHER##;SIMES_Supply Voltage Min##ELECTRICAL_POTENTIAL##VOLTS;SIMES_Supply Voltage Max##ELECTRICAL_POTENTIAL##VOLTS;SIMES_Supply Voltage##ELECTRICAL_POTENTIAL##VOLTS;SIMES_Source Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;SIMES_Remote Power Supply##OTHER##;SIMES_Protection Class##OTHER##;SIMES_Product Page URL##OTHER##;SIMES_Product Description##OTHER##;SIMES_Product Data Sheet URL##OTHER##;SIMES_Number of Poles##OTHER##;SIMES_Nominal Width##LENGTH##MILLIMETERS;SIMES_Nominal Length##LENGTH##MILLIMETERS;SIMES_Nominal Height##LENGTH##MILLIMETERS;SIMES_Mounting Type##OTHER##;SIMES_Model##OTHER##;SIMES_Material Description##OTHER##;SIMES_Manufacturer Comment##OTHER##;SIMES_Luminous Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;SIMES_Light Source Type##OTHER##;SIMES_Lamp Count##OTHER##;SIMES_Installation Note URL##OTHER##;SIMES_IP Rating##OTHER##;SIMES_IK Rating##OTHER##;SIMES_Frequency##OTHER##;SIMES_Energy Efficiency Class##OTHER##;SIMES_Dimmable##OTHER##;SIMES_Current##ELECTRICAL_CURRENT##AMPERES;SIMES_Control Gear##OTHER##;SIMES_Cable Length##OTHER##;SIMES_CRI##OTHER##;SIMES_Approval Mark##OTHER##;LightFixturePlacingType##OTHER##;LightFixtureMountingType##OTHER##;Light Source##OTHER##;HasProtectiveEarth##OTHER##;Ground Stake##OTHER##;Body##OTHER##;Photometric_Type##OTHER##
S.5339H.14_CUBIKS_2700K_1453lm_40W_H800_Aluminium grey;S.5339H.14;0;2700;40;1453;14 Aluminium Grey;10.7;3 years;220;240;230;4275;n/a;II;https://www.simes.it/en/overview/61/cubiks;CUBIKS is a range of bollards with a minimalistic and clean-cut design, suitable for the illumination of areas in modern urban context.;https://www.simes.it/en/search/?q=5339;1;180;180;800;Ground;CUBIKS BOLLARD H800;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRCUBIKS2.pdf;IP66;IK 10;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;0.4m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;SIMES_Cubiks_Bollard_Photometrics : S.5339H
S.5339H.24_CUBIKS_2700K_1453lm_40W_H800_Anthacite grey;S.5339H.24;0;2700;40;1453;24 Anthracite Grey;10.7;3 years;220;240;230;4275;n/a;II;https://www.simes.it/en/overview/61/cubiks;CUBIKS is a range of bollards with a minimalistic and clean-cut design, suitable for the illumination of areas in modern urban context.;https://www.simes.it/en/search/?q=5339;1;180;180;800;Ground;CUBIKS BOLLARD H800;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRCUBIKS2.pdf;IP66;IK 10;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;0.4m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_24_Anthracyte grey;SIMES_Cubiks_Bollard_Photometrics : S.5339H
S.5339W.14_CUBIKS_3000K_1530lm_40W_H800_Aluminium grey;S.5339W.14;0;3000;40;1530;14 Aluminium Grey;10.7;3 years;220;240;230;4500;n/a;II;https://www.simes.it/en/overview/61/cubiks;CUBIKS is a range of bollards with a minimalistic and clean-cut design, suitable for the illumination of areas in modern urban context.;https://www.simes.it/en/search/?q=5339;1;180;180;800;Ground;CUBIKS BOLLARD H800;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRCUBIKS2.pdf;IP66;IK 10;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;0.4m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;SIMES_Cubiks_Bollard_Photometrics : S.5339W
S.5339W.24_CUBIKS_3000K_1530lm_40W_H800_Anthacite grey;S.5339W.24;0;3000;40;1530;24 Anthracite Grey;10.7;3 years;220;240;230;4500;n/a;II;https://www.simes.it/en/overview/61/cubiks;CUBIKS is a range of bollards with a minimalistic and clean-cut design, suitable for the illumination of areas in modern urban context.;https://www.simes.it/en/search/?q=5339;1;180;180;800;Ground;CUBIKS BOLLARD H800;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRCUBIKS2.pdf;IP66;IK 10;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;0.4m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_24_Anthracyte grey;SIMES_Cubiks_Bollard_Photometrics : S.5339W
S.5339N.14_CUBIKS_4000K_1915lm_40W_H800_Aluminium grey;S.5339N.14;0;4000;40;1915;14 Aluminium Grey;10.7;3 years;220;240;230;4635;n/a;II;https://www.simes.it/en/overview/61/cubiks;CUBIKS is a range of bollards with a minimalistic and clean-cut design, suitable for the illumination of areas in modern urban context.;https://www.simes.it/en/search/?q=5339;1;180;180;800;Ground;CUBIKS BOLLARD H800;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRCUBIKS2.pdf;IP66;IK 10;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;0.4m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;SIMES_Cubiks_Bollard_Photometrics : S.5339N
S.5339N.24_CUBIKS_4000K_1915lm_40W_H800_Anthacite grey;S.5339N.24;0;4000;40;1915;24 Anthracite Grey;10.7;3 years;220;240;230;4635;n/a;II;https://www.simes.it/en/overview/61/cubiks;CUBIKS is a range of bollards with a minimalistic and clean-cut design, suitable for the illumination of areas in modern urban context.;https://www.simes.it/en/search/?q=5339;1;180;180;800;Ground;CUBIKS BOLLARD H800;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRCUBIKS2.pdf;IP66;IK 10;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;0.4m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;0;SIMES_Black_Polipropilene;SIMES_24_Anthracyte grey;SIMES_Cubiks_Bollard_Photometrics : S.5339N
