;SIMES_Product Code##OTHER##;SIMES_Beam Angle##ANGLE##DEGREES;SIMES_Color Temperature##COLOR_TEMPERATURE##KELVIN;SIMES_Rated Wattage##ELECTRICAL_POWER##WATTS;SIMES_Rated Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;SIMES_Finishes##OTHER##;SIMES_Weigth##MASS##KILOGRAMS;SIMES_Warranty Period##OTHER##;SIMES_Supply Voltage Min##ELECTRICAL_POTENTIAL##VOLTS;SIMES_Supply Voltage Max##ELECTRICAL_POTENTIAL##VOLTS;SIMES_Supply Voltage##ELECTRICAL_POTENTIAL##VOLTS;SIMES_Source Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;SIMES_Remote Power Supply##OTHER##;SIMES_Protection Class##OTHER##;SIMES_Product Page URL##OTHER##;SIMES_Product Description##OTHER##;SIMES_Product Data Sheet URL##OTHER##;SIMES_Number of Poles##OTHER##;SIMES_Nominal Width##LENGTH##MILLIMETERS;SIMES_Nominal Length##LENGTH##MILLIMETERS;SIMES_Nominal Height##LENGTH##MILLIMETERS;SIMES_Mounting Type##OTHER##;SIMES_Model##OTHER##;SIMES_Material Description##OTHER##;SIMES_Manufacturer Comment##OTHER##;SIMES_Luminous Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;SIMES_Light Source Type##OTHER##;SIMES_Lamp Count##OTHER##;SIMES_Installation Note URL##OTHER##;SIMES_IP Rating##OTHER##;SIMES_IK Rating##OTHER##;SIMES_Frequency##OTHER##;SIMES_Energy Efficiency Class##OTHER##;SIMES_Dimmable##OTHER##;SIMES_Current##ELECTRICAL_CURRENT##AMPERES;SIMES_Control Gear##OTHER##;SIMES_Cable Length##OTHER##;SIMES_CRI##OTHER##;SIMES_Approval Mark##OTHER##;LightFixturePlacingType##OTHER##;LightFixtureMountingType##OTHER##;Light Source##OTHER##;HasProtectiveEarth##OTHER##;Ground Stake##OTHER##;Body##OTHER##;Photometric_Type##OTHER##
L.9230H.01_MINISKILL VERTICAL WOOD WALL_2700K_129lm_4.7W_White;L.9230H.01;0;2700;4.7;129;01 White;0.5;3 years;24;24;24;402;need remote power supply type S.3400 230V/24V DC 10W;III;https://www.simes.it/en/overview/126/skill-wood;Design Matteo Thun A non-recessed wall installation, SKILL WOOD represents a new concept of outdoor light fitting where aluminum is combined with the natural character of teak wood, assuring warmth and emotion. Eco sustainability, absence of glare and visual comfort make SKILL WOOD an extremely contemporary light fitting.;https://www.simes.it/en/search/?q=9230;1;31;60;115;Wall mounted;MINISKILL VERTICAL WOOD WALL MOUNTED;Aluminium body + Teak;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRMSKILL2.pdf;IP65;IK 08;DC;A+;yes;0;n/a;1.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_01_White;Simes_Skill_Photometrics : L.9230H
L.9230H.20_MINISKILL VERTICAL WOOD WALL_2700K_129lm_4.7W_Burnished bronze;L.9230H.20;0;2700;4.7;129;20 Burnished bronze;0.5;3 years;24;24;24;402;need remote power supply type S.3400 230V/24V DC 10W;III;https://www.simes.it/en/overview/126/skill-wood;Design Matteo Thun A non-recessed wall installation, SKILL WOOD represents a new concept of outdoor light fitting where aluminum is combined with the natural character of teak wood, assuring warmth and emotion. Eco sustainability, absence of glare and visual comfort make SKILL WOOD an extremely contemporary light fitting.;https://www.simes.it/en/search/?q=9230;1;31;60;115;Wall mounted;MINISKILL VERTICAL WOOD WALL MOUNTED;Aluminium body + Teak;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRMSKILL2.pdf;IP65;IK 08;DC;A+;yes;0;n/a;1.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_20_Burnished bronze;Simes_Skill_Photometrics : L.9230H
L.9230N.01_MINISKILL VERTICAL WOOD WALL_4000K_133lm_4.7W_White;L.9230N.01;0;4000;4.7;133;01 White;0.5;3 years;24;24;24;505;need remote power supply type S.3400 230V/24V DC 10W;III;https://www.simes.it/en/overview/126/skill-wood;Design Matteo Thun A non-recessed wall installation, SKILL WOOD represents a new concept of outdoor light fitting where aluminum is combined with the natural character of teak wood, assuring warmth and emotion. Eco sustainability, absence of glare and visual comfort make SKILL WOOD an extremely contemporary light fitting.;https://www.simes.it/en/search/?q=9230;1;31;60;115;Wall mounted;MINISKILL VERTICAL WOOD WALL MOUNTED;Aluminium body + Teak;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRMSKILL2.pdf;IP65;IK 08;DC;A+;yes;0;n/a;1.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_01_White;Simes_Skill_Photometrics : L.9230N
L.9230N.20_MINISKILL VERTICAL WOOD WALL_4000K_133lm_4.7W_Burnished bronze;L.9230N.20;0;4000;4.7;133;20 Burnished bronze;0.5;3 years;24;24;24;505;need remote power supply type S.3400 230V/24V DC 10W;III;https://www.simes.it/en/overview/126/skill-wood;Design Matteo Thun A non-recessed wall installation, SKILL WOOD represents a new concept of outdoor light fitting where aluminum is combined with the natural character of teak wood, assuring warmth and emotion. Eco sustainability, absence of glare and visual comfort make SKILL WOOD an extremely contemporary light fitting.;https://www.simes.it/en/search/?q=9230;1;31;60;115;Wall mounted;MINISKILL VERTICAL WOOD WALL MOUNTED;Aluminium body + Teak;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRMSKILL2.pdf;IP65;IK 08;DC;A+;yes;0;n/a;1.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_20_Burnished bronze;Simes_Skill_Photometrics : L.9230N
L.9230W.01_MINISKILL VERTICAL WOOD WALL_3000K_136lm_4.7W_White;L.9230W.01;0;3000;4.7;136;01 White;0.5;3 years;24;24;24;424;need remote power supply type S.3400 230V/24V DC 10W;III;https://www.simes.it/en/overview/126/skill-wood;Design Matteo Thun A non-recessed wall installation, SKILL WOOD represents a new concept of outdoor light fitting where aluminum is combined with the natural character of teak wood, assuring warmth and emotion. Eco sustainability, absence of glare and visual comfort make SKILL WOOD an extremely contemporary light fitting.;https://www.simes.it/en/search/?q=9230;1;31;60;115;Wall mounted;MINISKILL VERTICAL WOOD WALL MOUNTED;Aluminium body + Teak;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRMSKILL2.pdf;IP65;IK 08;DC;A+;yes;0;n/a;1.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_01_White;Simes_Skill_Photometrics : L.9230W
L.9230W.20_MINISKILL VERTICAL WOOD WALL_3000K_136lm_4.7W_Burnished bronze;L.9230W.20;0;3000;4.7;136;20 Burnished bronze;0.5;3 years;24;24;24;424;need remote power supply type S.3400 230V/24V DC 10W;III;https://www.simes.it/en/overview/126/skill-wood;Design Matteo Thun A non-recessed wall installation, SKILL WOOD represents a new concept of outdoor light fitting where aluminum is combined with the natural character of teak wood, assuring warmth and emotion. Eco sustainability, absence of glare and visual comfort make SKILL WOOD an extremely contemporary light fitting.;https://www.simes.it/en/search/?q=9230;1;31;60;115;Wall mounted;MINISKILL VERTICAL WOOD WALL MOUNTED;Aluminium body + Teak;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRMSKILL2.pdf;IP65;IK 08;DC;A+;yes;0;n/a;1.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_20_Burnished bronze;Simes_Skill_Photometrics : L.9230W
