;SIMES_Product Code##OTHER##;SIMES_Beam Angle##ANGLE##DEGREES;SIMES_Color Temperature##COLOR_TEMPERATURE##KELVIN;SIMES_Rated Wattage##ELECTRICAL_POWER##WATTS;SIMES_Rated Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;SIMES_Finishes##OTHER##;SIMES_Weigth##MASS##KILOGRAMS;SIMES_Warranty Period##OTHER##;SIMES_Supply Voltage Min##ELECTRICAL_POTENTIAL##VOLTS;SIMES_Supply Voltage Max##ELECTRICAL_POTENTIAL##VOLTS;SIMES_Supply Voltage##ELECTRICAL_POTENTIAL##VOLTS;SIMES_Source Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;SIMES_Remote Power Supply##OTHER##;SIMES_Protection Class##OTHER##;SIMES_Product Page URL##OTHER##;SIMES_Product Description##OTHER##;SIMES_Product Data Sheet URL##OTHER##;SIMES_Number of Poles##OTHER##;SIMES_Nominal Width##LENGTH##MILLIMETERS;SIMES_Nominal Length##LENGTH##MILLIMETERS;SIMES_Nominal Height##LENGTH##MILLIMETERS;SIMES_Mounting Type##OTHER##;SIMES_Model##OTHER##;SIMES_Material Description##OTHER##;SIMES_Manufacturer Comment##OTHER##;SIMES_Luminous Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;SIMES_Light Source Type##OTHER##;SIMES_Lamp Count##OTHER##;SIMES_Installation Note URL##OTHER##;SIMES_IP Rating##OTHER##;SIMES_IK Rating##OTHER##;SIMES_Frequency##OTHER##;SIMES_Energy Efficiency Class##OTHER##;SIMES_Dimmable##OTHER##;SIMES_Current##ELECTRICAL_CURRENT##AMPERES;SIMES_Control Gear##OTHER##;SIMES_Cable Length##OTHER##;SIMES_CRI##OTHER##;SIMES_Approval Mark##OTHER##;LightFixturePlacingType##OTHER##;LightFixtureMountingType##OTHER##;Light Source##OTHER##;HasProtectiveEarth##OTHER##;Ground Stake##OTHER##;Body##OTHER##;Photometric_Type##OTHER##
S.8805N.19_MINIZIP_COMFORT_ACIDETCHEDGLASS_ROUND_4000K_33lm_3W_Stainless Steel;S.8805N.19;81;4000;3;33;19 Stainless Steel;1.1;3 years;220;240;230;150;n/a;I;https://www.simes.it/en/overview/167/zip-comfort;It has constantly evolved to achieve greater and more precise lighting control and high performance in terms of flux and efficiency. ZIP COMFORT is the right answer to the most difficult architectural challenges thanks to the availability of many different combinations.;https://www.simes.it/en/search/?q=8805;1;130;130;135;Inground;MINIZIP ROUND WALKOVER STAINLESS STEEL ACID-ETCHED GLASS;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRZIPCOMF-IN2.pdf;IP65/IP67;IK 09;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;0.5m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_19_Stainless Steel;Simes_Zip_Comfort_Round_Photometrics : S.8805N
S.8805W.19_MINIZIP_COMFORT_ACIDETCHEDGLASS_ROUND_3000K_32lm_3W_Stainless Steel;S.8805W.19;81;3000;3;32;19 Stainless Steel;1.1;3 years;220;240;230;140;n/a;I;https://www.simes.it/en/overview/167/zip-comfort;It has constantly evolved to achieve greater and more precise lighting control and high performance in terms of flux and efficiency. ZIP COMFORT is the right answer to the most difficult architectural challenges thanks to the availability of many different combinations.;https://www.simes.it/en/search/?q=8805;1;130;130;135;Inground;MINIZIP ROUND WALKOVER STAINLESS STEEL ACID-ETCHED GLASS;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRZIPCOMF-IN2.pdf;IP65/IP67;IK 09;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;0.5m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_19_Stainless Steel;Simes_Zip_Comfort_Round_Photometrics : S.8805W
S.8805H.19_MINIZIP_COMFORT_ACIDETCHEDGLASS_ROUND_2700K_31lm_3W_Stainless Steel;S.8805H.19;81;2700;3;31;19 Stainless Steel;1.1;3 years;220;240;230;130;n/a;I;https://www.simes.it/en/overview/167/zip-comfort;It has constantly evolved to achieve greater and more precise lighting control and high performance in terms of flux and efficiency. ZIP COMFORT is the right answer to the most difficult architectural challenges thanks to the availability of many different combinations.;https://www.simes.it/en/search/?q=8805;1;130;130;135;Inground;MINIZIP ROUND WALKOVER STAINLESS STEEL ACID-ETCHED GLASS;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRZIPCOMF-IN2.pdf;IP65/IP67;IK 09;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;0.5m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_19_Stainless Steel;Simes_Zip_Comfort_Round_Photometrics : S.8805H
S.8831N.19_MINIZIP_COMFORT_11°_ROUND_4000K_343lm_5.6W_Stainless Steel;S.8831N.19;11;4000;5.6;343;19 Stainless Steel;1.1;3 years;220;240;230;604;n/a;I;https://www.simes.it/en/overview/167/zip-comfort;It has constantly evolved to achieve greater and more precise lighting control and high performance in terms of flux and efficiency. ZIP COMFORT is the right answer to the most difficult architectural challenges thanks to the availability of many different combinations.;https://www.simes.it/en/search/?q=8831;1;130;130;135;Inground;MINIZIP ROUND WALKOVER STAINLESS STEEL 12°;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRZIPCOMF-IN2.pdf;IP65/IP67;IK 09;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;0.5m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_19_Stainless Steel;Simes_Zip_Comfort_Round_Photometrics : S.8831N
S.8831W.19_MINIZIP_COMFORT_11°_ROUND_3000K_306lm_5.6W_Stainless Steel;S.8831W.19;11;3000;5.6;306;19 Stainless Steel;1.1;3 years;220;240;230;552;n/a;I;https://www.simes.it/en/overview/167/zip-comfort;It has constantly evolved to achieve greater and more precise lighting control and high performance in terms of flux and efficiency. ZIP COMFORT is the right answer to the most difficult architectural challenges thanks to the availability of many different combinations.;https://www.simes.it/en/search/?q=8831;1;130;130;135;Inground;MINIZIP ROUND WALKOVER STAINLESS STEEL 12°;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRZIPCOMF-IN2.pdf;IP65/IP67;IK 09;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;0.5m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_19_Stainless Steel;Simes_Zip_Comfort_Round_Photometrics : S.8831W
S.8831H.19_MINIZIP_COMFORT_11°_ROUND_2700K_283lm_5.6W_Stainless Steel;S.8831H.19;11;2700;5.6;283;19 Stainless Steel;1.1;3 years;220;240;230;527;n/a;I;https://www.simes.it/en/overview/167/zip-comfort;It has constantly evolved to achieve greater and more precise lighting control and high performance in terms of flux and efficiency. ZIP COMFORT is the right answer to the most difficult architectural challenges thanks to the availability of many different combinations.;https://www.simes.it/en/search/?q=8831;1;130;130;135;Inground;MINIZIP ROUND WALKOVER STAINLESS STEEL 12°;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRZIPCOMF-IN2.pdf;IP65/IP67;IK 09;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;0.5m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_19_Stainless Steel;Simes_Zip_Comfort_Round_Photometrics : S.8831H
S.8832N.19_MINIZIP_COMFORT_ASY_ROUND_4000K_358lm_5.6W_Stainless Steel;S.8832N.19;0;4000;5.6;358;19 Stainless Steel;1.1;3 years;220;240;230;604;n/a;I;https://www.simes.it/en/overview/167/zip-comfort;It has constantly evolved to achieve greater and more precise lighting control and high performance in terms of flux and efficiency. ZIP COMFORT is the right answer to the most difficult architectural challenges thanks to the availability of many different combinations.;https://www.simes.it/en/search/?q=8832;1;130;130;135;Inground;MINIZIP ROUND WALKOVER STAINLESS STEEL ASY;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRZIPCOMF-IN2.pdf;IP65/IP67;IK 09;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;0.5m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_19_Stainless Steel;Simes_Zip_Comfort_Round_Photometrics : S.8832N
S.8832W.19_MINIZIP_COMFORT_ASY_ROUND_3000K_306lm_5.6W_Stainless Steel;S.8832W.19;0;3000;5.6;306;19 Stainless Steel;1.1;3 years;220;240;230;552;n/a;I;https://www.simes.it/en/overview/167/zip-comfort;It has constantly evolved to achieve greater and more precise lighting control and high performance in terms of flux and efficiency. ZIP COMFORT is the right answer to the most difficult architectural challenges thanks to the availability of many different combinations.;https://www.simes.it/en/search/?q=8832;1;130;130;135;Inground;MINIZIP ROUND WALKOVER STAINLESS STEEL ASY;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRZIPCOMF-IN2.pdf;IP65/IP67;IK 09;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;0.5m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_19_Stainless Steel;Simes_Zip_Comfort_Round_Photometrics : S.8832W
S.8832H.19_MINIZIP_COMFORT_ASY_ROUND_2700K_281lm_5.6W_Stainless Steel;S.8832H.19;0;2700;5.6;281;19 Stainless Steel;1.1;3 years;220;240;230;527;n/a;I;https://www.simes.it/en/overview/167/zip-comfort;It has constantly evolved to achieve greater and more precise lighting control and high performance in terms of flux and efficiency. ZIP COMFORT is the right answer to the most difficult architectural challenges thanks to the availability of many different combinations.;https://www.simes.it/en/search/?q=8832;1;130;130;135;Inground;MINIZIP ROUND WALKOVER STAINLESS STEEL ASY;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRZIPCOMF-IN2.pdf;IP65/IP67;IK 09;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;0.5m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_19_Stainless Steel;Simes_Zip_Comfort_Round_Photometrics : S.8832H
S.8833N.19_MINIZIP_COMFORT_31°_ROUND_4000K_458lm_8.7W_Stainless Steel;S.8833N.19;31;4000;8.7;458;19 Stainless Steel;1.1;3 years;220;240;230;696;n/a;I;https://www.simes.it/en/overview/167/zip-comfort;It has constantly evolved to achieve greater and more precise lighting control and high performance in terms of flux and efficiency. ZIP COMFORT is the right answer to the most difficult architectural challenges thanks to the availability of many different combinations.;https://www.simes.it/en/search/?q=8833;1;130;130;135;Inground;MINIZIP ROUND WALKOVER STAINLESS STEEL 33°;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRZIPCOMF-IN2.pdf;IP65/IP67;IK 09;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;0.5m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_19_Stainless Steel;Simes_Zip_Comfort_Round_Photometrics : S.8833N
S.8833W.19_MINIZIP_COMFORT_31°_ROUND_3000K_434lm_8.7W_Stainless Steel;S.8833W.19;31;3000;8.7;434;19 Stainless Steel;1.1;3 years;220;240;230;651;n/a;I;https://www.simes.it/en/overview/167/zip-comfort;It has constantly evolved to achieve greater and more precise lighting control and high performance in terms of flux and efficiency. ZIP COMFORT is the right answer to the most difficult architectural challenges thanks to the availability of many different combinations.;https://www.simes.it/en/search/?q=8833;1;130;130;135;Inground;MINIZIP ROUND WALKOVER STAINLESS STEEL 33°;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRZIPCOMF-IN2.pdf;IP65/IP67;IK 09;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;0.5m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_19_Stainless Steel;Simes_Zip_Comfort_Round_Photometrics : S.8833W
S.8833H.19_MINIZIP_COMFORT_31°_ROUND_2700K_411lm_8.7W_Stainless Steel;S.8833H.19;31;2700;8.7;411;19 Stainless Steel;1.1;3 years;220;240;230;621;n/a;I;https://www.simes.it/en/overview/167/zip-comfort;It has constantly evolved to achieve greater and more precise lighting control and high performance in terms of flux and efficiency. ZIP COMFORT is the right answer to the most difficult architectural challenges thanks to the availability of many different combinations.;https://www.simes.it/en/search/?q=8833;1;130;130;135;Inground;MINIZIP ROUND WALKOVER STAINLESS STEEL 33°;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRZIPCOMF-IN2.pdf;IP65/IP67;IK 09;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;0.5m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_19_Stainless Steel;Simes_Zip_Comfort_Round_Photometrics : S.8833H
S.7805N.09_MINIZIP_COMFORT_ACIDETCHEDGLASS_ROUND_4000K_33lm_3W_Black;S.7805N.09;81;4000;3;33;09 Black;1.1;3 years;220;240;230;150;n/a;I;https://www.simes.it/en/overview/167/zip-comfort;It has constantly evolved to achieve greater and more precise lighting control and high performance in terms of flux and efficiency. ZIP COMFORT is the right answer to the most difficult architectural challenges thanks to the availability of many different combinations.;https://www.simes.it/en/search/?q=7805;1;130;130;135;Inground;MINIZIP ROUND WALKOVER  ACID-ETCHED GLASS;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRZIPCOMF-IN2.pdf;IP65/IP67;IK 09;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;0.5m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_09_Black;Simes_Zip_Comfort_Round_Photometrics : S.8805N
S.7805W.09_MINIZIP_COMFORT_ACIDETCHEDGLASS_ROUND_3000K_32lm_3W_Black;S.7805W.09;81;3000;3;32;09 Black;1.1;3 years;220;240;230;140;n/a;I;https://www.simes.it/en/overview/167/zip-comfort;It has constantly evolved to achieve greater and more precise lighting control and high performance in terms of flux and efficiency. ZIP COMFORT is the right answer to the most difficult architectural challenges thanks to the availability of many different combinations.;https://www.simes.it/en/search/?q=7805;1;130;130;135;Inground;MINIZIP ROUND WALKOVER  ACID-ETCHED GLASS;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRZIPCOMF-IN2.pdf;IP65/IP67;IK 09;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;0.5m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_09_Black;Simes_Zip_Comfort_Round_Photometrics : S.8805W
S.7805H.09_MINIZIP_COMFORT_ACIDETCHEDGLASS_ROUND_2700K_1lm_3W_Black;S.7805H.09;81;2700;3;31;09 Black;1.1;3 years;220;240;230;130;n/a;I;https://www.simes.it/en/overview/167/zip-comfort;It has constantly evolved to achieve greater and more precise lighting control and high performance in terms of flux and efficiency. ZIP COMFORT is the right answer to the most difficult architectural challenges thanks to the availability of many different combinations.;https://www.simes.it/en/search/?q=7805;1;130;130;135;Inground;MINIZIP ROUND WALKOVER  ACID-ETCHED GLASS;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRZIPCOMF-IN2.pdf;IP65/IP67;IK 09;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;0.5m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_09_Black;Simes_Zip_Comfort_Round_Photometrics : S.8805H
S.7831N.09_MINIZIP_COMFORT_11°_ROUND_4000K_343lm_5.6W_Black;S.7831N.09;11;4000;5.6;343;09 Black;1.1;3 years;220;240;230;604;n/a;I;https://www.simes.it/en/overview/167/zip-comfort;It has constantly evolved to achieve greater and more precise lighting control and high performance in terms of flux and efficiency. ZIP COMFORT is the right answer to the most difficult architectural challenges thanks to the availability of many different combinations.;https://www.simes.it/en/search/?q=7831;1;130;130;135;Inground;MINIZIP ROUND WALKOVER  12°;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRZIPCOMF-IN2.pdf;IP65/IP67;IK 09;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;0.5m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_09_Black;Simes_Zip_Comfort_Round_Photometrics : S.8831N
S.7831W.09_MINIZIP_COMFORT_11°_ROUND_3000K_306lm_5.6W_Black;S.7831W.09;11;3000;5.6;306;09 Black;1.1;3 years;220;240;230;552;n/a;I;https://www.simes.it/en/overview/167/zip-comfort;It has constantly evolved to achieve greater and more precise lighting control and high performance in terms of flux and efficiency. ZIP COMFORT is the right answer to the most difficult architectural challenges thanks to the availability of many different combinations.;https://www.simes.it/en/search/?q=7831;1;130;130;135;Inground;MINIZIP ROUND WALKOVER  12°;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRZIPCOMF-IN2.pdf;IP65/IP67;IK 09;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;0.5m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_09_Black;Simes_Zip_Comfort_Round_Photometrics : S.8831W
S.7831H.09_MINIZIP_COMFORT_11°_ROUND_2700K_283lm_5.6W_Black;S.7831H.09;11;2700;5.6;283;09 Black;1.1;3 years;220;240;230;527;n/a;I;https://www.simes.it/en/overview/167/zip-comfort;It has constantly evolved to achieve greater and more precise lighting control and high performance in terms of flux and efficiency. ZIP COMFORT is the right answer to the most difficult architectural challenges thanks to the availability of many different combinations.;https://www.simes.it/en/search/?q=7831;1;130;130;135;Inground;MINIZIP ROUND WALKOVER  12°;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRZIPCOMF-IN2.pdf;IP65/IP67;IK 09;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;0.5m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_09_Black;Simes_Zip_Comfort_Round_Photometrics : S.8831H
S.7832N.09_MINIZIP_COMFORT_ASY_ROUND_4000K_358lm_5.6W_Black;S.7832N.09;0;4000;5.6;358;09 Black;1.1;3 years;220;240;230;604;n/a;I;https://www.simes.it/en/overview/167/zip-comfort;It has constantly evolved to achieve greater and more precise lighting control and high performance in terms of flux and efficiency. ZIP COMFORT is the right answer to the most difficult architectural challenges thanks to the availability of many different combinations.;https://www.simes.it/en/search/?q=7832;1;130;130;135;Inground;MINIZIP ROUND WALKOVER ASY;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRZIPCOMF-IN2.pdf;IP65/IP67;IK 09;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;0.5m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_09_Black;Simes_Zip_Comfort_Round_Photometrics : S.8832N
S.7832W.09_MINIZIP_COMFORT_ASY_ROUND_3000K_306lm_5.6W_Black;S.7832W.09;0;3000;5.6;306;09 Black;1.1;3 years;220;240;230;552;n/a;I;https://www.simes.it/en/overview/167/zip-comfort;It has constantly evolved to achieve greater and more precise lighting control and high performance in terms of flux and efficiency. ZIP COMFORT is the right answer to the most difficult architectural challenges thanks to the availability of many different combinations.;https://www.simes.it/en/search/?q=7832;1;130;130;135;Inground;MINIZIP ROUND WALKOVER ASY;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRZIPCOMF-IN2.pdf;IP65/IP67;IK 09;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;0.5m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_09_Black;Simes_Zip_Comfort_Round_Photometrics : S.8832W
S.7832H.09_MINIZIP_COMFORT_ASY_ROUND_2700K_281lm_5.6W_Black;S.7832H.09;0;2700;5.6;281;09 Black;1.1;3 years;220;240;230;527;n/a;I;https://www.simes.it/en/overview/167/zip-comfort;It has constantly evolved to achieve greater and more precise lighting control and high performance in terms of flux and efficiency. ZIP COMFORT is the right answer to the most difficult architectural challenges thanks to the availability of many different combinations.;https://www.simes.it/en/search/?q=7832;1;130;130;135;Inground;MINIZIP ROUND WALKOVER ASY;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRZIPCOMF-IN2.pdf;IP65/IP67;IK 09;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;0.5m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_09_Black;Simes_Zip_Comfort_Round_Photometrics : S.8832H
S.7833N.09_MINIZIP_COMFORT_31°_ROUND_4000K_458lm_8.7W_Black;S.7833N.09;31;4000;8.7;458;09 Black;1.1;3 years;220;240;230;696;n/a;I;https://www.simes.it/en/overview/167/zip-comfort;It has constantly evolved to achieve greater and more precise lighting control and high performance in terms of flux and efficiency. ZIP COMFORT is the right answer to the most difficult architectural challenges thanks to the availability of many different combinations.;https://www.simes.it/en/search/?q=7833;1;130;130;135;Inground;MINIZIP ROUND WALKOVER  33°;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRZIPCOMF-IN2.pdf;IP65/IP67;IK 09;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;0.5m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_09_Black;Simes_Zip_Comfort_Round_Photometrics : S.8833N
S.7833W.09_MINIZIP_COMFORT_31°_ROUND_3000K_434lm_8.7W_Black;S.7833W.09;31;3000;8.7;434;09 Black;1.1;3 years;220;240;230;651;n/a;I;https://www.simes.it/en/overview/167/zip-comfort;It has constantly evolved to achieve greater and more precise lighting control and high performance in terms of flux and efficiency. ZIP COMFORT is the right answer to the most difficult architectural challenges thanks to the availability of many different combinations.;https://www.simes.it/en/search/?q=7833;1;130;130;135;Inground;MINIZIP ROUND WALKOVER  33°;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRZIPCOMF-IN2.pdf;IP65/IP67;IK 09;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;0.5m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_09_Black;Simes_Zip_Comfort_Round_Photometrics : S.8833W
S.7833H.09_MINIZIP_COMFORT_31°_ROUND_2700K_411lm_8.7W_Black;S.7833H.09;31;2700;8.7;411;09 Black;1.1;3 years;220;240;230;621;n/a;I;https://www.simes.it/en/overview/167/zip-comfort;It has constantly evolved to achieve greater and more precise lighting control and high performance in terms of flux and efficiency. ZIP COMFORT is the right answer to the most difficult architectural challenges thanks to the availability of many different combinations.;https://www.simes.it/en/search/?q=7833;1;130;130;135;Inground;MINIZIP ROUND WALKOVER  33°;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRZIPCOMF-IN2.pdf;IP65/IP67;IK 09;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;0.5m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_09_Black;Simes_Zip_Comfort_Round_Photometrics : S.8833H
