;SIMES_Product Code##OTHER##;SIMES_Beam Angle##ANGLE##DEGREES;SIMES_Color Temperature##COLOR_TEMPERATURE##KELVIN;SIMES_Rated Wattage##ELECTRICAL_POWER##WATTS;SIMES_Rated Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;SIMES_Finishes##OTHER##;SIMES_Weigth##MASS##KILOGRAMS;SIMES_Warranty Period##OTHER##;SIMES_Supply Voltage Min##ELECTRICAL_POTENTIAL##VOLTS;SIMES_Supply Voltage Max##ELECTRICAL_POTENTIAL##VOLTS;SIMES_Supply Voltage##ELECTRICAL_POTENTIAL##VOLTS;SIMES_Source Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;SIMES_Remote Power Supply##OTHER##;SIMES_Protection Class##OTHER##;SIMES_Product Page URL##OTHER##;SIMES_Product Description##OTHER##;SIMES_Product Data Sheet URL##OTHER##;SIMES_Number of Poles##OTHER##;SIMES_Nominal Width##LENGTH##MILLIMETERS;SIMES_Nominal Length##LENGTH##MILLIMETERS;SIMES_Nominal Height##LENGTH##MILLIMETERS;SIMES_Mounting Type##OTHER##;SIMES_Model##OTHER##;SIMES_Material Description##OTHER##;SIMES_Manufacturer Comment##OTHER##;SIMES_Luminous Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;SIMES_Light Source Type##OTHER##;SIMES_Lamp Count##OTHER##;SIMES_Installation Note URL##OTHER##;SIMES_IP Rating##OTHER##;SIMES_IK Rating##OTHER##;SIMES_Frequency##OTHER##;SIMES_Energy Efficiency Class##OTHER##;SIMES_Dimmable##OTHER##;SIMES_Current##ELECTRICAL_CURRENT##AMPERES;SIMES_Control Gear##OTHER##;SIMES_Cable Length##OTHER##;SIMES_CRI##OTHER##;SIMES_Approval Mark##OTHER##;LightFixturePlacingType##OTHER##;LightFixtureMountingType##OTHER##;Light Source##OTHER##;HasProtectiveEarth##OTHER##;Ground Stake##OTHER##;Body##OTHER##;Photometric_Type##OTHER##
S.6306H.01_MICROKUBE LONG_2700K_370lm_13W_White;S.6306H.01;0;2700;13;370;01 White;2.5;3 years;220;240;230;921;n/a;I;https://www.simes.it/en/overview/115/kube;KUBE is an object of urban design that can be integrated into any context and is particularly suitable for paths, parks and landscape areas.;https://www.simes.it/en/search/?q=6306;1;120;120;450;Ground mounted;MICROKUBE LONG;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRKUBE2.pdf;IP54;IK 06;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;0.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_01_White;Simes_Kube_Photometrics : S.6306H
S.6306H.09_MICROKUBE LONG_2700K_370lm_13W_Black;S.6306H.09;0;2700;13;370;09 Black;2.5;3 years;220;240;230;921;n/a;I;https://www.simes.it/en/overview/115/kube;KUBE is an object of urban design that can be integrated into any context and is particularly suitable for paths, parks and landscape areas.;https://www.simes.it/en/search/?q=6306;1;120;120;450;Ground mounted;MICROKUBE LONG;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRKUBE2.pdf;IP54;IK 06;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;0.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_09_Black;Simes_Kube_Photometrics : S.6306H
S.6306H.14_MICROKUBE LONG_2700K_370lm_13W_Aluminium grey;S.6306H.14;0;2700;13;370;14 Aluminium Grey;2.5;3 years;220;240;230;921;n/a;I;https://www.simes.it/en/overview/115/kube;KUBE is an object of urban design that can be integrated into any context and is particularly suitable for paths, parks and landscape areas.;https://www.simes.it/en/search/?q=6306;1;120;120;450;Ground mounted;MICROKUBE LONG;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRKUBE2.pdf;IP54;IK 06;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;0.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Kube_Photometrics : S.6306H
S.6306N.01_MICROKUBE LONG_4000K_421lm_13W_White;S.6306N.01;0;4000;13;421;01 White;2.5;3 years;220;240;230;1048;n/a;I;https://www.simes.it/en/overview/115/kube;KUBE is an object of urban design that can be integrated into any context and is particularly suitable for paths, parks and landscape areas.;https://www.simes.it/en/search/?q=6306;1;120;120;450;Ground mounted;MICROKUBE LONG;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRKUBE2.pdf;IP54;IK 06;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;0.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_01_White;Simes_Kube_Photometrics : S.6306N
S.6306N.09_MICROKUBE LONG_4000K_421lm_13W_Black;S.6306N.09;0;4000;13;421;09 Black;2.5;3 years;220;240;230;1048;n/a;I;https://www.simes.it/en/overview/115/kube;KUBE is an object of urban design that can be integrated into any context and is particularly suitable for paths, parks and landscape areas.;https://www.simes.it/en/search/?q=6306;1;120;120;450;Ground mounted;MICROKUBE LONG;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRKUBE2.pdf;IP54;IK 06;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;0.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_09_Black;Simes_Kube_Photometrics : S.6306N
S.6306N.14_MICROKUBE LONG_4000K_421lm_13W_Aluminium grey;S.6306N.14;0;4000;13;421;14 Aluminium Grey;2.5;3 years;220;240;230;1048;n/a;I;https://www.simes.it/en/overview/115/kube;KUBE is an object of urban design that can be integrated into any context and is particularly suitable for paths, parks and landscape areas.;https://www.simes.it/en/search/?q=6306;1;120;120;450;Ground mounted;MICROKUBE LONG;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRKUBE2.pdf;IP54;IK 06;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;0.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Kube_Photometrics : S.6306N
S.6306W.01_MICROKUBE LONG_3000K_390lm_13W_White;S.6306W.01;0;3000;13;390;01 White;2.5;3 years;220;240;230;970;n/a;I;https://www.simes.it/en/overview/115/kube;KUBE is an object of urban design that can be integrated into any context and is particularly suitable for paths, parks and landscape areas.;https://www.simes.it/en/search/?q=6306;1;120;120;450;Ground mounted;MICROKUBE LONG;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRKUBE2.pdf;IP54;IK 06;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;0.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_01_White;Simes_Kube_Photometrics : S.6306W
S.6306W.09_MICROKUBE LONG_3000K_390lm_13W_Black;S.6306W.09;0;3000;13;390;09 Black;2.5;3 years;220;240;230;970;n/a;I;https://www.simes.it/en/overview/115/kube;KUBE is an object of urban design that can be integrated into any context and is particularly suitable for paths, parks and landscape areas.;https://www.simes.it/en/search/?q=6306;1;120;120;450;Ground mounted;MICROKUBE LONG;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRKUBE2.pdf;IP54;IK 06;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;0.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_09_Black;Simes_Kube_Photometrics : S.6306W
S.6306W.14_MICROKUBE LONG_3000K_390lm_13W_Aluminium grey;S.6306W.14;0;3000;13;390;14 Aluminium Grey;2.5;3 years;220;240;230;970;n/a;I;https://www.simes.it/en/overview/115/kube;KUBE is an object of urban design that can be integrated into any context and is particularly suitable for paths, parks and landscape areas.;https://www.simes.it/en/search/?q=6306;1;120;120;450;Ground mounted;MICROKUBE LONG;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRKUBE2.pdf;IP54;IK 06;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;0.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Kube_Photometrics : S.6306W
S.6307H.01_MICROKUBE LONG BOLLARD_2700K_370lm_13W_White;S.6307H.01;0;2700;13;370;01 White;5.5;3 years;220;240;230;921;n/a;I;https://www.simes.it/en/overview/115/kube;KUBE is an object of urban design that can be integrated into any context and is particularly suitable for paths, parks and landscape areas.;https://www.simes.it/en/search/?q=6307;1;120;120;900;Ground mounted;MICROKUBE LONG BOLLARD;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRKUBE2.pdf;IP54;IK 06;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;0.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_01_White;Simes_Kube_Photometrics : S.6306H
S.6307H.09_MICROKUBE LONG BOLLARD_2700K_370lm_13W_Black;S.6307H.09;0;2700;13;370;09 Black;5.5;3 years;220;240;230;921;n/a;I;https://www.simes.it/en/overview/115/kube;KUBE is an object of urban design that can be integrated into any context and is particularly suitable for paths, parks and landscape areas.;https://www.simes.it/en/search/?q=6307;1;120;120;900;Ground mounted;MICROKUBE LONG BOLLARD;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRKUBE2.pdf;IP54;IK 06;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;0.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_09_Black;Simes_Kube_Photometrics : S.6306H
S.6307H.14_MICROKUBE LONG BOLLARD_2700K_370lm_13W_Aluminium grey;S.6307H.14;0;2700;13;370;14 Aluminium Grey;5.5;3 years;220;240;230;921;n/a;I;https://www.simes.it/en/overview/115/kube;KUBE is an object of urban design that can be integrated into any context and is particularly suitable for paths, parks and landscape areas.;https://www.simes.it/en/search/?q=6307;1;120;120;900;Ground mounted;MICROKUBE LONG BOLLARD;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRKUBE2.pdf;IP54;IK 06;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;0.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Kube_Photometrics : S.6306H
S.6307N.01_MICROKUBE LONG BOLLARD_4000K_421lm_13W_White;S.6307N.01;0;4000;13;421;01 White;5.5;3 years;220;240;230;1048;n/a;I;https://www.simes.it/en/overview/115/kube;KUBE is an object of urban design that can be integrated into any context and is particularly suitable for paths, parks and landscape areas.;https://www.simes.it/en/search/?q=6307;1;120;120;900;Ground mounted;MICROKUBE LONG BOLLARD;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRKUBE2.pdf;IP54;IK 06;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;0.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_01_White;Simes_Kube_Photometrics : S.6306N
S.6307N.09_MICROKUBE LONG BOLLARD_4000K_421lm_13W_Black;S.6307N.09;0;4000;13;421;09 Black;5.5;3 years;220;240;230;1048;n/a;I;https://www.simes.it/en/overview/115/kube;KUBE is an object of urban design that can be integrated into any context and is particularly suitable for paths, parks and landscape areas.;https://www.simes.it/en/search/?q=6307;1;120;120;900;Ground mounted;MICROKUBE LONG BOLLARD;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRKUBE2.pdf;IP54;IK 06;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;0.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_09_Black;Simes_Kube_Photometrics : S.6306N
S.6307N.14_MICROKUBE LONG BOLLARD_4000K_421lm_13W_Aluminium grey;S.6307N.14;0;4000;13;421;14 Aluminium Grey;5.5;3 years;220;240;230;1048;n/a;I;https://www.simes.it/en/overview/115/kube;KUBE is an object of urban design that can be integrated into any context and is particularly suitable for paths, parks and landscape areas.;https://www.simes.it/en/search/?q=6307;1;120;120;900;Ground mounted;MICROKUBE LONG BOLLARD;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRKUBE2.pdf;IP54;IK 06;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;0.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Kube_Photometrics : S.6306N
S.6307W.01_MICROKUBE LONG BOLLARD_3000K_390lm_13W_White;S.6307W.01;0;3000;13;390;01 White;5.5;3 years;220;240;230;970;n/a;I;https://www.simes.it/en/overview/115/kube;KUBE is an object of urban design that can be integrated into any context and is particularly suitable for paths, parks and landscape areas.;https://www.simes.it/en/search/?q=6307;1;120;120;900;Ground mounted;MICROKUBE LONG BOLLARD;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRKUBE2.pdf;IP54;IK 06;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;0.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_01_White;Simes_Kube_Photometrics : S.6306W
S.6307W.09_MICROKUBE LONG BOLLARD_3000K_390lm_13W_Black;S.6307W.09;0;3000;13;390;09 Black;5.5;3 years;220;240;230;970;n/a;I;https://www.simes.it/en/overview/115/kube;KUBE is an object of urban design that can be integrated into any context and is particularly suitable for paths, parks and landscape areas.;https://www.simes.it/en/search/?q=6307;1;120;120;900;Ground mounted;MICROKUBE LONG BOLLARD;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRKUBE2.pdf;IP54;IK 06;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;0.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_09_Black;Simes_Kube_Photometrics : S.6306W
S.6307W.14_MICROKUBE LONG BOLLARD_3000K_390lm_13W_Aluminium grey;S.6307W.14;0;3000;13;390;14 Aluminium Grey;5.5;3 years;220;240;230;970;n/a;I;https://www.simes.it/en/overview/115/kube;KUBE is an object of urban design that can be integrated into any context and is particularly suitable for paths, parks and landscape areas.;https://www.simes.it/en/search/?q=6307;1;120;120;900;Ground mounted;MICROKUBE LONG BOLLARD;Aluminium body;n/a;0;LED;1;https://www.simes.it/download/montaggio/ISTRKUBE2.pdf;IP54;IK 06;AC 50-60Hz / DC;A+;n/a;0;Electronic ballast;0.0m;CRI90;CE;UNSET;UNSET;SIMES_Light Source;1;SIMES_Black_Polipropilene;SIMES_14_Aluminium grey;Simes_Kube_Photometrics : S.6306W
